| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
NPNZ_ADC_TRGCTRL_s Struct Reference

`#include <power_control/drivers/npnz16b.h>`

Collaboration diagram for NPNZ_ADC_TRGCTRL_s:

## Data Fields
volatile uint16_t * | ptrADCTriggerARegister
| Pointer to ADC trigger #1 register (e.g. TRIG1) More...
volatile uint16_t | ADCTriggerAOffset
| ADC trigger #1 offset to compensate propagation delays. More...
volatile uint16_t * | ptrADCTriggerBRegister
| Pointer to ADC trigger #2 register (e.g. TRIG2) More...
volatile uint16_t | ADCTriggerBOffset
| ADC trigger #2 offset to compensate propagation delays. More...

## Detailed Description

Definition at line 354 of file npnz16b.h.

## Field Documentation

## ◆ ADCTriggerAOffset

volatile uint16_t ADCTriggerAOffset

ADC trigger #1 offset to compensate propagation delays.

Definition at line 357 of file npnz16b.h.

## ◆ ADCTriggerBOffset

volatile uint16_t ADCTriggerBOffset

ADC trigger #2 offset to compensate propagation delays.

Definition at line 359 of file npnz16b.h.

## ◆ ptrADCTriggerARegister

volatile uint16_t* ptrADCTriggerARegister

Pointer to ADC trigger #1 register (e.g. TRIG1)

Definition at line 356 of file npnz16b.h.

## ◆ ptrADCTriggerBRegister

volatile uint16_t* ptrADCTriggerBRegister

Pointer to ADC trigger #2 register (e.g. TRIG2)

Definition at line 358 of file npnz16b.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/drivers/npnz16b.h