| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
UART_DATBUF_STATUS_s Struct Reference

`#include <common/p33c_pral/p33c_uart.h>`

Collaboration diagram for UART_DATBUF_STATUS_s:

## Data Fields
union {
volatile uint16_t value
}; |
volatile bool | buffer_empty: 1
volatile bool | buffer_full: 1
volatile | unsigned: 6
volatile bool | buffer_overun: 1
volatile bool | msg_complete: 1

## Detailed Description

Definition at line 133 of file p33c_uart.h.

## Field Documentation

## ◆ @347

union { ... }

## ◆ buffer_empty

volatile bool buffer_empty

Definition at line 137 of file p33c_uart.h.

## ◆ buffer_full

volatile bool buffer_full

Definition at line 138 of file p33c_uart.h.

## ◆ buffer_overun

volatile bool buffer_overun

Definition at line 140 of file p33c_uart.h.

## ◆ msg_complete

volatile bool msg_complete

Definition at line 142 of file p33c_uart.h.

## ◆ unsigned

volatile unsigned

Definition at line 139 of file p33c_uart.h.

## ◆ value

volatile uint16_t value

Definition at line 144 of file p33c_uart.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_uart.h