| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
APPTASK_TASKLINK_s Struct Reference

DESCRIPTION. More...

`#include <os/apptask_typedef.h>`

Collaboration diagram for APPTASK_TASKLINK_s:

## Data Fields
volatile uint16_t(* | Initialize )(void)
| Function pointer to INITIALIZATION routine. More...
volatile uint16_t(* | Start )(void)
| Function pointer to START routine. More...
volatile uint16_t(* | Execute )(void)
| Function pointer to EXECUTE routine. More...
volatile uint16_t(* | Dispose )(void)
| Function pointer to DISPOSE routine. More...

## Detailed Description

DESCRIPTION.

Definition at line 112 of file apptask_typedef.h.

## Field Documentation

## ◆ Dispose

volatile uint16_t(* Dispose) (void)

Function pointer to DISPOSE routine.

Definition at line 117 of file apptask_typedef.h.

## ◆ Execute

volatile uint16_t(* Execute) (void)

Function pointer to EXECUTE routine.

Definition at line 116 of file apptask_typedef.h.

## ◆ Initialize

volatile uint16_t(* Initialize) (void)

Function pointer to INITIALIZATION routine.

Definition at line 114 of file apptask_typedef.h.

## ◆ Start

volatile uint16_t(* Start) (void)

Function pointer to START routine.

Definition at line 115 of file apptask_typedef.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/os/apptask_typedef.h