| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
P33C_OSC_CONFIG_s Struct Reference

`#include <common/p33c_pral/p33c_osc.h>`

Collaboration diagram for P33C_OSC_CONFIG_s:

## Data Fields
union {
volatile uint16_t value
}; |
enum OSCCON_OSWEN_e | OSWEN: 1
volatile | unsigned: 1
enum OSCCON_CF_e | CF: 1
enum OSCCON_LOCK_e | LOCK: 1
enum OSCCON_CLKLOCK_e | CLKLOCK: 1
enum OSCCON_xOSC_TYPE_e | NOSC: 3
enum OSCCON_xOSC_TYPE_e | COSC: 3

## Detailed Description

Definition at line 238 of file p33c_osc.h.

## Field Documentation

## ◆ @206

union { ... }

## ◆ CF

enum OSCCON_CF_e CF

Definition at line 244 of file p33c_osc.h.

## ◆ CLKLOCK

enum OSCCON_CLKLOCK_e CLKLOCK

Definition at line 248 of file p33c_osc.h.

## ◆ COSC

enum OSCCON_xOSC_TYPE_e COSC

Definition at line 251 of file p33c_osc.h.

## ◆ LOCK

enum OSCCON_LOCK_e LOCK

Definition at line 246 of file p33c_osc.h.

## ◆ NOSC

enum OSCCON_xOSC_TYPE_e NOSC

Definition at line 249 of file p33c_osc.h.

## ◆ OSWEN

enum OSCCON_OSWEN_e OSWEN

Definition at line 241 of file p33c_osc.h.

## ◆ unsigned

volatile unsigned

Definition at line 242 of file p33c_osc.h.

## ◆ value

volatile uint16_t value

Definition at line 254 of file p33c_osc.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_osc.h