| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
TASK_INFO_s Struct Reference

`#include <fault_handler/drivers/drv_trap_handler.h>`

Collaboration diagram for TASK_INFO_s:

## Data Fields
volatile uint16_t | task_id
volatile uint16_t | fault_id
volatile uint16_t | op_mode

## Detailed Description

Definition at line 263 of file drv_trap_handler.h.

## Field Documentation

## ◆ fault_id

volatile uint16_t fault_id

Definition at line 266 of file drv_trap_handler.h.

## ◆ op_mode

volatile uint16_t op_mode

Definition at line 267 of file drv_trap_handler.h.

## ◆ task_id

volatile uint16_t task_id

Definition at line 265 of file drv_trap_handler.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/fault_handler/drivers/drv_trap_handler.h