# kengine_input

* [data](data)
    * [buffer](data/buffer.md): holds the input events since last frame
    * [handler](data/handler.md): reacts to input events
* [systems](systems)
    * [system](systems/system.md): forwards events from a buffer to handlers