Peripherals API
***************

.. toctree::
   :maxdepth: 1

   GPIO <gpio>
   UART <uart>
   I2C <i2c>
   SPI Master <spi_master>
   Timer <timer>
   Pulse Counter <pcnt>
   Sigma-delta Modulation <sigmadelta>
   LED Control <ledc>
   Remote Control <rmt>


Example code for this API section is provided in :example:`peripherals` directory of ESP-IDF examples.
