Storage API
***********

.. toctree::
   :maxdepth: 1

   SPI Flash and Partition APIs <spi_flash>
   SD/MMC <sdmmc>
   Non-Volatile Storage <nvs_flash>
   Virtual Filesystem <vfs>
   FAT Filesystem <fatfs>


Example code for this API section is provided in :example:`storage` directory of ESP-IDF examples.
