# Example: rmt_nec_tx_rx

This example uses the remote control (RMT) peripheral to transmit and receive codes for the NEC infrared remote protocol.

Configuration (pin numbers, etc.) can be modified in top of the main/infrared_nec.c file.

