v2.0.0
Data Fields
_cyw43_wifi_scan_options_t Struct Reference
Networking Libraries » pico_cyw43_arch » cyw43_driver » cyw43_ll

wifi scan options passed to cyw43_wifi_scan More...

`#include <cyw43_ll.h>`

## Data Fields
uint32_t | version
| version (not used)
uint16_t | action
| action (not used)
uint16_t | _
| not used
uint32_t | ssid_len
| ssid length, 0=all
uint8_t | ssid [32]
| ssid name
uint8_t | bssid [6]
| bssid (not used)
int8_t | bss_type
| bssid type (not used)
int8_t | scan_type
| scan type 0=active, 1=passive
int32_t | nprobes
| number of probes (not used)
int32_t | active_time
| active time (not used)
int32_t | passive_time
| passive time (not used)
int32_t | home_time
| home time (not used)
int32_t | channel_num
| number of channels (not used)
uint16_t | channel_list [1]
| channel list (not used)

## Detailed Description

wifi scan options passed to cyw43_wifi_scan

The documentation for this struct was generated from the following file:

- cyw43_ll.h