v2.0.0

### - _ -

- __fast_mul : platform.h

### - a -

- ADC_TEMPERATURE_CHANNEL_NUM : adc.h
- auto_init_mutex : mutex.h
- auto_init_recursive_mutex : mutex.h

### - c -

- CYW43_AGGRESSIVE_PM : cyw43.h
- CYW43_COUNTRY : cyw43_country.h
- CYW43_DEFAULT_PM : cyw43.h
- CYW43_LINK_BADAUTH : cyw43.h
- CYW43_LINK_DOWN : cyw43.h
- CYW43_LINK_FAIL : cyw43.h
- CYW43_LINK_JOIN : cyw43.h
- CYW43_LINK_NOIP : cyw43.h
- CYW43_LINK_NONET : cyw43.h
- CYW43_LINK_UP : cyw43.h
- CYW43_PERFORMANCE_PM : cyw43.h

### - d -

- DMA_IRQ_NUM : dma.h
- DOORBELL_IRQ_NUM : multicore.h

### - i -

- i2c0 : i2c.h
- i2c1 : i2c.h
- I2C_DREQ_NUM : i2c.h
- I2C_INSTANCE : i2c.h
- I2C_NUM : i2c.h

### - l -

- lock_get_caller_owner_id : lock_core.h
- lock_internal_spin_unlock_with_best_effort_wait_or_timeout : lock_core.h
- lock_internal_spin_unlock_with_notify : lock_core.h
- lock_internal_spin_unlock_with_wait : lock_core.h
- LOCK_INVALID_OWNER_ID : lock_core.h
- lock_owner_id_t : lock_core.h

### - p -

- PHEAP_DEFINE_STATIC : pheap.h
- PICO_DEFAULT_TIMER : timer.h
- PICO_DEFAULT_TIMER_INSTANCE : timer.h
- PICO_DEFAULT_UART_BAUD_RATE : uart.h
- PICO_TIME_DEFAULT_ALARM_POOL_DISABLED : time.h
- PICO_TIME_DEFAULT_ALARM_POOL_HARDWARE_ALARM_NUM : time.h
- PICO_TIME_DEFAULT_ALARM_POOL_MAX_TIMERS : time.h
- pio0 : pio.h
- pio1 : pio.h
- PIO_DREQ_NUM : pio.h
- PIO_FUNCSEL_NUM : pio.h
- PIO_INSTANCE : pio.h
- PIO_IRQ_NUM : pio.h
- PIO_NUM : pio.h
- PLL_RESET_NUM : pll.h
- PWM_DEFAULT_IRQ_NUM : pwm.h
- PWM_DREQ_NUM : pwm.h
- PWM_GPIO_SLICE_NUM : pwm.h

### - s -

- SHA256_RESULT_BYTES : sha256.h
- SIO_FIFO_IRQ_NUM : multicore.h
- spi0 : spi.h
- spi1 : spi.h
- SPI_DREQ_NUM : spi.h
- SPI_INSTANCE : spi.h
- SPI_NUM : spi.h
- sync_internal_yield_until_before : lock_core.h

### - t -

- TIMER_ALARM_IRQ_NUM : timer.h
- TIMER_ALARM_NUM_FROM_IRQ : timer.h
- TIMER_NUM_FROM_IRQ : timer.h

### - u -

- uart0 : uart.h
- uart1 : uart.h
- UART_CLOCK_NUM : uart.h
- UART_DREQ_NUM : uart.h
- UART_FUNCSEL_NUM : uart.h
- UART_INSTANCE : uart.h
- UART_IRQ_NUM : uart.h
- UART_NUM : uart.h
- UART_RESET_NUM : uart.h