v2.0.0

### - c -

- cancel_alarm() : time.h
- cancel_repeating_timer() : time.h
- channel_config_get_ctrl_value() : dma.h
- channel_config_set_bswap() : dma.h
- channel_config_set_chain_to() : dma.h
- channel_config_set_dreq() : dma.h
- channel_config_set_enable() : dma.h
- channel_config_set_high_priority() : dma.h
- channel_config_set_irq_quiet() : dma.h
- channel_config_set_read_increment() : dma.h
- channel_config_set_ring() : dma.h
- channel_config_set_sniff_enable() : dma.h
- channel_config_set_transfer_data_size() : dma.h
- channel_config_set_write_increment() : dma.h
- check_sys_clock_hz() : clocks.h
- check_sys_clock_khz() : clocks.h
- clock_configure() : clocks.h
- clock_configure_gpin() : clocks.h
- clock_configure_int_divider() : clocks.h
- clock_configure_undivided() : clocks.h
- clock_get_hz() : clocks.h
- clock_gpio_init() : clocks.h
- clock_gpio_init_int_frac() : clocks.h
- clock_set_reported_hz() : clocks.h
- clock_stop() : clocks.h
- clocks_enable_resus() : clocks.h
- clocks_init() : runtime_init.h
- critical_section_deinit() : critical_section.h
- critical_section_enter_blocking() : critical_section.h
- critical_section_exit() : critical_section.h
- critical_section_init() : critical_section.h
- critical_section_init_with_lock_num() : critical_section.h
- critical_section_is_initialized() : critical_section.h
- cyw43_arch_async_context() : cyw43_arch.h
- cyw43_arch_deinit() : cyw43_arch.h
- cyw43_arch_disable_ap_mode() : cyw43_arch.h
- cyw43_arch_disable_sta_mode() : cyw43_arch.h
- cyw43_arch_enable_ap_mode() : cyw43_arch.h
- cyw43_arch_enable_sta_mode() : cyw43_arch.h
- cyw43_arch_get_country_code() : cyw43_arch.h
- cyw43_arch_gpio_get() : cyw43_arch.h
- cyw43_arch_gpio_put() : cyw43_arch.h
- cyw43_arch_init() : cyw43_arch.h
- cyw43_arch_init_default_async_context() : cyw43_arch.h
- cyw43_arch_init_with_country() : cyw43_arch.h
- cyw43_arch_lwip_begin() : cyw43_arch.h
- cyw43_arch_lwip_end() : cyw43_arch.h
- cyw43_arch_lwip_protect() : cyw43_arch.h
- cyw43_arch_poll() : cyw43_arch.h
- cyw43_arch_set_async_context() : cyw43_arch.h
- cyw43_arch_wait_for_work_until() : cyw43_arch.h
- cyw43_arch_wifi_connect_async() : cyw43_arch.h
- cyw43_arch_wifi_connect_blocking() : cyw43_arch.h
- cyw43_arch_wifi_connect_bssid_async() : cyw43_arch.h
- cyw43_arch_wifi_connect_bssid_blocking() : cyw43_arch.h
- cyw43_arch_wifi_connect_bssid_timeout_ms() : cyw43_arch.h
- cyw43_arch_wifi_connect_timeout_ms() : cyw43_arch.h
- cyw43_cb_tcpip_deinit() : cyw43.h
- cyw43_cb_tcpip_init() : cyw43.h
- cyw43_cb_tcpip_set_link_down() : cyw43.h
- cyw43_cb_tcpip_set_link_up() : cyw43.h
- cyw43_deinit() : cyw43.h
- cyw43_driver_deinit() : cyw43_driver.h
- cyw43_driver_init() : cyw43_driver.h
- cyw43_init() : cyw43.h
- cyw43_ioctl() : cyw43.h
- cyw43_is_initialized() : cyw43.h
- cyw43_pm_value() : cyw43.h
- cyw43_send_ethernet() : cyw43.h
- cyw43_tcpip_link_status() : cyw43.h
- cyw43_wifi_ap_get_auth() : cyw43.h
- cyw43_wifi_ap_get_max_stas() : cyw43.h
- cyw43_wifi_ap_get_ssid() : cyw43.h
- cyw43_wifi_ap_get_stas() : cyw43.h
- cyw43_wifi_ap_set_auth() : cyw43.h
- cyw43_wifi_ap_set_channel() : cyw43.h
- cyw43_wifi_ap_set_password() : cyw43.h
- cyw43_wifi_ap_set_ssid() : cyw43.h
- cyw43_wifi_get_bssid() : cyw43.h
- cyw43_wifi_get_mac() : cyw43.h
- cyw43_wifi_get_pm() : cyw43.h
- cyw43_wifi_get_rssi() : cyw43.h
- cyw43_wifi_join() : cyw43.h
- cyw43_wifi_leave() : cyw43.h
- cyw43_wifi_link_status() : cyw43.h
- cyw43_wifi_pm() : cyw43.h
- cyw43_wifi_scan() : cyw43.h
- cyw43_wifi_scan_active() : cyw43.h
- cyw43_wifi_set_up() : cyw43.h
- cyw43_wifi_update_multicast_filter() : cyw43.h