v2.0.0
coresight_trace.h
1// THIS HEADER FILE IS AUTOMATICALLY GENERATED -- DO NOT EDIT
2
8#ifndef _HARDWARE_STRUCTS_CORESIGHT_TRACE_H
9#define _HARDWARE_STRUCTS_CORESIGHT_TRACE_H
10
15#include "hardware/address_mapped.h"
16#include "hardware/regs/coresight_trace.h"
17
18// Reference to datasheet: https://datasheets.raspberrypi.com/rp2350/rp2350-datasheet.pdf#tab-registerlist_coresight_trace
19//
20// The _REG_ macro is intended to help make the register navigable in your IDE (for example, using the "Go to Definition" feature)
21// _REG_(x) will link to the corresponding register in hardware/regs/coresight_trace.h.
22//
23// Bit-field descriptions are of the form:
24// BITMASK [BITRANGE] FIELDNAME (RESETVALUE) DESCRIPTION
25
26 typedef struct {
27 _REG_(CORESIGHT_TRACE_CTRL_STATUS_OFFSET) // CORESIGHT_TRACE_CTRL_STATUS
28 // Control and status register
29 // 0x00000002 [1] TRACE_CAPTURE_FIFO_OVERFLOW (0) This status flag is set high when trace data has been...
30 // 0x00000001 [0] TRACE_CAPTURE_FIFO_FLUSH (1) Set to 1 to continuously hold the trace FIFO in a...
31 io_rw_32 ctrl_status;
32
33 _REG_(CORESIGHT_TRACE_TRACE_CAPTURE_FIFO_OFFSET) // CORESIGHT_TRACE_TRACE_CAPTURE_FIFO
34 // FIFO for trace data captured from the TPIU
35 // 0xffffffff [31:0] RDATA (0x00000000) Read from an 8 x 32-bit FIFO containing trace data...
36 io_ro_32 trace_capture_fifo;
37} coresight_trace_hw_t;
38
39#define coresight_trace_hw ((coresight_trace_hw_t *)CORESIGHT_TRACE_BASE)
40static_assert(sizeof (coresight_trace_hw_t) == 0x0008, "");
41
42#endif // _HARDWARE_STRUCTS_CORESIGHT_TRACE_H
43
address_mapped.h
coresight_trace_hw_t
Definition: coresight_trace.h:26