v2.0.0
Public Member Functions | Data Fields
io_qspi_hw_t Struct Reference
Collaboration diagram for io_qspi_hw_t:
[legend]

## Public Member Functions
| _REG_ (IO_QSPI_INTR_OFFSET) io_rw_32 intr
| _REG_ (IO_QSPI_USBPHY_DP_STATUS_OFFSET) io_ro_32 usbphy_dp_status
| _REG_ (IO_QSPI_USBPHY_DP_CTRL_OFFSET) io_rw_32 usbphy_dp_ctrl
| _REG_ (IO_QSPI_USBPHY_DM_STATUS_OFFSET) io_ro_32 usbphy_dm_status
| _REG_ (IO_QSPI_USBPHY_DM_CTRL_OFFSET) io_rw_32 usbphy_dm_ctrl
| _REG_ (IO_QSPI_IRQSUMMARY_PROC0_SECURE_OFFSET) io_ro_32 irqsummary_proc0_secure
| _REG_ (IO_QSPI_IRQSUMMARY_PROC0_NONSECURE_OFFSET) io_ro_32 irqsummary_proc0_nonsecure
| _REG_ (IO_QSPI_IRQSUMMARY_PROC1_SECURE_OFFSET) io_ro_32 irqsummary_proc1_secure
| _REG_ (IO_QSPI_IRQSUMMARY_PROC1_NONSECURE_OFFSET) io_ro_32 irqsummary_proc1_nonsecure
| _REG_ (IO_QSPI_IRQSUMMARY_DORMANT_WAKE_SECURE_OFFSET) io_ro_32 irqsummary_dormant_wake_secure
| _REG_ (IO_QSPI_IRQSUMMARY_DORMANT_WAKE_NONSECURE_OFFSET) io_ro_32 irqsummary_dormant_wake_nonsecure
| _REG_ (IO_QSPI_INTR_OFFSET) io_rw_32 intr

## Data Fields
io_qspi_status_ctrl_hw_t | io [6]
union {
struct {
io_qspi_irq_ctrl_hw_t proc0_irq_ctrl
io_qspi_irq_ctrl_hw_t proc1_irq_ctrl
io_qspi_irq_ctrl_hw_t dormant_wake_irq_ctrl
} |
io_qspi_irq_ctrl_hw_t irq_ctrl [3]
}; |
uint32_t | _pad0 [112]
union {
struct {
io_qspi_irq_ctrl_hw_t proc0_irq_ctrl
io_qspi_irq_ctrl_hw_t proc1_irq_ctrl
io_qspi_irq_ctrl_hw_t dormant_wake_irq_ctrl
} |
io_qspi_irq_ctrl_hw_t irq_ctrl [3]
}; |

The documentation for this struct was generated from the following files:

- include/hardware/structs/io_qspi.h
- include/hardware/structs/io_qspi.h