v2.0.0
Data Fields
_cyw43_t Struct Reference
Networking Libraries » pico_cyw43_arch » cyw43_driver
Collaboration diagram for _cyw43_t:
[legend]

## Data Fields
cyw43_ll_t | cyw43_ll
uint8_t | itf_state
uint32_t | trace_flags
volatile uint32_t | wifi_scan_state
uint32_t | wifi_join_state
void * | wifi_scan_env
int(* | wifi_scan_cb )(void *, const cyw43_ev_scan_result_t *)
bool | initted
bool | pend_disassoc
bool | pend_rejoin
bool | pend_rejoin_wpa
uint32_t | ap_auth
uint8_t | ap_channel
uint8_t | ap_ssid_len
uint8_t | ap_key_len
uint8_t | ap_ssid [32]
uint8_t | ap_key [64]
struct netif | netif [2]
uint8_t | mac [6]

The documentation for this struct was generated from the following file:

- cyw43.h