v2.0.0
Data Structures | Data Fields
usb_host_dpram_t Struct Reference
Collaboration diagram for usb_host_dpram_t:
[legend]

## Data Structures
struct | usb_host_dpram_ep_buf_ctrl
struct | usb_host_dpram_ep_ctrl

## Data Fields
volatile uint8_t | setup_packet [8]
struct usb_host_dpram_t::usb_host_dpram_ep_ctrl | int_ep_ctrl [(16 - 1)]
io_rw_32 | epx_buf_ctrl
io_rw_32 | _spare0
struct usb_host_dpram_t::usb_host_dpram_ep_buf_ctrl | int_ep_buffer_ctrl [(16 - 1)]
io_rw_32 | epx_ctrl
uint8_t | _spare1 [124]
uint8_t | epx_data [4096u - 0x180]

The documentation for this struct was generated from the following files:

- include/hardware/structs/usb_dpram.h
- include/hardware/structs/usb_dpram.h