v2.0.0
Data Fields
_cyw43_scan_result_internal_t Struct Reference

## Data Fields
uint32_t | version
uint32_t | length
uint8_t | bssid [6]
uint16_t | beacon_period
uint16_t | capability
uint8_t | ssid_len
uint8_t | ssid [32]
uint32_t | rateset_count
uint8_t | rateset_rates [16]
uint16_t | chanspec
uint16_t | atim_window
uint8_t | dtim_period
int16_t | rssi
int8_t | phy_noise
uint8_t | n_cap
uint32_t | nbss_cap
uint8_t | ctl_ch
uint32_t | reserved32 [1]
uint8_t | flags
uint8_t | reserved [3]
uint8_t | basic_mcs [16]
uint16_t | ie_offset
uint32_t | ie_length
int16_t | SNR

The documentation for this struct was generated from the following file:

- cyw43_ll.c