v2.0.0
pads_bank0.h
1// THIS HEADER FILE IS AUTOMATICALLY GENERATED -- DO NOT EDIT
2
8#ifndef _HARDWARE_STRUCTS_PADS_BANK0_H
9#define _HARDWARE_STRUCTS_PADS_BANK0_H
10
15#include "hardware/address_mapped.h"
16#include "hardware/regs/pads_bank0.h"
17
18// Reference to datasheet: https://datasheets.raspberrypi.com/rp2350/rp2350-datasheet.pdf#tab-registerlist_pads_bank0
19//
20// The _REG_ macro is intended to help make the register navigable in your IDE (for example, using the "Go to Definition" feature)
21// _REG_(x) will link to the corresponding register in hardware/regs/pads_bank0.h.
22//
23// Bit-field descriptions are of the form:
24// BITMASK [BITRANGE] FIELDNAME (RESETVALUE) DESCRIPTION
25
26typedef struct {
27 _REG_(PADS_BANK0_VOLTAGE_SELECT_OFFSET) // PADS_BANK0_VOLTAGE_SELECT
28 // Voltage select
29 // 0x00000001 [0] VOLTAGE_SELECT (0)
30 io_rw_32 voltage_select;
31
32 // (Description copied from array index 0 register PADS_BANK0_GPIO0 applies similarly to other array indexes)
33 _REG_(PADS_BANK0_GPIO0_OFFSET) // PADS_BANK0_GPIO0
34 // 0x00000100 [8] ISO (1) Pad isolation control
35 // 0x00000080 [7] OD (0) Output disable
36 // 0x00000040 [6] IE (0) Input enable
37 // 0x00000030 [5:4] DRIVE (0x1) Drive strength
38 // 0x00000008 [3] PUE (0) Pull up enable
39 // 0x00000004 [2] PDE (1) Pull down enable
40 // 0x00000002 [1] SCHMITT (1) Enable schmitt trigger
41 // 0x00000001 [0] SLEWFAST (0) Slew rate control
42 io_rw_32 io[48];
43} pads_bank0_hw_t;
44
45#define pads_bank0_hw ((pads_bank0_hw_t *)PADS_BANK0_BASE)
46static_assert(sizeof (pads_bank0_hw_t) == 0x00c4, "");
47
48#endif // _HARDWARE_STRUCTS_PADS_BANK0_H
49
address_mapped.h
pads_bank0_hw_t
Definition: pads_bank0.h:26