v2.0.0
SEGGER_RTT.h
1/*********************************************************************
2* SEGGER Microcontroller GmbH *
3* The Embedded Experts *
4**********************************************************************
5* *
6* (c) 1995 - 2021 SEGGER Microcontroller GmbH *
7* *
8* www.segger.com Support: support@segger.com *
9* *
10**********************************************************************
11* *
12* SEGGER RTT * Real Time Transfer for embedded targets *
13* *
14**********************************************************************
15* *
16* All rights reserved. *
17* *
18* SEGGER strongly recommends to not make any changes *
19* to or modify the source code of this software in order to stay *
20* compatible with the RTT protocol and J-Link. *
21* *
22* Redistribution and use in source and binary forms, with or *
23* without modification, are permitted provided that the following *
24* condition is met: *
25* *
26* o Redistributions of source code must retain the above copyright *
27* notice, this condition and the following disclaimer. *
28* *
29* THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND *
30* CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, *
31* INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF *
32* MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE *
33* DISCLAIMED. IN NO EVENT SHALL SEGGER Microcontroller BE LIABLE FOR *
34* ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR *
35* CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT *
36* OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; *
37* OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF *
38* LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT *
39* (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE *
40* USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH *
41* DAMAGE. *
42* *
43**********************************************************************
44* *
45* RTT version: 7.88c *
46* *
47**********************************************************************
48
49---------------------------END-OF-HEADER------------------------------
50File : SEGGER_RTT.h
51Purpose : Implementation of SEGGER real-time transfer which allows
52 real-time communication on targets which support debugger
53 memory accesses while the CPU is running.
54Revision: $Rev: 25842 $
55----------------------------------------------------------------------
56*/
57
58#ifndef SEGGER_RTT_H
59#define SEGGER_RTT_H
60
61#include "../Config/SEGGER_RTT_Conf.h"
62
63/*********************************************************************
64*
65* Defines, defaults
66*
67**********************************************************************
68*/
69
70#ifndef RTT_USE_ASM
71 //
72 // Some cores support out-of-order memory accesses (reordering of memory accesses in the core)
73 // For such cores, we need to define a memory barrier to guarantee the order of certain accesses to the RTT ring buffers.
74 // Needed for:
75 // Cortex-M7 (ARMv7-M)
76 // Cortex-M23 (ARM-v8M)
77 // Cortex-M33 (ARM-v8M)
78 // Cortex-A/R (ARM-v7A/R)
79 //
80 // We do not explicitly check for "Embedded Studio" as the compiler in use determines what we support.
81 // You can use an external toolchain like IAR inside ES. So there is no point in checking for "Embedded Studio"
82 //
83 #if (defined __CROSSWORKS_ARM) // Rowley Crossworks
84 #define _CC_HAS_RTT_ASM_SUPPORT 1
85 #if (defined __ARM_ARCH_7M__) // Cortex-M3
86 #define _CORE_HAS_RTT_ASM_SUPPORT 1
87 #elif (defined __ARM_ARCH_7EM__) // Cortex-M4/M7
88 #define _CORE_HAS_RTT_ASM_SUPPORT 1
89 #define _CORE_NEEDS_DMB 1
90 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
91 #elif (defined __ARM_ARCH_8M_BASE__) // Cortex-M23
92 #define _CORE_HAS_RTT_ASM_SUPPORT 0
93 #define _CORE_NEEDS_DMB 1
94 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
95 #elif (defined __ARM_ARCH_8M_MAIN__) // Cortex-M33
96 #define _CORE_HAS_RTT_ASM_SUPPORT 1
97 #define _CORE_NEEDS_DMB 1
98 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
99 #else
100 #define _CORE_HAS_RTT_ASM_SUPPORT 0
101 #endif
102 #elif (defined __ARMCC_VERSION)
103 //
104 // ARM compiler
105 // ARM compiler V6.0 and later is clang based.
106 // Our ASM part is compatible to clang.
107 //
108 #if (__ARMCC_VERSION >= 6000000)
109 #define _CC_HAS_RTT_ASM_SUPPORT 1
110 #else
111 #define _CC_HAS_RTT_ASM_SUPPORT 0
112 #endif
113 #if (defined __ARM_ARCH_6M__) // Cortex-M0 / M1
114 #define _CORE_HAS_RTT_ASM_SUPPORT 0 // No ASM support for this architecture
115 #elif (defined __ARM_ARCH_7M__) // Cortex-M3
116 #define _CORE_HAS_RTT_ASM_SUPPORT 1
117 #elif (defined __ARM_ARCH_7EM__) // Cortex-M4/M7
118 #define _CORE_HAS_RTT_ASM_SUPPORT 1
119 #define _CORE_NEEDS_DMB 1
120 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
121 #elif (defined __ARM_ARCH_8M_BASE__) // Cortex-M23
122 #define _CORE_HAS_RTT_ASM_SUPPORT 0
123 #define _CORE_NEEDS_DMB 1
124 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
125 #elif (defined __ARM_ARCH_8M_MAIN__) // Cortex-M33
126 #define _CORE_HAS_RTT_ASM_SUPPORT 1
127 #define _CORE_NEEDS_DMB 1
128 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
129 #elif ((defined __ARM_ARCH_7A__) || (defined __ARM_ARCH_7R__)) // Cortex-A/R 32-bit ARMv7-A/R
130 #define _CORE_NEEDS_DMB 1
131 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
132 #else
133 #define _CORE_HAS_RTT_ASM_SUPPORT 0
134 #endif
135 #elif ((defined __GNUC__) || (defined __clang__))
136 //
137 // GCC / Clang
138 //
139 #define _CC_HAS_RTT_ASM_SUPPORT 1
140 // ARM 7/9: __ARM_ARCH_5__ / __ARM_ARCH_5E__ / __ARM_ARCH_5T__ / __ARM_ARCH_5T__ / __ARM_ARCH_5TE__
141 #if (defined __ARM_ARCH_7M__) // Cortex-M3
142 #define _CORE_HAS_RTT_ASM_SUPPORT 1
143 #elif (defined __ARM_ARCH_7EM__) // Cortex-M4/M7
144 #define _CORE_HAS_RTT_ASM_SUPPORT 1
145 #define _CORE_NEEDS_DMB 1 // Only Cortex-M7 needs a DMB but we cannot distinguish M4 and M7 here...
146 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
147 #elif (defined __ARM_ARCH_8M_BASE__) // Cortex-M23
148 #define _CORE_HAS_RTT_ASM_SUPPORT 0
149 #define _CORE_NEEDS_DMB 1
150 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
151 #elif (defined __ARM_ARCH_8M_MAIN__) // Cortex-M33
152 #define _CORE_HAS_RTT_ASM_SUPPORT 1
153 #define _CORE_NEEDS_DMB 1
154 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
155 #elif ((defined __ARM_ARCH_7A__) || (defined __ARM_ARCH_7R__)) // Cortex-A/R 32-bit ARMv7-A/R
156 #define _CORE_NEEDS_DMB 1
157 #define RTT__DMB() __asm volatile ("dmb\n" : : :);
158 #else
159 #define _CORE_HAS_RTT_ASM_SUPPORT 0
160 #endif
161 #elif ((defined __IASMARM__) || (defined __ICCARM__))
162 //
163 // IAR assembler/compiler
164 //
165 #define _CC_HAS_RTT_ASM_SUPPORT 1
166 #if (__VER__ < 6300000)
167 #define VOLATILE
168 #else
169 #define VOLATILE volatile
170 #endif
171 #if (defined __ARM7M__) // Needed for old versions that do not know the define yet
172 #if (__CORE__ == __ARM7M__) // Cortex-M3
173 #define _CORE_HAS_RTT_ASM_SUPPORT 1
174 #endif
175 #endif
176 #if (defined __ARM7EM__)
177 #if (__CORE__ == __ARM7EM__) // Cortex-M4/M7
178 #define _CORE_HAS_RTT_ASM_SUPPORT 1
179 #define _CORE_NEEDS_DMB 1
180 #define RTT__DMB() asm VOLATILE ("DMB");
181 #endif
182 #endif
183 #if (defined __ARM8M_BASELINE__)
184 #if (__CORE__ == __ARM8M_BASELINE__) // Cortex-M23
185 #define _CORE_HAS_RTT_ASM_SUPPORT 0
186 #define _CORE_NEEDS_DMB 1
187 #define RTT__DMB() asm VOLATILE ("DMB");
188 #endif
189 #endif
190 #if (defined __ARM8M_MAINLINE__)
191 #if (__CORE__ == __ARM8M_MAINLINE__) // Cortex-M33
192 #define _CORE_HAS_RTT_ASM_SUPPORT 1
193 #define _CORE_NEEDS_DMB 1
194 #define RTT__DMB() asm VOLATILE ("DMB");
195 #endif
196 #endif
197 #if (defined __ARM8EM_MAINLINE__)
198 #if (__CORE__ == __ARM8EM_MAINLINE__) // Cortex-???
199 #define _CORE_HAS_RTT_ASM_SUPPORT 1
200 #define _CORE_NEEDS_DMB 1
201 #define RTT__DMB() asm VOLATILE ("DMB");
202 #endif
203 #endif
204 #if (defined __ARM7A__)
205 #if (__CORE__ == __ARM7A__) // Cortex-A 32-bit ARMv7-A
206 #define _CORE_NEEDS_DMB 1
207 #define RTT__DMB() asm VOLATILE ("DMB");
208 #endif
209 #endif
210 #if (defined __ARM7R__)
211 #if (__CORE__ == __ARM7R__) // Cortex-R 32-bit ARMv7-R
212 #define _CORE_NEEDS_DMB 1
213 #define RTT__DMB() asm VOLATILE ("DMB");
214 #endif
215 #endif
216// TBD: __ARM8A__ => Cortex-A 64-bit ARMv8-A
217// TBD: __ARM8R__ => Cortex-R 64-bit ARMv8-R
218 #else
219 //
220 // Other compilers
221 //
222 #define _CC_HAS_RTT_ASM_SUPPORT 0
223 #define _CORE_HAS_RTT_ASM_SUPPORT 0
224 #endif
225 //
226 // If IDE and core support the ASM version, enable ASM version by default
227 //
228 #ifndef _CORE_HAS_RTT_ASM_SUPPORT
229 #define _CORE_HAS_RTT_ASM_SUPPORT 0 // Default for unknown cores
230 #endif
231 #if (_CC_HAS_RTT_ASM_SUPPORT && _CORE_HAS_RTT_ASM_SUPPORT)
232 #define RTT_USE_ASM (1)
233 #else
234 #define RTT_USE_ASM (0)
235 #endif
236#endif
237
238#ifndef _CORE_NEEDS_DMB
239 #define _CORE_NEEDS_DMB 0
240#endif
241
242#ifndef RTT__DMB
243 #if _CORE_NEEDS_DMB
244 #error "Don't know how to place inline assembly for DMB"
245 #else
246 #define RTT__DMB()
247 #endif
248#endif
249
250#ifndef SEGGER_RTT_CPU_CACHE_LINE_SIZE
251 #define SEGGER_RTT_CPU_CACHE_LINE_SIZE (0) // On most target systems where RTT is used, we do not have a CPU cache, therefore 0 is a good default here
252#endif
253
254#ifndef SEGGER_RTT_UNCACHED_OFF
255 #if SEGGER_RTT_CPU_CACHE_LINE_SIZE
256 #error "SEGGER_RTT_UNCACHED_OFF must be defined when setting SEGGER_RTT_CPU_CACHE_LINE_SIZE != 0"
257 #else
258 #define SEGGER_RTT_UNCACHED_OFF (0)
259 #endif
260#endif
261#if RTT_USE_ASM
262 #if SEGGER_RTT_CPU_CACHE_LINE_SIZE
263 #error "RTT_USE_ASM is not available if SEGGER_RTT_CPU_CACHE_LINE_SIZE != 0"
264 #endif
265#endif
266
267#ifndef SEGGER_RTT_ASM // defined when SEGGER_RTT.h is included from assembly file
268#include <stdlib.h>
269#include <stdarg.h>
270
271/*********************************************************************
272*
273* Defines, fixed
274*
275**********************************************************************
276*/
277
278//
279// Determine how much we must pad the control block to make it a multiple of a cache line in size
280// Assuming: U8 = 1B
281// U16 = 2B
282// U32 = 4B
283// U8/U16/U32* = 4B
284//
285#if SEGGER_RTT_CPU_CACHE_LINE_SIZE // Avoid division by zero in case we do not have any cache
286 #define SEGGER_RTT__ROUND_UP_2_CACHE_LINE_SIZE(NumBytes) (((NumBytes + SEGGER_RTT_CPU_CACHE_LINE_SIZE - 1) / SEGGER_RTT_CPU_CACHE_LINE_SIZE) * SEGGER_RTT_CPU_CACHE_LINE_SIZE)
287#else
288 #define SEGGER_RTT__ROUND_UP_2_CACHE_LINE_SIZE(NumBytes) (NumBytes)
289#endif
290#define SEGGER_RTT__CB_SIZE (16 + 4 + 4 + (SEGGER_RTT_MAX_NUM_UP_BUFFERS * 24) + (SEGGER_RTT_MAX_NUM_DOWN_BUFFERS * 24))
291#define SEGGER_RTT__CB_PADDING (SEGGER_RTT__ROUND_UP_2_CACHE_LINE_SIZE(SEGGER_RTT__CB_SIZE) - SEGGER_RTT__CB_SIZE)
292
293/*********************************************************************
294*
295* Types
296*
297**********************************************************************
298*/
299
300//
301// Description for a circular buffer (also called "ring buffer")
302// which is used as up-buffer (T->H)
303//
304 typedef struct {
305 const char* sName; // Optional name. Standard names so far are: "Terminal", "SysView", "J-Scope_t4i4"
306 char* pBuffer; // Pointer to start of buffer
307 unsigned SizeOfBuffer; // Buffer size in bytes. Note that one byte is lost, as this implementation does not fill up the buffer in order to avoid the problem of being unable to distinguish between full and empty.
308 unsigned WrOff; // Position of next item to be written by either target.
309 volatile unsigned RdOff; // Position of next item to be read by host. Must be volatile since it may be modified by host.
310 unsigned Flags; // Contains configuration flags. Flags[31:24] are used for validity check and must be zero. Flags[23:2] are reserved for future use. Flags[1:0] = RTT operating mode.
311} SEGGER_RTT_BUFFER_UP;
312
313//
314// Description for a circular buffer (also called "ring buffer")
315// which is used as down-buffer (H->T)
316//
317 typedef struct {
318 const char* sName; // Optional name. Standard names so far are: "Terminal", "SysView", "J-Scope_t4i4"
319 char* pBuffer; // Pointer to start of buffer
320 unsigned SizeOfBuffer; // Buffer size in bytes. Note that one byte is lost, as this implementation does not fill up the buffer in order to avoid the problem of being unable to distinguish between full and empty.
321 volatile unsigned WrOff; // Position of next item to be written by host. Must be volatile since it may be modified by host.
322 unsigned RdOff; // Position of next item to be read by target (down-buffer).
323 unsigned Flags; // Contains configuration flags. Flags[31:24] are used for validity check and must be zero. Flags[23:2] are reserved for future use. Flags[1:0] = RTT operating mode.
324} SEGGER_RTT_BUFFER_DOWN;
325
326//
327// RTT control block which describes the number of buffers available
328// as well as the configuration for each buffer
329//
330//
331 typedef struct {
332 char acID[16]; // Initialized to "SEGGER RTT"
333 int MaxNumUpBuffers; // Initialized to SEGGER_RTT_MAX_NUM_UP_BUFFERS (type. 2)
334 int MaxNumDownBuffers; // Initialized to SEGGER_RTT_MAX_NUM_DOWN_BUFFERS (type. 2)
335 SEGGER_RTT_BUFFER_UP aUp[SEGGER_RTT_MAX_NUM_UP_BUFFERS]; // Up buffers, transferring information up from target via debug probe to host
336 SEGGER_RTT_BUFFER_DOWN aDown[SEGGER_RTT_MAX_NUM_DOWN_BUFFERS]; // Down buffers, transferring information down from host via debug probe to target
337#if SEGGER_RTT__CB_PADDING
338 unsigned char aDummy[SEGGER_RTT__CB_PADDING];
339#endif
340} SEGGER_RTT_CB;
341
342/*********************************************************************
343*
344* Global data
345*
346**********************************************************************
347*/
348extern SEGGER_RTT_CB _SEGGER_RTT;
349
350/*********************************************************************
351*
352* RTT API functions
353*
354**********************************************************************
355*/
356#ifdef __cplusplus
357 extern "C" {
358#endif
359int SEGGER_RTT_AllocDownBuffer (const char* sName, void* pBuffer, unsigned BufferSize, unsigned Flags);
360int SEGGER_RTT_AllocUpBuffer (const char* sName, void* pBuffer, unsigned BufferSize, unsigned Flags);
361int SEGGER_RTT_ConfigUpBuffer (unsigned BufferIndex, const char* sName, void* pBuffer, unsigned BufferSize, unsigned Flags);
362int SEGGER_RTT_ConfigDownBuffer (unsigned BufferIndex, const char* sName, void* pBuffer, unsigned BufferSize, unsigned Flags);
363int SEGGER_RTT_GetKey (void);
364unsigned SEGGER_RTT_HasData (unsigned BufferIndex);
365int SEGGER_RTT_HasKey (void);
366unsigned SEGGER_RTT_HasDataUp (unsigned BufferIndex);
367void SEGGER_RTT_Init (void);
368unsigned SEGGER_RTT_Read (unsigned BufferIndex, void* pBuffer, unsigned BufferSize);
369unsigned SEGGER_RTT_ReadNoLock (unsigned BufferIndex, void* pData, unsigned BufferSize);
370int SEGGER_RTT_SetNameDownBuffer (unsigned BufferIndex, const char* sName);
371int SEGGER_RTT_SetNameUpBuffer (unsigned BufferIndex, const char* sName);
372int SEGGER_RTT_SetFlagsDownBuffer (unsigned BufferIndex, unsigned Flags);
373int SEGGER_RTT_SetFlagsUpBuffer (unsigned BufferIndex, unsigned Flags);
374int SEGGER_RTT_WaitKey (void);
375unsigned SEGGER_RTT_Write (unsigned BufferIndex, const void* pBuffer, unsigned NumBytes);
376unsigned SEGGER_RTT_WriteNoLock (unsigned BufferIndex, const void* pBuffer, unsigned NumBytes);
377unsigned SEGGER_RTT_WriteSkipNoLock (unsigned BufferIndex, const void* pBuffer, unsigned NumBytes);
378unsigned SEGGER_RTT_ASM_WriteSkipNoLock (unsigned BufferIndex, const void* pBuffer, unsigned NumBytes);
379unsigned SEGGER_RTT_WriteString (unsigned BufferIndex, const char* s);
380void SEGGER_RTT_WriteWithOverwriteNoLock(unsigned BufferIndex, const void* pBuffer, unsigned NumBytes);
381unsigned SEGGER_RTT_PutChar (unsigned BufferIndex, char c);
382unsigned SEGGER_RTT_PutCharSkip (unsigned BufferIndex, char c);
383unsigned SEGGER_RTT_PutCharSkipNoLock (unsigned BufferIndex, char c);
384unsigned SEGGER_RTT_GetAvailWriteSpace (unsigned BufferIndex);
385unsigned SEGGER_RTT_GetBytesInBuffer (unsigned BufferIndex);
386//
387// Function macro for performance optimization
388//
389#define SEGGER_RTT_HASDATA(n) (((SEGGER_RTT_BUFFER_DOWN*)((char*)&_SEGGER_RTT.aDown[n] + SEGGER_RTT_UNCACHED_OFF))->WrOff - ((SEGGER_RTT_BUFFER_DOWN*)((char*)&_SEGGER_RTT.aDown[n] + SEGGER_RTT_UNCACHED_OFF))->RdOff)
390
391#if RTT_USE_ASM
392 #define SEGGER_RTT_WriteSkipNoLock SEGGER_RTT_ASM_WriteSkipNoLock
393#endif
394
395/*********************************************************************
396*
397* RTT transfer functions to send RTT data via other channels.
398*
399**********************************************************************
400*/
401unsigned SEGGER_RTT_ReadUpBuffer (unsigned BufferIndex, void* pBuffer, unsigned BufferSize);
402unsigned SEGGER_RTT_ReadUpBufferNoLock (unsigned BufferIndex, void* pData, unsigned BufferSize);
403unsigned SEGGER_RTT_WriteDownBuffer (unsigned BufferIndex, const void* pBuffer, unsigned NumBytes);
404unsigned SEGGER_RTT_WriteDownBufferNoLock (unsigned BufferIndex, const void* pBuffer, unsigned NumBytes);
405
406#define SEGGER_RTT_HASDATA_UP(n) (((SEGGER_RTT_BUFFER_UP*)((char*)&_SEGGER_RTT.aUp[n] + SEGGER_RTT_UNCACHED_OFF))->WrOff - ((SEGGER_RTT_BUFFER_UP*)((char*)&_SEGGER_RTT.aUp[n] + SEGGER_RTT_UNCACHED_OFF))->RdOff) // Access uncached to make sure we see changes made by the J-Link side and all of our changes go into HW directly
407
408/*********************************************************************
409*
410* RTT "Terminal" API functions
411*
412**********************************************************************
413*/
414int SEGGER_RTT_SetTerminal (unsigned char TerminalId);
415int SEGGER_RTT_TerminalOut (unsigned char TerminalId, const char* s);
416
417/*********************************************************************
418*
419* RTT printf functions (require SEGGER_RTT_printf.c)
420*
421**********************************************************************
422*/
423int SEGGER_RTT_printf(unsigned BufferIndex, const char * sFormat, ...);
424int SEGGER_RTT_vprintf(unsigned BufferIndex, const char * sFormat, va_list * pParamList);
425
426#ifdef __cplusplus
427 }
428#endif
429
430#endif // ifndef(SEGGER_RTT_ASM)
431
432/*********************************************************************
433*
434* Defines
435*
436**********************************************************************
437*/
438
439//
440// Operating modes. Define behavior if buffer is full (not enough space for entire message)
441//
442#define SEGGER_RTT_MODE_NO_BLOCK_SKIP (0) // Skip. Do not block, output nothing. (Default)
443#define SEGGER_RTT_MODE_NO_BLOCK_TRIM (1) // Trim: Do not block, output as much as fits.
444#define SEGGER_RTT_MODE_BLOCK_IF_FIFO_FULL (2) // Block: Wait until there is space in the buffer.
445#define SEGGER_RTT_MODE_MASK (3)
446
447//
448// Control sequences, based on ANSI.
449// Can be used to control color, and clear the screen
450//
451#define RTT_CTRL_RESET "\x1B[0m" // Reset to default colors
452#define RTT_CTRL_CLEAR "\x1B[2J" // Clear screen, reposition cursor to top left
453
454#define RTT_CTRL_TEXT_BLACK "\x1B[2;30m"
455#define RTT_CTRL_TEXT_RED "\x1B[2;31m"
456#define RTT_CTRL_TEXT_GREEN "\x1B[2;32m"
457#define RTT_CTRL_TEXT_YELLOW "\x1B[2;33m"
458#define RTT_CTRL_TEXT_BLUE "\x1B[2;34m"
459#define RTT_CTRL_TEXT_MAGENTA "\x1B[2;35m"
460#define RTT_CTRL_TEXT_CYAN "\x1B[2;36m"
461#define RTT_CTRL_TEXT_WHITE "\x1B[2;37m"
462
463#define RTT_CTRL_TEXT_BRIGHT_BLACK "\x1B[1;30m"
464#define RTT_CTRL_TEXT_BRIGHT_RED "\x1B[1;31m"
465#define RTT_CTRL_TEXT_BRIGHT_GREEN "\x1B[1;32m"
466#define RTT_CTRL_TEXT_BRIGHT_YELLOW "\x1B[1;33m"
467#define RTT_CTRL_TEXT_BRIGHT_BLUE "\x1B[1;34m"
468#define RTT_CTRL_TEXT_BRIGHT_MAGENTA "\x1B[1;35m"
469#define RTT_CTRL_TEXT_BRIGHT_CYAN "\x1B[1;36m"
470#define RTT_CTRL_TEXT_BRIGHT_WHITE "\x1B[1;37m"
471
472#define RTT_CTRL_BG_BLACK "\x1B[24;40m"
473#define RTT_CTRL_BG_RED "\x1B[24;41m"
474#define RTT_CTRL_BG_GREEN "\x1B[24;42m"
475#define RTT_CTRL_BG_YELLOW "\x1B[24;43m"
476#define RTT_CTRL_BG_BLUE "\x1B[24;44m"
477#define RTT_CTRL_BG_MAGENTA "\x1B[24;45m"
478#define RTT_CTRL_BG_CYAN "\x1B[24;46m"
479#define RTT_CTRL_BG_WHITE "\x1B[24;47m"
480
481#define RTT_CTRL_BG_BRIGHT_BLACK "\x1B[4;40m"
482#define RTT_CTRL_BG_BRIGHT_RED "\x1B[4;41m"
483#define RTT_CTRL_BG_BRIGHT_GREEN "\x1B[4;42m"
484#define RTT_CTRL_BG_BRIGHT_YELLOW "\x1B[4;43m"
485#define RTT_CTRL_BG_BRIGHT_BLUE "\x1B[4;44m"
486#define RTT_CTRL_BG_BRIGHT_MAGENTA "\x1B[4;45m"
487#define RTT_CTRL_BG_BRIGHT_CYAN "\x1B[4;46m"
488#define RTT_CTRL_BG_BRIGHT_WHITE "\x1B[4;47m"
489
490
491#endif
492
493/*************************** End of file ****************************/
stdlib.h
SEGGER_RTT_BUFFER_DOWN
Definition: SEGGER_RTT.h:317
SEGGER_RTT_BUFFER_UP
Definition: SEGGER_RTT.h:304
SEGGER_RTT_CB
Definition: SEGGER_RTT.h:331