Vin: V

Vout: V

Iout: A

Vo_max: V

Temp1: °C

Temp2: °C

DC 5V: V

Out Mode: N/A

Work State: N/A

# Alientek DP100

Just plug in the DP100 using the USB-A to USB-A cable (make sure it's in "USBD" mode; double-tap ◀ to switch), and click connect!

## Connect...

# Alientek DP100 / High Performance Digital Power

If you like this project, you can buy me a cup of coffee ☕
Bitcoin(BTC): 19xg6pA4RzSW3o4ZUyTyn5t4tY3tqLXHbe
TonCoin(TON): UQBY_xXK_25L-UHq_h2ocfhS0c_lZoA4PIHxt-SktxLa_So7

0
Volts
0
Amps
0
Load