---
<!-- Copyright © SixtyFPS GmbH <info@slint.dev> ; SPDX-License-Identifier: MIT -->
title: Embedded 
description: Embedded Platforms on which Slint has been tested
---

{/* cSpell: Toradex Vivante espflash pico */}

import { Tabs, TabItem } from '@astrojs/starlight/components';

Slint runs on many embedded platforms.

The platform descriptions below cover what has been tested for deployment. For the development environment,
we recommend using a recent desktop operating system and compiler version.

## Embedded Linux

Slint runs on a variety of embedded Linux platforms. Generally speaking, Slint requires a modern Linux userspace
with working OpenGL ES 2.0 (or newer) or Vulkan drivers. We've had success running Slint on

-   Yocto based distributions. 
-   BuildRoot based distributions.
-   Torizon.

<Tabs>
<TabItem label="Yocto Linux">
For C++ applications see [meta-slint](https://github.com/slint-ui/meta-slint) for recipes. 

Rust application work out of the box with Yocto's Rust support.
</TabItem>
<TabItem label="Torizon">
Toradex provides [TorizonCore](https://developer.toradex.com/torizon/), a Linux based platform for its embedded devices that packages applications in docker containers.

We provide our demos compiled for Toradex as docker containers.

#### Prerequisites

 - A device running Torizon
 - A running [weston container](https://developer.toradex.com/torizon/5.0/provided-containers/working-with-weston-on-torizoncore)
 - SSH access to the Torizon device

#### Running

Our pre-compiled demos are available in four different variants:

1. Compiled for ARM 32-bit as `armhf` and compiled for ARM 64-bit as `arm64`
2. Compiled with Linux DRI or with support for Vivante GPUs (`-vivante` suffix)

A complete list of all containers can be found at

https://github.com/orgs/slint-ui/packages?q=torizon&tab=packages&q=torizon

For example, to run the container on an i.MX8 board with Vivante GPU, use the following command line:

```
docker run --user=torizon -v /dev:/dev -v /tmp:/tmp --device-cgroup-rule='c 199:* rmw' --device-cgroup-rule='c 226:* rmw' ghcr.io/slint-ui/slint/torizon-demos-arm64-vivante
```

#### Selecting Demos

By default, the printer demo from /usr/bin is run. The containers however package multiple demos:

 * printerdemo
 * slide_puzzle
 * gallery
 * opengl_underlay
 * carousel
 * todo
 * energy-monitor
 * home-automation

Run then by specifying them as parameter to `docker run`, for example:

```
docker run --user=torizon -v /dev:/dev -v /tmp:/tmp --device-cgroup-rule='c 199:* rmw' --device-cgroup-rule='c 226:* rmw' ghcr.io/slint-ui/slint/torizon-demos-arm64-vivante opengl_underlay
```
</TabItem>
</Tabs>

## Microcontrollers

Slint's platform abstraction allows for integration into any Rust or C++ based Microcontroller development
environment. Developers need to implement functionality to feed input events such as touch or keyboard, as
well as displaying the pixels rendered by Slint into a frame- or linebuffer.

<Tabs syncKey="dev-language">
<TabItem label="C++">
We provide templates for a few off-the-shelf development boards from some of the silicon vendors.
</TabItem>
<TabItem label="Rust">
You will need to use the `mcu-board-support` crate. This crate re-export a `entry` attribute macro to apply to the `main` function, and a `init()`
function that should be called before creating the Slint UI.

In order to use this backend, the final program must depend on both `slint` and `mcu-board-support`.
The main.rs will look something like this

```rust
#![no_std]
#![cfg_attr(not(feature = "simulator"), no_main)]
slint::include_modules!();

#[mcu_board_support::entry]
fn main() -> ! {
    mcu_board_support::init();
    MainWindow::new().run();
    panic!("The event loop should not return");
}
```

Since mcu-board-support is at the moment an internal crate not uploaded to crates.io, you must
use the git version of slint, slint-build, and mcu-board-support

```toml
[dependencies]
slint = { git = "https://github.com/slint-ui/slint", default-features = false }
mcu-board-support = { git = "https://github.com/slint-ui/slint" }
# ...
[build-dependencies]
slint-build = { git = "https://github.com/slint-ui/slint" }
```

In your build.rs, you must include a call to `slint_build::print_rustc_flags().unwrap()` to set some of the flags.

</TabItem>
</Tabs>

### Espressif (ESP32)

<Tabs syncKey="dev-language">
<TabItem label="C++">
To use Slint with your C++ application, you can follow the instructions on the [Espressif Documentation site](https://components.espressif.com/components/slint/slint)
</TabItem>
<TabItem label="Rust">
#### Prerequisites

 * ESP Rust Toolchain: https://esp-rs.github.io/book/installation/installation.html
 * `espflash`: Install via `cargo install espflash`.

When flashing, with `espflash`, you will be prompted to select a USB port. If this port is always the same, then you can also pass it as a parameter on the command line to avoid the prompt. For example if
`/dev/ttyUSB1` is the device file for your port, the command line changes to `espflash --monitor /dev/ttyUSB1 path/to/binary/to/flash_and_monitor`.

#### ESP32-S2-Kaluga-1

To compile and run the Slint Printer demo:

```sh
CARGO_PROFILE_RELEASE_OPT_LEVEL=s cargo +esp run -p printerdemo_mcu --target xtensa-esp32s2-none-elf --no-default-features --features=mcu-board-support/esp32-s2-kaluga-1 --release --config examples/mcu-board-support/esp32_s2_kaluga_1/cargo-config.toml
```

The device needs to be connected with the two USB cables (one for power, one for data)

#### ESP32-S3-Box

To compile and run the Slint Printer demo:

```sh
CARGO_PROFILE_RELEASE_OPT_LEVEL=s cargo +esp run -p printerdemo_mcu --target xtensa-esp32s3-none-elf --no-default-features --features=mcu-board-support/esp32-s3-box --release --config examples/mcu-board-support/esp32_s3_box/cargo-config.toml
```
</TabItem>
</Tabs>

### ST (STM32)

<Tabs syncKey="dev-language">
<TabItem label="C++">
#### STM32H735G-DK
You can start with the template [slint-cpp-template-stm32h735g-dk.zip](https://github.com/slint-ui/slint/releases/download/%7Bdownload_version%7D/slint-cpp-template-stm32h735g-dk.zip)

#### STM32H747I-DISCO
You can start with the template [slint-cpp-template-stm32h747i-disco.zip](https://github.com/slint-ui/slint/releases/download/%7Bdownload_version%7D/slint-cpp-template-stm32h747i-disco.zip)

</TabItem>
<TabItem label="Rust">
Follow the steps below to run the Slint Printer Demo 

#### STM32H735G-DK

Using [probe-rs](https://probe.rs).

```sh
CARGO_PROFILE_RELEASE_OPT_LEVEL=s CARGO_TARGET_THUMBV7EM_NONE_EABIHF_RUNNER="probe-rs run --chip STM32H735IGKx" cargo run -p printerdemo_mcu --no-default-features  --features=mcu-board-support/stm32h735g --target=thumbv7em-none-eabihf --release
```
</TabItem>
</Tabs>

### Raspberry Pi (Pico)

Only Rust programs are currently supported on the Raspberry Pi Pico.

#### On the Raspberry Pi Pico

Build the Slint Printer demo with:

```sh
cargo build -p printerdemo_mcu --no-default-features --features=mcu-board-support/pico-st7789 --target=thumbv6m-none-eabi --release
```

The resulting file can be flashed conveniently with [elf2uf2-rs](https://github.com/jonil/elf2uf2-rs). Install it using `cargo install`:

```sh
cargo install elf2uf2-rs
```

Then upload the demo to the Raspberry Pi Pico: push the "bootsel" white button on the device while connecting the
micro-usb cable to the device, this connect some storage where you can store the binary.

Or from the command on linux: (connect the device while pressing the "bootsel" button.

```sh
# If you're on Linux: mount the device
udisksctl mount -b /dev/sda1
# upload
elf2uf2-rs -d target/thumbv6m-none-eabi/release/printerdemo_mcu
```

#### On the Raspberry Pi Pico2

Build the Slint Printer demo with:

```sh
cargo build -p printerdemo_mcu --no-default-features --features=mcu-board-support/pico2-st7789 --target=thumbv8m.main-none-eabihf --release
```

The resulting file can be flashed conveniently with [picotool](https://github.com/raspberrypi/picotool). You should build it from source.

Then upload the demo to the Raspberry Pi Pico: push the "bootsel" white button on the device while connecting the
micro-usb cable to the device, this connects some USB storage on your workstation where you can store the binary.

Or from the command on linux (connect the device while pressing the "bootsel" button):

```sh
# If you're on Linux: mount the device
udisksctl mount -b /dev/sda1
# upload
picotool load -u -v -x -t elf target/thumbv8m.main-none-eabihf/release/printerdemo_mcu
```

#### Using probe-rs

This requires [probe-rs](https://probe.rs) and to connect the pico via a probe
(for example another pico running the probe).

Then you can simply run with `cargo run`

```sh
CARGO_TARGET_THUMBV6M_NONE_EABI_LINKER="flip-link" CARGO_TARGET_THUMBV6M_NONE_EABI_RUNNER="probe-rs run --chip RP2040" cargo run -p printerdemo_mcu --no-default-features --features=mcu-board-support/pico-st7789 --target=thumbv6m-none-eabi --release
```

#### Flashing and Debugging the Pico with `probe-rs`'s VSCode Plugin

Install `probe-rs-debugger` and the VSCode plugin as described [here](https://probe.rs/docs/tools/vscode/).

Add this build task to your `.vscode/tasks.json`:
```json
{
	"version": "2.0.0",
	"tasks": [
		{
			"type": "cargo",
			"command": "build",
			"args": [
				"--package=printerdemo_mcu",
				"--features=mcu-pico-st7789",
				"--target=thumbv6m-none-eabi",
				"--profile=release-with-debug"
			],
			"problemMatcher": [
				"$rustc"
			],
			"group": "build",
			"label": "build mcu demo for pico"
		},
	]
}
```

The `release-with-debug` profile is needed, because the debug build does not fit into flash.

You can define it like this in your top level `Cargo.toml`:

```toml
[profile.release-with-debug]
inherits = "release"
debug = true
```

Now you can add the launch configuration to `.vscode/launch.json`:

```json
{
    "version": "0.2.0",
    "configurations": [
        {
            "preLaunchTask": "build mcu demo for pico",
            "type": "probe-rs-debug",
            "request": "launch",
            "name": "Flash and Debug MCU Demo",
            "cwd": "${workspaceFolder}",
            "connectUnderReset": false,
            "chip": "RP2040",
            "flashingConfig": {
                "flashingEnabled": true,
                "resetAfterFlashing": true,
                "haltAfterReset": true
            },
            "coreConfigs": [
                {
                    "coreIndex": 0,
                    "rttEnabled": true,
                    "programBinary": "./target/thumbv6m-none-eabi/release-with-debug/printerdemo_mcu"
                }
            ]
        },
    ]
}
```

This was tested using a second Raspberry Pi Pico programmed as a probe with [DapperMime](https://github.com/majbthrd/DapperMime).

## What about other platforms?
[Contact us](https://slint.dev/contact) if you need to support specific or older versions.
