panel size, 143x195mm
PCB thickness, 1.6mm
number of layers, 2
soldermask color, Red
silkscreen color, White
oz copper, 1oz
finish, HASL lead free
stencils, top+bottom
pcs per panel, 35
min trace width, 0.203200mm / 0.008000in
min drill size, 0.381000mm / 0.015000in
