# Probably realistic but impractical with *current year* technology coilgun specifications used in this mod.

## GC166 Gauss Carbine

* Single shot power consumption: 6.68 kJ

  **Capacitor
      Dielectric composition: hafnia
      Diameter: 4 cm
      Length: 8.9 cm
      Separation: 100 nm
      Breakdown voltage: 100 V
      Capacitance: 1.24 F
      Total energy: 3.96 kJ
      Charge time: 59.3 ms

  **Coil
      Composition: maraging steel
      Wire diameter: 1 mm
      Number of turns: 45
      Number of layers: 1

  Number of stages: 1

  **Barrel reinforcement / heat dissipation  
      Composition: reinforced carbon-carbon
      Thickness:  1.4 cm

  **Armature
      Name: magpin
      Composition: iron
      Bore diameter: Same as nails and flechettes
      Mass: 4 g
      Compatible alternatives: nail, flechette.

  Length: 500 mm
  Mass(no mag): 2.22 kg
  Muzzle velocity: 900 m/s
  Projectile energy: 1.62 kJ w/ magpins
  Maximum range: 500 m w/ magpins
  Rate of fire: 600 rpm
  Magazine: 120-round helical

----------------------------------------

## GG285 Gauss Gun

* Single shot power consumption: 8.55 kJ

  **Capacitor
      Dielectric composition: hafnia
      Diameter  5.4 cm
      Length: 9.1 cm
      Separation: 100 nm
      Breakdown voltage: 100 V
      Capacitance: 2.31 F
      Total energy: 7.38 kJ
      Charge time: 86.3 ms

  **Coil
      Composition: maraging steel
      Wire diameter: 7 mm
      Number of turns: 47
      Number of layers: 1
      
  Number of stages: 1

  **Barrel reinforcement / heat dissipation
      Composition: reinforced carbon-carbon
      Thickness: 4.3 mm

  **Armature
      Name: 1.06mm magmg
      Composition: magnetic metal glass *( info: https://en.wikipedia.org/wiki/Amorphous_metal )
      Bore diameter: 1.06 mm
      Mass: 1 g
      Compatible alternatives: none

  Length: 742 mm
  Mass(no mag): 3.27 kg
  Muzzle velocity: 2520 m/s
  Projectile energy: 3.19 kJ
  Maximum range: > 1 km
  Rate of fire: 600 rpm
  Magazine: 300-round helical