board_rotenc

This sample code demonstrates the use of a virtual Panasonic EVEP rotary
encoder. The encoder is hooked up to an LED array, and is used to scroll
an LED up and down. It behaves just like in real life, except contact
bounce is not modelled.
