| LibDriver LLCC68 1.0.0 LLCC68 full function driver

### - l -

- llcc68_cad_test() : driver_llcc68_cad_test.c , driver_llcc68_cad_test.h
- llcc68_cad_test_irq_handler() : driver_llcc68_cad_test.c , driver_llcc68_cad_test.h
- llcc68_check_packet_error() : driver_llcc68.c , driver_llcc68.h
- llcc68_clear_device_errors() : driver_llcc68.c , driver_llcc68.h
- llcc68_clear_irq_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_continuous_receive() : driver_llcc68.c , driver_llcc68.h
- llcc68_deinit() : driver_llcc68.c , driver_llcc68.h
- llcc68_frequency_convert_to_data() : driver_llcc68.c , driver_llcc68.h
- llcc68_frequency_convert_to_register() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_device_errors() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_dio3_output_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_dio_input_enable() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_dio_output_enable() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_event_mask() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_broadcast_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_crc_initical_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_crc_polynomial_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_node_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_sync_word() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_whitening_initial_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_gfsk_packet_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_instantaneous_rssi() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_iq_polarity() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_irq_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_lora_packet_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_lora_sync_word() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_ocp() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_packet_type() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_pull_down_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_pull_up_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_random_number() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_rtc_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_rx_buffer_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_rx_gain() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_stats() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_tx_clamp_config() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_tx_modulation() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_xta_trim() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_xtb_trim() : driver_llcc68.c , driver_llcc68.h
- llcc68_gfsk_bit_rate_convert_to_data() : driver_llcc68.c , driver_llcc68.h
- llcc68_gfsk_bit_rate_convert_to_register() : driver_llcc68.c , driver_llcc68.h
- llcc68_gfsk_frequency_deviation_convert_to_data() : driver_llcc68.c , driver_llcc68.h
- llcc68_gfsk_frequency_deviation_convert_to_register() : driver_llcc68.c , driver_llcc68.h
- llcc68_info() : driver_llcc68.c , driver_llcc68.h
- llcc68_init() : driver_llcc68.c , driver_llcc68.h
- llcc68_interface_busy_gpio_deinit() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_busy_gpio_init() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_busy_gpio_read() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_debug_print() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_delay_ms() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_receive_callback() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_reset_gpio_deinit() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_reset_gpio_init() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_reset_gpio_write() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_spi_deinit() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_spi_init() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_spi_write_read() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interrupt_test_irq_handler() : driver_llcc68_send_receive_test.c , driver_llcc68_send_receive_test.h
- llcc68_irq_handler() : driver_llcc68.c , driver_llcc68.h
- llcc68_lora_cad() : driver_llcc68.c , driver_llcc68.h
- llcc68_lora_check_packet_error() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_deinit() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_get_status() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_init() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_irq_handler() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_run_cad() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_send() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_set_continuous_receive_mode() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_set_send_mode() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_set_shot_receive_mode() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_sleep() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_transmit() : driver_llcc68.c , driver_llcc68.h
- llcc68_lora_wake_up() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_read_buffer() : driver_llcc68.c , driver_llcc68.h
- llcc68_read_register() : driver_llcc68.c , driver_llcc68.h
- llcc68_receive_test() : driver_llcc68_send_receive_test.c , driver_llcc68_send_receive_test.h
- llcc68_register_test() : driver_llcc68_register_test.c , driver_llcc68_register_test.h
- llcc68_reset_stats() : driver_llcc68.c , driver_llcc68.h
- llcc68_send_test() : driver_llcc68_send_receive_test.c , driver_llcc68_send_receive_test.h
- llcc68_set_buffer_base_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_cad() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_cad_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_calibration() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_calibration_image() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio2_as_rf_switch_ctrl() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio3_as_tcxo_ctrl() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio3_output_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio_input_enable() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio_irq_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio_output_enable() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_event_mask() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_frequency_synthesis() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_broadcast_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_crc_initical_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_crc_polynomial_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_node_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_sync_word() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_whitening_initial_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_gfsk_modulation_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_gfsk_packet_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_iq_polarity() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_lora_modulation_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_lora_packet_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_lora_symb_num_timeout() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_lora_sync_word() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_ocp() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_pa_config() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_packet_type() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_pull_down_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_pull_up_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_regulator_mode() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rf_frequency() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rtc_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rx() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rx_duty_cycle() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rx_gain() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rx_tx_fallback_mode() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_sleep() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_standby() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_stop_timer_on_preamble() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_clamp_config() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_continuous_wave() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_infinite_preamble() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_modulation() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_xta_trim() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_xtb_trim() : driver_llcc68.c , driver_llcc68.h
- llcc68_single_receive() : driver_llcc68.c , driver_llcc68.h
- llcc68_timeout_convert_to_data() : driver_llcc68.c , driver_llcc68.h
- llcc68_timeout_convert_to_register() : driver_llcc68.c , driver_llcc68.h
- llcc68_write_buffer() : driver_llcc68.c , driver_llcc68.h
- llcc68_write_read_reg() : driver_llcc68.c , driver_llcc68.h
- llcc68_write_register() : driver_llcc68.c , driver_llcc68.h