| LibDriver LLCC68 1.0.0 LLCC68 full function driver

Macros
llcc68 link driver function
llcc68 driver function

llcc68 link driver modules More...

## Macros
#define | DRIVER_LLCC68_LINK_INIT(HANDLE, STRUCTURE) memset(HANDLE, 0, sizeof(STRUCTURE))
| initialize llcc68_handle_t structure More...
#define | DRIVER_LLCC68_LINK_SPI_INIT(HANDLE, FUC) (HANDLE)->spi_init = FUC
| link spi_init function More...
#define | DRIVER_LLCC68_LINK_SPI_DEINIT(HANDLE, FUC) (HANDLE)->spi_deinit = FUC
| link spi_deinit function More...
#define | DRIVER_LLCC68_LINK_SPI_WRITE_READ(HANDLE, FUC) (HANDLE)->spi_write_read = FUC
| link spi_write_read function More...
#define | DRIVER_LLCC68_LINK_RESET_GPIO_INIT(HANDLE, FUC) (HANDLE)->reset_gpio_init = FUC
| link reset_gpio_init function More...
#define | DRIVER_LLCC68_LINK_RESET_GPIO_DEINIT(HANDLE, FUC) (HANDLE)->reset_gpio_deinit = FUC
| link reset_gpio_deinit function More...
#define | DRIVER_LLCC68_LINK_RESET_GPIO_WRITE(HANDLE, FUC) (HANDLE)->reset_gpio_write = FUC
| link reset_gpio_write function More...
#define | DRIVER_LLCC68_LINK_BUSY_GPIO_INIT(HANDLE, FUC) (HANDLE)->busy_gpio_init = FUC
| link busy_gpio_init function More...
#define | DRIVER_LLCC68_LINK_BUSY_GPIO_DEINIT(HANDLE, FUC) (HANDLE)->busy_gpio_deinit = FUC
| link busy_gpio_deinit function More...
#define | DRIVER_LLCC68_LINK_BUSY_GPIO_READ(HANDLE, FUC) (HANDLE)->busy_gpio_read = FUC
| link busy_gpio_read function More...
#define | DRIVER_LLCC68_LINK_DELAY_MS(HANDLE, FUC) (HANDLE)->delay_ms = FUC
| link delay_ms function More...
#define | DRIVER_LLCC68_LINK_DEBUG_PRINT(HANDLE, FUC) (HANDLE)->debug_print = FUC
| link debug_print function More...
#define | DRIVER_LLCC68_LINK_RECEIVE_CALLBACK(HANDLE, FUC) (HANDLE)->receive_callback = FUC
| link receive_callback function More...

## Detailed Description

llcc68 link driver modules

## Macro Definition Documentation

## ◆ DRIVER_LLCC68_LINK_BUSY_GPIO_DEINIT

#define DRIVER_LLCC68_LINK_BUSY_GPIO_DEINIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->busy_gpio_deinit = FUC

link busy_gpio_deinit function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a busy_gpio_deinit function address

Note
  none

Definition at line 493 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_BUSY_GPIO_INIT

#define DRIVER_LLCC68_LINK_BUSY_GPIO_INIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->busy_gpio_init = FUC

link busy_gpio_init function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a busy_gpio_init function address

Note
  none

Definition at line 485 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_BUSY_GPIO_READ

#define DRIVER_LLCC68_LINK_BUSY_GPIO_READ | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->busy_gpio_read = FUC

link busy_gpio_read function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a busy_gpio_read function address

Note
  none

Definition at line 501 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_DEBUG_PRINT

#define DRIVER_LLCC68_LINK_DEBUG_PRINT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->debug_print = FUC

link debug_print function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a debug_print function address

Note
  none

Definition at line 517 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_DELAY_MS

#define DRIVER_LLCC68_LINK_DELAY_MS | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->delay_ms = FUC

link delay_ms function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a delay_ms function address

Note
  none

Definition at line 509 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_INIT

#define DRIVER_LLCC68_LINK_INIT | ( |  | HANDLE,
|  |  | STRUCTURE
| ) |  | memset(HANDLE, 0, sizeof(STRUCTURE))

initialize llcc68_handle_t structure

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | STRUCTURE | llcc68_handle_t

Note
  none

Definition at line 429 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_RECEIVE_CALLBACK

#define DRIVER_LLCC68_LINK_RECEIVE_CALLBACK | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->receive_callback = FUC

link receive_callback function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a receive_callback function address

Note
  none

Definition at line 525 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_RESET_GPIO_DEINIT

#define DRIVER_LLCC68_LINK_RESET_GPIO_DEINIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->reset_gpio_deinit = FUC

link reset_gpio_deinit function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a reset_gpio_deinit function address

Note
  none

Definition at line 469 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_RESET_GPIO_INIT

#define DRIVER_LLCC68_LINK_RESET_GPIO_INIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->reset_gpio_init = FUC

link reset_gpio_init function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a reset_gpio_init function address

Note
  none

Definition at line 461 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_RESET_GPIO_WRITE

#define DRIVER_LLCC68_LINK_RESET_GPIO_WRITE | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->reset_gpio_write = FUC

link reset_gpio_write function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a reset_gpio_write function address

Note
  none

Definition at line 477 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_SPI_DEINIT

#define DRIVER_LLCC68_LINK_SPI_DEINIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_deinit = FUC

link spi_deinit function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a spi_deinit function address

Note
  none

Definition at line 445 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_SPI_INIT

#define DRIVER_LLCC68_LINK_SPI_INIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_init = FUC

link spi_init function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a spi_init function address

Note
  none

Definition at line 437 of file driver_llcc68.h.

## ◆ DRIVER_LLCC68_LINK_SPI_WRITE_READ

#define DRIVER_LLCC68_LINK_SPI_WRITE_READ | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_write_read = FUC

link spi_write_read function

Parameters

  [in] | HANDLE | pointer to an llcc68 handle structure
  [in] | FUC | pointer to a spi_write_read function address

Note
  none

Definition at line 453 of file driver_llcc68.h.