| LibDriver LLCC68 1.0.0 LLCC68 full function driver

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - l -

- LLCC68_BOOL_FALSE : driver_llcc68.h
- llcc68_bool_t : driver_llcc68.h
- LLCC68_BOOL_TRUE : driver_llcc68.h
- llcc68_cad_test() : driver_llcc68_cad_test.c , driver_llcc68_cad_test.h
- llcc68_cad_test_irq_handler() : driver_llcc68_cad_test.c , driver_llcc68_cad_test.h
- LLCC68_CALIBRATION_ADC_BULK_N : driver_llcc68.h
- LLCC68_CALIBRATION_ADC_BULK_P : driver_llcc68.h
- LLCC68_CALIBRATION_ADC_PULSE : driver_llcc68.h
- LLCC68_CALIBRATION_IMAGE : driver_llcc68.h
- LLCC68_CALIBRATION_PLL : driver_llcc68.h
- LLCC68_CALIBRATION_RC13M : driver_llcc68.h
- LLCC68_CALIBRATION_RC64K : driver_llcc68.h
- llcc68_calibration_t : driver_llcc68.h
- llcc68_check_packet_error() : driver_llcc68.c , driver_llcc68.h
- llcc68_clear_device_errors() : driver_llcc68.c , driver_llcc68.h
- llcc68_clear_irq_status() : driver_llcc68.c , driver_llcc68.h
- LLCC68_CLOCK_SOURCE_RC_13M : driver_llcc68.h
- llcc68_clock_source_t : driver_llcc68.h
- LLCC68_CLOCK_SOURCE_XTAL_32MHZ : driver_llcc68.h
- LLCC68_COMMAND_CLEAR_DEVICE_ERRORS : driver_llcc68.c
- LLCC68_COMMAND_CLEAR_IRQ_STATUS : driver_llcc68.c
- LLCC68_COMMAND_GET_DEVICE_ERRORS : driver_llcc68.c
- LLCC68_COMMAND_GET_IRQ_STATUS : driver_llcc68.c
- LLCC68_COMMAND_GET_PACKET_STATUS : driver_llcc68.c
- LLCC68_COMMAND_GET_PACKET_TYPE : driver_llcc68.c
- LLCC68_COMMAND_GET_RSSI_LNST : driver_llcc68.c
- LLCC68_COMMAND_GET_RX_BUFFER_STATUS : driver_llcc68.c
- LLCC68_COMMAND_GET_STATS : driver_llcc68.c
- LLCC68_COMMAND_GET_STATUS : driver_llcc68.c
- LLCC68_COMMAND_READ_BUFFER : driver_llcc68.c
- LLCC68_COMMAND_READ_REGISTER : driver_llcc68.c
- LLCC68_COMMAND_RESET_STATS : driver_llcc68.c
- LLCC68_COMMAND_SET_BUFFER_BASE_ADDRESS : driver_llcc68.c
- LLCC68_COMMAND_SET_CAD : driver_llcc68.c
- LLCC68_COMMAND_SET_CAD_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_SET_CALIBRATE : driver_llcc68.c
- LLCC68_COMMAND_SET_CALIBRATE_IMAGE : driver_llcc68.c
- LLCC68_COMMAND_SET_DIO2_AS_RF_SWITCH_CTRL : driver_llcc68.c
- LLCC68_COMMAND_SET_DIO3_AS_TCXO_CTRL : driver_llcc68.c
- LLCC68_COMMAND_SET_DIO_IRQ_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_SET_FS : driver_llcc68.c
- LLCC68_COMMAND_SET_LORA_SYMB_NUM_TIMEOUT : driver_llcc68.c
- LLCC68_COMMAND_SET_MODULATION_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_SET_PA_CONFIG : driver_llcc68.c
- LLCC68_COMMAND_SET_PACKET_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_SET_PACKET_TYPE : driver_llcc68.c
- LLCC68_COMMAND_SET_REGULATOR_MODE : driver_llcc68.c
- LLCC68_COMMAND_SET_RF_FREQUENCY : driver_llcc68.c
- LLCC68_COMMAND_SET_RX : driver_llcc68.c
- LLCC68_COMMAND_SET_RX_DUTY_CYCLE : driver_llcc68.c
- LLCC68_COMMAND_SET_RX_TX_FALLBACK_MODE : driver_llcc68.c
- LLCC68_COMMAND_SET_SLEEP : driver_llcc68.c
- LLCC68_COMMAND_SET_STANDBY : driver_llcc68.c
- LLCC68_COMMAND_SET_TX : driver_llcc68.c
- LLCC68_COMMAND_SET_TX_CONTINUOUS_WAVE : driver_llcc68.c
- LLCC68_COMMAND_SET_TX_INFINITE_PREAMBLE : driver_llcc68.c
- LLCC68_COMMAND_SET_TX_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_STOP_TIMER_ON_PREAMBLE : driver_llcc68.c
- LLCC68_COMMAND_WRITE_BUFFER : driver_llcc68.c
- LLCC68_COMMAND_WRITE_REGISTER : driver_llcc68.c
- llcc68_continuous_receive() : driver_llcc68.c , driver_llcc68.h
- llcc68_deinit() : driver_llcc68.c , driver_llcc68.h
- llcc68_frequency_convert_to_data() : driver_llcc68.c , driver_llcc68.h
- llcc68_frequency_convert_to_register() : driver_llcc68.c , driver_llcc68.h
- LLCC68_FSK_RX_STATUS_ABORT_ERR : driver_llcc68.h
- LLCC68_FSK_RX_STATUS_ADDR_ERR : driver_llcc68.h
- LLCC68_FSK_RX_STATUS_CRC_ERR : driver_llcc68.h
- LLCC68_FSK_RX_STATUS_LENGTH_ERR : driver_llcc68.h
- LLCC68_FSK_RX_STATUS_PKT_RECEIVED : driver_llcc68.h
- LLCC68_FSK_RX_STATUS_PKT_SEND : driver_llcc68.h
- LLCC68_FSK_RX_STATUS_PREAMBLE_ERR : driver_llcc68.h
- LLCC68_FSK_RX_STATUS_SYNC_ERR : driver_llcc68.h
- llcc68_fsk_rx_status_t : driver_llcc68.h
- llcc68_get_device_errors() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_dio3_output_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_dio_input_enable() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_dio_output_enable() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_event_mask() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_broadcast_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_crc_initical_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_crc_polynomial_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_node_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_sync_word() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_fsk_whitening_initial_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_gfsk_packet_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_instantaneous_rssi() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_iq_polarity() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_irq_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_lora_packet_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_lora_sync_word() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_ocp() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_packet_type() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_pull_down_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_pull_up_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_random_number() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_rtc_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_rx_buffer_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_rx_gain() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_stats() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_status() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_tx_clamp_config() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_tx_modulation() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_xta_trim() : driver_llcc68.c , driver_llcc68.h
- llcc68_get_xtb_trim() : driver_llcc68.c , driver_llcc68.h
- LLCC68_GFSK_ADDR_FILTER_ACTIVATED_NODE_ADDR : driver_llcc68.h
- LLCC68_GFSK_ADDR_FILTER_ACTIVATED_NODE_BROADCAST_ADDR : driver_llcc68.h
- LLCC68_GFSK_ADDR_FILTER_DISABLE : driver_llcc68.h
- llcc68_gfsk_addr_filter_t : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_117P3_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_11P7_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_14P6_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_156P2_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_187P2_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_19P5_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_232P3_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_23P4_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_29P3_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_312_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_373P6_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_39_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_467_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_46P9_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_4P8_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_58P6_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_5P8_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_78P2_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_7P3_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_93P8_KHZ : driver_llcc68.h
- LLCC68_GFSK_BANDWIDTH_9P7_KHZ : driver_llcc68.h
- llcc68_gfsk_bandwidth_t : driver_llcc68.h
- llcc68_gfsk_bit_rate_convert_to_data() : driver_llcc68.c , driver_llcc68.h
- llcc68_gfsk_bit_rate_convert_to_register() : driver_llcc68.c , driver_llcc68.h
- LLCC68_GFSK_CRC_TYPE_1_BYTE : driver_llcc68.h
- LLCC68_GFSK_CRC_TYPE_1_BYTE_INV : driver_llcc68.h
- LLCC68_GFSK_CRC_TYPE_2_BYTE : driver_llcc68.h
- LLCC68_GFSK_CRC_TYPE_2_BYTE_INV : driver_llcc68.h
- LLCC68_GFSK_CRC_TYPE_OFF : driver_llcc68.h
- llcc68_gfsk_crc_type_t : driver_llcc68.h
- llcc68_gfsk_frequency_deviation_convert_to_data() : driver_llcc68.c , driver_llcc68.h
- llcc68_gfsk_frequency_deviation_convert_to_register() : driver_llcc68.c , driver_llcc68.h
- LLCC68_GFSK_PACKET_TYPE_KNOWN_LENGTH : driver_llcc68.h
- llcc68_gfsk_packet_type_t : driver_llcc68.h
- LLCC68_GFSK_PACKET_TYPE_VARIABLE_SIZE : driver_llcc68.h
- LLCC68_GFSK_PREAMBLE_DETECTOR_LENGTH_16_BITS : driver_llcc68.h
- LLCC68_GFSK_PREAMBLE_DETECTOR_LENGTH_24_BITS : driver_llcc68.h
- LLCC68_GFSK_PREAMBLE_DETECTOR_LENGTH_32_BITS : driver_llcc68.h
- LLCC68_GFSK_PREAMBLE_DETECTOR_LENGTH_8_BITS : driver_llcc68.h
- LLCC68_GFSK_PREAMBLE_DETECTOR_LENGTH_OFF : driver_llcc68.h
- llcc68_gfsk_preamble_detector_length_t : driver_llcc68.h
- LLCC68_GFSK_PULSE_SHAPE_GAUSSIAN_BT_0P3 : driver_llcc68.h
- LLCC68_GFSK_PULSE_SHAPE_GAUSSIAN_BT_0P5 : driver_llcc68.h
- LLCC68_GFSK_PULSE_SHAPE_GAUSSIAN_BT_0P7 : driver_llcc68.h
- LLCC68_GFSK_PULSE_SHAPE_GAUSSIAN_BT_1 : driver_llcc68.h
- LLCC68_GFSK_PULSE_SHAPE_NO_FILTER : driver_llcc68.h
- llcc68_gfsk_pulse_shape_t : driver_llcc68.h
- llcc68_handle_t : driver_llcc68.h
- llcc68_info() : driver_llcc68.c , driver_llcc68.h
- llcc68_info_t : driver_llcc68.h
- llcc68_init() : driver_llcc68.c , driver_llcc68.h
- llcc68_interface_busy_gpio_deinit() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_busy_gpio_init() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_busy_gpio_read() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_debug_print() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_delay_ms() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_receive_callback() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_reset_gpio_deinit() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_reset_gpio_init() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_reset_gpio_write() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_spi_deinit() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_spi_init() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interface_spi_write_read() : driver_llcc68_interface.h , driver_llcc68_interface_template.c
- llcc68_interrupt_test_irq_handler() : driver_llcc68_send_receive_test.c , driver_llcc68_send_receive_test.h
- LLCC68_IRQ_CAD_DETECTED : driver_llcc68.h
- LLCC68_IRQ_CAD_DONE : driver_llcc68.h
- LLCC68_IRQ_CRC_ERR : driver_llcc68.h
- llcc68_irq_handler() : driver_llcc68.c , driver_llcc68.h
- LLCC68_IRQ_HEADER_ERR : driver_llcc68.h
- LLCC68_IRQ_HEADER_VALID : driver_llcc68.h
- LLCC68_IRQ_PREAMBLE_DETECTED : driver_llcc68.h
- LLCC68_IRQ_RX_DONE : driver_llcc68.h
- LLCC68_IRQ_SYNC_WORD_VALID : driver_llcc68.h
- llcc68_irq_t : driver_llcc68.h
- LLCC68_IRQ_TIMEOUT : driver_llcc68.h
- LLCC68_IRQ_TX_DONE : driver_llcc68.h
- LLCC68_LORA_BANDWIDTH_125_KHZ : driver_llcc68.h
- LLCC68_LORA_BANDWIDTH_250_KHZ : driver_llcc68.h
- LLCC68_LORA_BANDWIDTH_500_KHZ : driver_llcc68.h
- llcc68_lora_bandwidth_t : driver_llcc68.h
- llcc68_lora_cad() : driver_llcc68.c , driver_llcc68.h
- LLCC68_LORA_CAD_EXIT_MODE_ONLY : driver_llcc68.h
- LLCC68_LORA_CAD_EXIT_MODE_RX : driver_llcc68.h
- llcc68_lora_cad_exit_mode_t : driver_llcc68.h
- LLCC68_LORA_CAD_SYMBOL_NUM_1 : driver_llcc68.h
- LLCC68_LORA_CAD_SYMBOL_NUM_16 : driver_llcc68.h
- LLCC68_LORA_CAD_SYMBOL_NUM_2 : driver_llcc68.h
- LLCC68_LORA_CAD_SYMBOL_NUM_4 : driver_llcc68.h
- LLCC68_LORA_CAD_SYMBOL_NUM_8 : driver_llcc68.h
- llcc68_lora_cad_symbol_num_t : driver_llcc68.h
- llcc68_lora_check_packet_error() : driver_llcc68_lora.c , driver_llcc68_lora.h
- LLCC68_LORA_CR_4_5 : driver_llcc68.h
- LLCC68_LORA_CR_4_6 : driver_llcc68.h
- LLCC68_LORA_CR_4_7 : driver_llcc68.h
- LLCC68_LORA_CR_4_8 : driver_llcc68.h
- llcc68_lora_cr_t : driver_llcc68.h
- LLCC68_LORA_CRC_TYPE_OFF : driver_llcc68.h
- LLCC68_LORA_CRC_TYPE_ON : driver_llcc68.h
- llcc68_lora_crc_type_t : driver_llcc68.h
- LLCC68_LORA_DEFAULT_BANDWIDTH : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_BUFFER_SIZE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CAD_DET_MIN : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CAD_DET_PEAK : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CAD_SYMBOL_NUM : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CR : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CRC_TYPE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_HEADER : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_INVERT_IQ : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_LOW_DATA_RATE_OPTIMIZE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_OCP : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_PA_CONFIG_DUTY_CYCLE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_PA_CONFIG_HP_MAX : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_PREAMBLE_LENGTH : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_RAMP_TIME : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_REGULATOR_MODE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_RF_FREQUENCY : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_RTC_WAKE_UP : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_RX_GAIN : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_SF : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_START_MODE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_STOP_TIMER_ON_PREAMBLE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_SYMB_NUM_TIMEOUT : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_SYNC_WORD : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_TX_DBM : driver_llcc68_lora.h
- llcc68_lora_deinit() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_get_status() : driver_llcc68_lora.c , driver_llcc68_lora.h
- LLCC68_LORA_HEADER_EXPLICIT : driver_llcc68.h
- LLCC68_LORA_HEADER_IMPLICIT : driver_llcc68.h
- llcc68_lora_header_t : driver_llcc68.h
- llcc68_lora_init() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_irq_handler() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_run_cad() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_send() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_set_continuous_receive_mode() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_set_send_mode() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_set_shot_receive_mode() : driver_llcc68_lora.c , driver_llcc68_lora.h
- LLCC68_LORA_SF_10 : driver_llcc68.h
- LLCC68_LORA_SF_11 : driver_llcc68.h
- LLCC68_LORA_SF_5 : driver_llcc68.h
- LLCC68_LORA_SF_6 : driver_llcc68.h
- LLCC68_LORA_SF_7 : driver_llcc68.h
- LLCC68_LORA_SF_8 : driver_llcc68.h
- LLCC68_LORA_SF_9 : driver_llcc68.h
- llcc68_lora_sf_t : driver_llcc68.h
- llcc68_lora_sleep() : driver_llcc68_lora.c , driver_llcc68_lora.h
- llcc68_lora_transmit() : driver_llcc68.c , driver_llcc68.h
- llcc68_lora_wake_up() : driver_llcc68_lora.c , driver_llcc68_lora.h
- LLCC68_OP_ERROR_ADC_CALIB_ERR : driver_llcc68.h
- LLCC68_OP_ERROR_IMG_CALIB_ERR : driver_llcc68.h
- LLCC68_OP_ERROR_PA_RAMP_ERR : driver_llcc68.h
- LLCC68_OP_ERROR_PLL_CALIB_ERR : driver_llcc68.h
- LLCC68_OP_ERROR_PLL_LOCK_ERR : driver_llcc68.h
- LLCC68_OP_ERROR_RC13M_CALIB_ERR : driver_llcc68.h
- LLCC68_OP_ERROR_RC64K_CALIB_ERR : driver_llcc68.h
- llcc68_op_error_t : driver_llcc68.h
- LLCC68_OP_ERROR_XOSC_START_ERR : driver_llcc68.h
- LLCC68_PACKET_TYPE_GFSK : driver_llcc68.h
- LLCC68_PACKET_TYPE_LORA : driver_llcc68.h
- llcc68_packet_type_t : driver_llcc68.h
- LLCC68_RAMP_TIME_10US : driver_llcc68.h
- LLCC68_RAMP_TIME_1700US : driver_llcc68.h
- LLCC68_RAMP_TIME_200US : driver_llcc68.h
- LLCC68_RAMP_TIME_20US : driver_llcc68.h
- LLCC68_RAMP_TIME_3400US : driver_llcc68.h
- LLCC68_RAMP_TIME_40US : driver_llcc68.h
- LLCC68_RAMP_TIME_800US : driver_llcc68.h
- LLCC68_RAMP_TIME_80US : driver_llcc68.h
- llcc68_ramp_time_t : driver_llcc68.h
- llcc68_read_buffer() : driver_llcc68.c , driver_llcc68.h
- llcc68_read_register() : driver_llcc68.c , driver_llcc68.h
- llcc68_receive_test() : driver_llcc68_send_receive_test.c , driver_llcc68_send_receive_test.h
- LLCC68_REG_BROADCAST_ADDRESS : driver_llcc68.c
- LLCC68_REG_CRC_INIT_VALUE_LSB : driver_llcc68.c
- LLCC68_REG_CRC_INIT_VALUE_MSB : driver_llcc68.c
- LLCC68_REG_CRC_POLYNOMIAL_VALUE_LSB : driver_llcc68.c
- LLCC68_REG_CRC_POLYNOMIAL_VALUE_MSB : driver_llcc68.c
- LLCC68_REG_DIO3_OUTPUT_CONTROL : driver_llcc68.c
- LLCC68_REG_DIOX_INPUT_ENABLE : driver_llcc68.c
- LLCC68_REG_DIOX_OUTPUT_ENABLE : driver_llcc68.c
- LLCC68_REG_DIOX_PULL_DOWN_CONTROL : driver_llcc68.c
- LLCC68_REG_DIOX_PULL_UP_CONTROL : driver_llcc68.c
- LLCC68_REG_EVENT_MASK : driver_llcc68.c
- LLCC68_REG_IQ_POLARITY_SETUP : driver_llcc68.c
- LLCC68_REG_LORA_SYNC_WORD_LSB : driver_llcc68.c
- LLCC68_REG_LORA_SYNC_WORD_MSB : driver_llcc68.c
- LLCC68_REG_NODE_ADDRESS : driver_llcc68.c
- LLCC68_REG_OCP_CONFIGURATION : driver_llcc68.c
- LLCC68_REG_RANDOM_NUMBER_GEN_0 : driver_llcc68.c
- LLCC68_REG_RANDOM_NUMBER_GEN_1 : driver_llcc68.c
- LLCC68_REG_RANDOM_NUMBER_GEN_2 : driver_llcc68.c
- LLCC68_REG_RANDOM_NUMBER_GEN_3 : driver_llcc68.c
- LLCC68_REG_RTC_CONTROL : driver_llcc68.c
- LLCC68_REG_RX_GAIN : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_0 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_1 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_2 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_3 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_4 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_5 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_6 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_7 : driver_llcc68.c
- LLCC68_REG_TX_CLAMP_CONFIG : driver_llcc68.c
- LLCC68_REG_TX_MODULATION : driver_llcc68.c
- LLCC68_REG_WHITENING_INIT_VALUE_LSB : driver_llcc68.c
- LLCC68_REG_WHITENING_INIT_VALUE_MSB : driver_llcc68.c
- LLCC68_REG_XTA_TRIM : driver_llcc68.c
- LLCC68_REG_XTB_TRIM : driver_llcc68.c
- llcc68_register_test() : driver_llcc68_register_test.c , driver_llcc68_register_test.h
- LLCC68_REGULATOR_MODE_DC_DC_LDO : driver_llcc68.h
- LLCC68_REGULATOR_MODE_ONLY_LDO : driver_llcc68.h
- llcc68_regulator_mode_t : driver_llcc68.h
- llcc68_reset_stats() : driver_llcc68.c , driver_llcc68.h
- LLCC68_RX_TX_FALLBACK_MODE_FS : driver_llcc68.h
- LLCC68_RX_TX_FALLBACK_MODE_STDBY_RC : driver_llcc68.h
- LLCC68_RX_TX_FALLBACK_MODE_STDBY_XOSC : driver_llcc68.h
- llcc68_rx_tx_fallback_mode_t : driver_llcc68.h
- llcc68_send_test() : driver_llcc68_send_receive_test.c , driver_llcc68_send_receive_test.h
- llcc68_set_buffer_base_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_cad() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_cad_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_calibration() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_calibration_image() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio2_as_rf_switch_ctrl() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio3_as_tcxo_ctrl() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio3_output_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio_input_enable() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio_irq_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_dio_output_enable() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_event_mask() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_frequency_synthesis() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_broadcast_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_crc_initical_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_crc_polynomial_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_node_address() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_sync_word() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_fsk_whitening_initial_value() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_gfsk_modulation_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_gfsk_packet_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_iq_polarity() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_lora_modulation_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_lora_packet_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_lora_symb_num_timeout() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_lora_sync_word() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_ocp() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_pa_config() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_packet_type() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_pull_down_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_pull_up_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_regulator_mode() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rf_frequency() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rtc_control() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rx() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rx_duty_cycle() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rx_gain() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_rx_tx_fallback_mode() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_sleep() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_standby() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_stop_timer_on_preamble() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_clamp_config() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_continuous_wave() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_infinite_preamble() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_modulation() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_tx_params() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_xta_trim() : driver_llcc68.c , driver_llcc68.h
- llcc68_set_xtb_trim() : driver_llcc68.c , driver_llcc68.h
- llcc68_single_receive() : driver_llcc68.c , driver_llcc68.h
- LLCC68_START_MODE_COLD : driver_llcc68.h
- llcc68_start_mode_t : driver_llcc68.h
- LLCC68_START_MODE_WARM : driver_llcc68.h
- LLCC68_TCXO_VOLTAGE_1P6V : driver_llcc68.h
- LLCC68_TCXO_VOLTAGE_1P7V : driver_llcc68.h
- LLCC68_TCXO_VOLTAGE_1P8V : driver_llcc68.h
- LLCC68_TCXO_VOLTAGE_2P2V : driver_llcc68.h
- LLCC68_TCXO_VOLTAGE_2P4V : driver_llcc68.h
- LLCC68_TCXO_VOLTAGE_2P7V : driver_llcc68.h
- LLCC68_TCXO_VOLTAGE_3P0V : driver_llcc68.h
- LLCC68_TCXO_VOLTAGE_3P3V : driver_llcc68.h
- llcc68_tcxo_voltage_t : driver_llcc68.h
- llcc68_timeout_convert_to_data() : driver_llcc68.c , driver_llcc68.h
- llcc68_timeout_convert_to_register() : driver_llcc68.c , driver_llcc68.h
- llcc68_write_buffer() : driver_llcc68.c , driver_llcc68.h
- llcc68_write_read_reg() : driver_llcc68.c , driver_llcc68.h
- llcc68_write_register() : driver_llcc68.c , driver_llcc68.h