| LibDriver LLCC68 1.0.0 LLCC68 full function driver

### - c -

- CHIP_NAME : driver_llcc68.c

### - d -

- DRIVER_LLCC68_LINK_BUSY_GPIO_DEINIT : driver_llcc68.h
- DRIVER_LLCC68_LINK_BUSY_GPIO_INIT : driver_llcc68.h
- DRIVER_LLCC68_LINK_BUSY_GPIO_READ : driver_llcc68.h
- DRIVER_LLCC68_LINK_DEBUG_PRINT : driver_llcc68.h
- DRIVER_LLCC68_LINK_DELAY_MS : driver_llcc68.h
- DRIVER_LLCC68_LINK_INIT : driver_llcc68.h
- DRIVER_LLCC68_LINK_RECEIVE_CALLBACK : driver_llcc68.h
- DRIVER_LLCC68_LINK_RESET_GPIO_DEINIT : driver_llcc68.h
- DRIVER_LLCC68_LINK_RESET_GPIO_INIT : driver_llcc68.h
- DRIVER_LLCC68_LINK_RESET_GPIO_WRITE : driver_llcc68.h
- DRIVER_LLCC68_LINK_SPI_DEINIT : driver_llcc68.h
- DRIVER_LLCC68_LINK_SPI_INIT : driver_llcc68.h
- DRIVER_LLCC68_LINK_SPI_WRITE_READ : driver_llcc68.h
- DRIVER_VERSION : driver_llcc68.c

### - l -

- LLCC68_COMMAND_CLEAR_DEVICE_ERRORS : driver_llcc68.c
- LLCC68_COMMAND_CLEAR_IRQ_STATUS : driver_llcc68.c
- LLCC68_COMMAND_GET_DEVICE_ERRORS : driver_llcc68.c
- LLCC68_COMMAND_GET_IRQ_STATUS : driver_llcc68.c
- LLCC68_COMMAND_GET_PACKET_STATUS : driver_llcc68.c
- LLCC68_COMMAND_GET_PACKET_TYPE : driver_llcc68.c
- LLCC68_COMMAND_GET_RSSI_LNST : driver_llcc68.c
- LLCC68_COMMAND_GET_RX_BUFFER_STATUS : driver_llcc68.c
- LLCC68_COMMAND_GET_STATS : driver_llcc68.c
- LLCC68_COMMAND_GET_STATUS : driver_llcc68.c
- LLCC68_COMMAND_READ_BUFFER : driver_llcc68.c
- LLCC68_COMMAND_READ_REGISTER : driver_llcc68.c
- LLCC68_COMMAND_RESET_STATS : driver_llcc68.c
- LLCC68_COMMAND_SET_BUFFER_BASE_ADDRESS : driver_llcc68.c
- LLCC68_COMMAND_SET_CAD : driver_llcc68.c
- LLCC68_COMMAND_SET_CAD_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_SET_CALIBRATE : driver_llcc68.c
- LLCC68_COMMAND_SET_CALIBRATE_IMAGE : driver_llcc68.c
- LLCC68_COMMAND_SET_DIO2_AS_RF_SWITCH_CTRL : driver_llcc68.c
- LLCC68_COMMAND_SET_DIO3_AS_TCXO_CTRL : driver_llcc68.c
- LLCC68_COMMAND_SET_DIO_IRQ_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_SET_FS : driver_llcc68.c
- LLCC68_COMMAND_SET_LORA_SYMB_NUM_TIMEOUT : driver_llcc68.c
- LLCC68_COMMAND_SET_MODULATION_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_SET_PA_CONFIG : driver_llcc68.c
- LLCC68_COMMAND_SET_PACKET_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_SET_PACKET_TYPE : driver_llcc68.c
- LLCC68_COMMAND_SET_REGULATOR_MODE : driver_llcc68.c
- LLCC68_COMMAND_SET_RF_FREQUENCY : driver_llcc68.c
- LLCC68_COMMAND_SET_RX : driver_llcc68.c
- LLCC68_COMMAND_SET_RX_DUTY_CYCLE : driver_llcc68.c
- LLCC68_COMMAND_SET_RX_TX_FALLBACK_MODE : driver_llcc68.c
- LLCC68_COMMAND_SET_SLEEP : driver_llcc68.c
- LLCC68_COMMAND_SET_STANDBY : driver_llcc68.c
- LLCC68_COMMAND_SET_TX : driver_llcc68.c
- LLCC68_COMMAND_SET_TX_CONTINUOUS_WAVE : driver_llcc68.c
- LLCC68_COMMAND_SET_TX_INFINITE_PREAMBLE : driver_llcc68.c
- LLCC68_COMMAND_SET_TX_PARAMS : driver_llcc68.c
- LLCC68_COMMAND_STOP_TIMER_ON_PREAMBLE : driver_llcc68.c
- LLCC68_COMMAND_WRITE_BUFFER : driver_llcc68.c
- LLCC68_COMMAND_WRITE_REGISTER : driver_llcc68.c
- LLCC68_LORA_DEFAULT_BANDWIDTH : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_BUFFER_SIZE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CAD_DET_MIN : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CAD_DET_PEAK : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CAD_SYMBOL_NUM : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CR : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_CRC_TYPE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_HEADER : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_INVERT_IQ : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_LOW_DATA_RATE_OPTIMIZE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_OCP : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_PA_CONFIG_DUTY_CYCLE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_PA_CONFIG_HP_MAX : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_PREAMBLE_LENGTH : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_RAMP_TIME : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_REGULATOR_MODE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_RF_FREQUENCY : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_RTC_WAKE_UP : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_RX_GAIN : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_SF : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_START_MODE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_STOP_TIMER_ON_PREAMBLE : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_SYMB_NUM_TIMEOUT : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_SYNC_WORD : driver_llcc68_lora.h
- LLCC68_LORA_DEFAULT_TX_DBM : driver_llcc68_lora.h
- LLCC68_REG_BROADCAST_ADDRESS : driver_llcc68.c
- LLCC68_REG_CRC_INIT_VALUE_LSB : driver_llcc68.c
- LLCC68_REG_CRC_INIT_VALUE_MSB : driver_llcc68.c
- LLCC68_REG_CRC_POLYNOMIAL_VALUE_LSB : driver_llcc68.c
- LLCC68_REG_CRC_POLYNOMIAL_VALUE_MSB : driver_llcc68.c
- LLCC68_REG_DIO3_OUTPUT_CONTROL : driver_llcc68.c
- LLCC68_REG_DIOX_INPUT_ENABLE : driver_llcc68.c
- LLCC68_REG_DIOX_OUTPUT_ENABLE : driver_llcc68.c
- LLCC68_REG_DIOX_PULL_DOWN_CONTROL : driver_llcc68.c
- LLCC68_REG_DIOX_PULL_UP_CONTROL : driver_llcc68.c
- LLCC68_REG_EVENT_MASK : driver_llcc68.c
- LLCC68_REG_IQ_POLARITY_SETUP : driver_llcc68.c
- LLCC68_REG_LORA_SYNC_WORD_LSB : driver_llcc68.c
- LLCC68_REG_LORA_SYNC_WORD_MSB : driver_llcc68.c
- LLCC68_REG_NODE_ADDRESS : driver_llcc68.c
- LLCC68_REG_OCP_CONFIGURATION : driver_llcc68.c
- LLCC68_REG_RANDOM_NUMBER_GEN_0 : driver_llcc68.c
- LLCC68_REG_RANDOM_NUMBER_GEN_1 : driver_llcc68.c
- LLCC68_REG_RANDOM_NUMBER_GEN_2 : driver_llcc68.c
- LLCC68_REG_RANDOM_NUMBER_GEN_3 : driver_llcc68.c
- LLCC68_REG_RTC_CONTROL : driver_llcc68.c
- LLCC68_REG_RX_GAIN : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_0 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_1 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_2 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_3 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_4 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_5 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_6 : driver_llcc68.c
- LLCC68_REG_SYNC_WORD_7 : driver_llcc68.c
- LLCC68_REG_TX_CLAMP_CONFIG : driver_llcc68.c
- LLCC68_REG_TX_MODULATION : driver_llcc68.c
- LLCC68_REG_WHITENING_INIT_VALUE_LSB : driver_llcc68.c
- LLCC68_REG_WHITENING_INIT_VALUE_MSB : driver_llcc68.c
- LLCC68_REG_XTA_TRIM : driver_llcc68.c
- LLCC68_REG_XTB_TRIM : driver_llcc68.c

### - m -

- MANUFACTURER_NAME : driver_llcc68.c
- MAX_CURRENT : driver_llcc68.c

### - s -

- SUPPLY_VOLTAGE_MAX : driver_llcc68.c
- SUPPLY_VOLTAGE_MIN : driver_llcc68.c

### - t -

- TEMPERATURE_MAX : driver_llcc68.c
- TEMPERATURE_MIN : driver_llcc68.c