| LibDriver NRF24L01 1.0.0 NRF24L01 full function driver

### - c -

- CHIP_NAME : driver_nrf24l01.c

### - d -

- DRIVER_NRF24L01_LINK_DEBUG_PRINT : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_DELAY_MS : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_GPIO_DEINIT : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_GPIO_INIT : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_GPIO_WRITE : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_INIT : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_RECEIVE_CALLBACK : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_SPI_DEINIT : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_SPI_INIT : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_SPI_READ : driver_nrf24l01.h
- DRIVER_NRF24L01_LINK_SPI_WRITE : driver_nrf24l01.h
- DRIVER_VERSION : driver_nrf24l01.c

### - m -

- MANUFACTURER_NAME : driver_nrf24l01.c
- MAX_CURRENT : driver_nrf24l01.c

### - n -

- NRF24L01_BASIC_DEFAULT_ADDRESS_WIDTH : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_CHANNEL_FREQUENCY : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_CRCO : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_DATA_RATE : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_DYNAMIC_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_ENABLE_CRC : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_OUTPUT_POWER : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PAYLOAD_WITH_ACK : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_0_AUTO_ACKNOWLEDGMENT : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_0_DYNAMIC_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_0_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_1_AUTO_ACKNOWLEDGMENT : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_1_DYNAMIC_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_1_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_2_AUTO_ACKNOWLEDGMENT : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_2_DYNAMIC_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_2_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_3_AUTO_ACKNOWLEDGMENT : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_3_DYNAMIC_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_3_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_4_AUTO_ACKNOWLEDGMENT : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_4_DYNAMIC_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_4_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_5_AUTO_ACKNOWLEDGMENT : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_5_DYNAMIC_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_PIPE_5_PAYLOAD : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RETRANSMIT_COUNT : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RETRANSMIT_DELAY : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_ADDR_0 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_ADDR_1 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_ADDR_2 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_ADDR_3 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_ADDR_4 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_ADDR_5 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_PIPE_0 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_PIPE_1 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_PIPE_2 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_PIPE_3 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_PIPE_4 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_RX_PIPE_5 : driver_nrf24l01_basic.h
- NRF24L01_BASIC_DEFAULT_TX_PAYLOAD_WITH_NO_ACK : driver_nrf24l01_basic.h
- NRF24L01_COMMAND_FLUSH_RX : driver_nrf24l01.c
- NRF24L01_COMMAND_FLUSH_TX : driver_nrf24l01.c
- NRF24L01_COMMAND_NOP : driver_nrf24l01.c
- NRF24L01_COMMAND_R_REGISTER : driver_nrf24l01.c
- NRF24L01_COMMAND_R_RX_PAYLOAD : driver_nrf24l01.c
- NRF24L01_COMMAND_R_RX_PL_WID : driver_nrf24l01.c
- NRF24L01_COMMAND_REUSE_TX_PL : driver_nrf24l01.c
- NRF24L01_COMMAND_W_ACK_PAYLOAD : driver_nrf24l01.c
- NRF24L01_COMMAND_W_REGISTER : driver_nrf24l01.c
- NRF24L01_COMMAND_W_TX_PAYLOAD : driver_nrf24l01.c
- NRF24L01_COMMAND_W_TX_PAYLOAD_NO_ACK : driver_nrf24l01.c
- NRF24L01_REG_CONFIG : driver_nrf24l01.c
- NRF24L01_REG_DYNPD : driver_nrf24l01.c
- NRF24L01_REG_EN_AA : driver_nrf24l01.c
- NRF24L01_REG_EN_RXADDR : driver_nrf24l01.c
- NRF24L01_REG_FEATURE : driver_nrf24l01.c
- NRF24L01_REG_FIFO_STATUS : driver_nrf24l01.c
- NRF24L01_REG_OBSERVE_TX : driver_nrf24l01.c
- NRF24L01_REG_RF_CH : driver_nrf24l01.c
- NRF24L01_REG_RF_SETUP : driver_nrf24l01.c
- NRF24L01_REG_RPD : driver_nrf24l01.c
- NRF24L01_REG_RX_ADDR_P0 : driver_nrf24l01.c
- NRF24L01_REG_RX_ADDR_P1 : driver_nrf24l01.c
- NRF24L01_REG_RX_ADDR_P2 : driver_nrf24l01.c
- NRF24L01_REG_RX_ADDR_P3 : driver_nrf24l01.c
- NRF24L01_REG_RX_ADDR_P4 : driver_nrf24l01.c
- NRF24L01_REG_RX_ADDR_P5 : driver_nrf24l01.c
- NRF24L01_REG_RX_PW_P0 : driver_nrf24l01.c
- NRF24L01_REG_RX_PW_P1 : driver_nrf24l01.c
- NRF24L01_REG_RX_PW_P2 : driver_nrf24l01.c
- NRF24L01_REG_RX_PW_P3 : driver_nrf24l01.c
- NRF24L01_REG_RX_PW_P4 : driver_nrf24l01.c
- NRF24L01_REG_RX_PW_P5 : driver_nrf24l01.c
- NRF24L01_REG_SETUP_AW : driver_nrf24l01.c
- NRF24L01_REG_SETUP_RETR : driver_nrf24l01.c
- NRF24L01_REG_STATUS : driver_nrf24l01.c
- NRF24L01_REG_TX_ADDR : driver_nrf24l01.c

### - s -

- SUPPLY_VOLTAGE_MAX : driver_nrf24l01.c
- SUPPLY_VOLTAGE_MIN : driver_nrf24l01.c

### - t -

- TEMPERATURE_MAX : driver_nrf24l01.c
- TEMPERATURE_MIN : driver_nrf24l01.c