| LibDriver NRF24L01 1.0.0 NRF24L01 full function driver

Data Fields
nrf24l01_info_s Struct Reference
nrf24l01 driver function » nrf24l01 basic driver function

nrf24l01 information structure definition More...

`#include <driver_nrf24l01.h>`

## Data Fields
char | chip_name [32]
char | manufacturer_name [32]
char | interface [8]
float | supply_voltage_min_v
float | supply_voltage_max_v
float | max_current_ma
float | temperature_min
float | temperature_max
uint32_t | driver_version

## Detailed Description

nrf24l01 information structure definition

Definition at line 180 of file driver_nrf24l01.h.

## Field Documentation

## ◆ chip_name

char chip_name[32]

chip name

Definition at line 182 of file driver_nrf24l01.h.

## ◆ driver_version

uint32_t driver_version

driver version

Definition at line 190 of file driver_nrf24l01.h.

## ◆ interface

char interface[8]

chip interface name

Definition at line 184 of file driver_nrf24l01.h.

## ◆ manufacturer_name

char manufacturer_name[32]

manufacturer name

Definition at line 183 of file driver_nrf24l01.h.

## ◆ max_current_ma

float max_current_ma

chip max current

Definition at line 187 of file driver_nrf24l01.h.

## ◆ supply_voltage_max_v

float supply_voltage_max_v

chip max supply voltage

Definition at line 186 of file driver_nrf24l01.h.

## ◆ supply_voltage_min_v

float supply_voltage_min_v

chip min supply voltage

Definition at line 185 of file driver_nrf24l01.h.

## ◆ temperature_max

float temperature_max

chip max operating temperature

Definition at line 189 of file driver_nrf24l01.h.

## ◆ temperature_min

float temperature_min

chip min operating temperature

Definition at line 188 of file driver_nrf24l01.h.

The documentation for this struct was generated from the following file:

- src/driver_nrf24l01.h