<h1 id="interactive_analysis">Interactive vocal tract model - analysis</h1>

<p><img class="screenshot" src="img/gama_tts_editor-interactive-analysis.png"
	alt="Screenshot of the interactive vocal tract model - analysis window"></p>

<p>This is a simple spectrum/signal viewer. External spectrum viewers can be connected through JACK.
</p>

<p>Operations:</p>
<ul>
<li>Change the view:<br>Select "Spectrum" to view the spectrum, and "Signal" to see the time domain waveform.</li>
<li>Start/stop the viewer:<br>Click on "Start" or "Stop".</li>
<li>Change the parameters of the spectrum:<br>Select the window size and window type.</li>
<li>Select the maximum frequency of the spectrum:<br>The graph will show from 0 Hz to the selected frequency.</li>
<li>Select the y-axis scale for the spectrum:<br>Select "Linear" or "Log".</li>
<li>Select the y log scale limits:<br>Select the minimum dB level.</li>
<li>Move the mouse over the graph and the coordinates will appear in the top-left corner.</li>
</ul>
