ECU NAME: UNKNOWN, ID: 0x0000. MSG COUNT: 36
	MSG NAME: KG_KL_AKT - Keyless Go terminal control active, OFFSET 0, LENGTH 1
	MSG NAME: KL_50_EIN - Terminal 50 is turned on, OFFSET 3, LENGTH 1
	MSG NAME: KL_15X_EIN - 15X terminal is turned on, OFFSET 4, LENGTH 1
	MSG NAME: KL_15_EIN - Terminal 15 is turned on, OFFSET 5, LENGTH 1
	MSG NAME: KL_15R_EIN - Terminal 15R is turned on, OFFSET 6, LENGTH 1
	MSG NAME: FZG_RECH - Message: "vehicle calculated Wait", OFFSET 8, LENGTH 1
	MSG NAME: DIAG_TGL - diagnosis toggle, OFFSET 9, LENGTH 1
	MSG NAME: APPL_AUS - Application ID's do not send just NM IDs, OFFSET 10, LENGTH 1
	MSG NAME: PNK_ALM_AUS - Panic alarm by key, OFFSET 11, LENGTH 1
	MSG NAME: PNK_ALM_EIN - Panic alarm by key, OFFSET 12, LENGTH 1
	MSG NAME: FERN_ALARM - Remote triggering MSS alarm, OFFSET 13, LENGTH 1
	MSG NAME: SCHLUE_NEU - Message: renew key, OFFSET 16, LENGTH 1
	MSG NAME: ZV_PASSIV - closing passive, OFFSET 17, LENGTH 1
	MSG NAME: HD_STOPP - Trunk lid stop, OFFSET 19, LENGTH 1
	MSG NAME: ZV_N_VER_MW_AKT - ZV not lock value SBC active during, OFFSET 20, LENGTH 1
	MSG NAME: SPEI_NR - Current memory block number, OFFSET 21, LENGTH 3
	MSG NAME: AUSS_SICH - perimeter security, OFFSET 24, LENGTH 1
	MSG NAME: AUSS_ENTSI - Außenentsicherung, OFFSET 25, LENGTH 1
	MSG NAME: BLI_SICH - secure ZV flasher feedback, OFFSET 26, LENGTH 1
	MSG NAME: BLI_ENTSI - ZV flasher feedback unlock, OFFSET 27, LENGTH 1
	MSG NAME: HFE_EZS - Heckdeckelfernentriegelung, OFFSET 32, LENGTH 1
	MSG NAME: HD_SICH - secure boot lid, OFFSET 33, LENGTH 1
	MSG NAME: HD_ENTSI - Unlock the boot lid, OFFSET 34, LENGTH 1
	MSG NAME: TD_VERRI - locking gas cap, OFFSET 35, LENGTH 1
	MSG NAME: TD_ENTRI - unlock fuel filler cap, OFFSET 36, LENGTH 1
	MSG NAME: RWTFE_EZS - Far open rear door, OFFSET 37, LENGTH 1
	MSG NAME: ZV_NV - ZV Nachverriegelung, OFFSET 38, LENGTH 1
	MSG NAME: SCHL_BEF - Mechanical / FB key active, OFFSET 39, LENGTH 1
	MSG NAME: THR_VERRI - Right rear door lock, OFFSET 40, LENGTH 1
	MSG NAME: THR_ENTRI - Unlocking doors, rear right, OFFSET 41, LENGTH 1
	MSG NAME: THL_VERRI - Left rear door lock, OFFSET 42, LENGTH 1
	MSG NAME: THL_ENTRI - Unlocking doors, rear left, OFFSET 43, LENGTH 1
	MSG NAME: TVR_VERRI - Right front door lock, OFFSET 44, LENGTH 1
	MSG NAME: TVR_ENTRI - Unlock Right front door, OFFSET 45, LENGTH 1
	MSG NAME: TVL_VERRI - Left front door lock, OFFSET 46, LENGTH 1
	MSG NAME: TVL_ENTRI - Unlock Left front door, OFFSET 47, LENGTH 1
ECU NAME: EZS_A11, ID: 0x0016. MSG COUNT: 1
	MSG NAME: U_BATT - (V) Batteriespannung, OFFSET 0, LENGTH 8
ECU NAME: EZS_A12, ID: 0x0180. MSG COUNT: 2
	MSG NAME: MOB_STAT - Status mobility account, OFFSET 0, LENGTH 3
	MSG NAME: MOB_AKT - Mobility account activated, OFFSET 8, LENGTH 1
ECU NAME: EZS_A4, ID: 0x0058. MSG COUNT: 2
	MSG NAME: SCHLUE_ID - SchlüsselID from EZS, OFFSET 0, LENGTH 32
	MSG NAME: KM_EZS - (km) (Km) sailed derter mileage from EZS, OFFSET 32, LENGTH 24
ECU NAME: EZS_A9, ID: 0x00B2. MSG COUNT: 2
	MSG NAME: VIN_MSG - VIN Control unit, OFFSET 6, LENGTH 2
	MSG NAME: VIN_DATA - VIN data, OFFSET 8, LENGTH 56
ECU NAME: KG_A1, ID: 0x01B2. MSG COUNT: 15
	MSG NAME: M5 - Messg. 5: "selector lever in P please od N position.", OFFSET 0, LENGTH 1
	MSG NAME: M4 - Messg. 4: "Check chip card / key battery" (white), OFFSET 1, LENGTH 1
	MSG NAME: M3 - Messg. 3: "selector lever to the P" (red tone), OFFSET 2, LENGTH 1
	MSG NAME: M2 - Messg. 2 "/ recognized chip card keys in the vehicle" (white), OFFSET 3, LENGTH 1
	MSG NAME: M1 - Messg. 1 "/ not recognized chip card key" (White), OFFSET 4, LENGTH 1
	MSG NAME: M0 - Messg. 0 "chip card / key is not recognized" (red), OFFSET 5, LENGTH 1
	MSG NAME: WARNTON_KG - switch on warning, OFFSET 6, LENGTH 1
	MSG NAME: M12 - Messg. "Take chip card / key!": 12, OFFSET 9, LENGTH 1
	MSG NAME: M11 - Messg. 11: "Reserved", OFFSET 10, LENGTH 1
	MSG NAME: M10 - Messg. 10: "Reserved", OFFSET 11, LENGTH 1
	MSG NAME: M9 - Messg. 9: "Keyless Go in diagnosis", OFFSET 12, LENGTH 1
	MSG NAME: M8 - Messg. 8: "Door open", OFFSET 13, LENGTH 1
	MSG NAME: M7 - Messg. 7: Reserved, OFFSET 14, LENGTH 1
	MSG NAME: M6 - Messg. 6: "Reserved", OFFSET 15, LENGTH 1
	MSG NAME: KM_REST_KG - (km) (Km) way indication Keyless Go, OFFSET 16, LENGTH 8
ECU NAME: KG_A2, ID: 0x0050. MSG COUNT: 7
	MSG NAME: FHR_KG - rear window open / close right, OFFSET 0, LENGTH 1
	MSG NAME: FHL_KG - Open windows, rear left / Close, OFFSET 1, LENGTH 1
	MSG NAME: FVR_KG - Front windows open / close right, OFFSET 2, LENGTH 1
	MSG NAME: FVL_KG - Open windows front left / Close, OFFSET 3, LENGTH 1
	MSG NAME: SHD_KG - Open / close SHD, OFFSET 4, LENGTH 1
	MSG NAME: KB_RI_KG - Direction touch control: open [0] include [1], OFFSET 5, LENGTH 1
	MSG NAME: KB_MOD_KG - Touch control automatic operation [1] Manual [0], OFFSET 6, LENGTH 1
ECU NAME: EZS_ANZ, ID: 0x0332. MSG COUNT: 8
	MSG NAME: EZS_M7 - Meldg.7: "MK", OFFSET 0, LENGTH 1
	MSG NAME: EZS_M6 - Meldg.6: "MK Manual recharging failed", OFFSET 1, LENGTH 1
	MSG NAME: EZS_M5 - Meldg.5: "MK Manual recharging successful", OFFSET 2, LENGTH 1
	MSG NAME: EZS_M4 - Meldg.4: "MK Manual recharging is done", OFFSET 3, LENGTH 1
	MSG NAME: EZS_M3 - Meldg.3: "MK Authorization Error", OFFSET 4, LENGTH 1
	MSG NAME: EZS_M2 - Meldg.2 "expired MK, veh locked.", OFFSET 5, LENGTH 1
	MSG NAME: EZS_M1 - Meldg.1: "MK immediately reload", OFFSET 6, LENGTH 1
	MSG NAME: EZS_M0 - Meldg.0: "MK state reduces", OFFSET 7, LENGTH 1
ECU NAME: TP_EZS_CP5, ID: 0x03BE. MSG COUNT: 1
	MSG NAME: TP_EZS_CP - Kommunikation EZS zur CP, OFFSET 0, LENGTH 64
ECU NAME: NM_EZS, ID: 0x0400. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_EZS, ID: 0x05FF. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_EZS, ID: 0x0760. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_EZS, ID: 0x07C0. MSG COUNT: 56
	MSG NAME: EZS_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: EZS_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: EZS_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: EZS_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: EZS_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: EZS_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: EZS_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: EZS_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: EZS_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: EZS_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: EZS_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: EZS_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: EZS_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: EZS_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: EZS_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: EZS_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: EZS_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: EZS_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: EZS_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: EZS_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: EZS_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: EZS_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: EZS_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: EZS_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: EZS_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: EZS_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: EZS_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: EZS_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: EZS_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: EZS_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: EZS_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: EZS_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: EZS_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: EZS_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: EZS_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: EZS_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: EZS_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: EZS_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: EZS_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: EZS_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: EZS_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: EZS_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: EZS_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: EZS_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: EZS_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: EZS_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: EZS_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: EZS_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: EZS_PGV04 - State variable 04h, OFFSET 48, LENGTH 1
	MSG NAME: EZS_PGV03 - State variable 03h, OFFSET 49, LENGTH 1
	MSG NAME: EZS_PGV02 - State variable 02h, OFFSET 50, LENGTH 1
	MSG NAME: EZS_PGV01 - State variable 01h, OFFSET 51, LENGTH 1
	MSG NAME: EZS_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: EZS_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: EZS_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: EZS_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
ECU NAME: PROD_A1, ID: 0x001D. MSG COUNT: 1
	MSG NAME: PROD_MODE - Produktionsmodus aktiv, OFFSET 0, LENGTH 1
ECU NAME: ZGW_A4, ID: 0x01BC. MSG COUNT: 10
	MSG NAME: RLS_KM_M - Remaining distance in km [0] miles [1], OFFSET 0, LENGTH 1
	MSG NAME: RLSZ_PRIO - Priority: remaining distance [0], remaining time [1], OFFSET 1, LENGTH 1
	MSG NAME: SV_WARN - Status Service Warning, OFFSET 2, LENGTH 2
	MSG NAME: SV_ANZ_MOD - display mode, OFFSET 4, LENGTH 2
	MSG NAME: SV_UMFANG - scope of service, OFFSET 6, LENGTH 2
	MSG NAME: SV_WERT - (ASCII) (ASCII) Service quality, OFFSET 8, LENGTH 8
	MSG NAME: REST_ZEIT - (Tage) (Days) Maturity, OFFSET 16, LENGTH 16
	MSG NAME: SV_ANZ_SS - Num. Sonderserv. [0], no Qty. See [1], OFFSET 36, LENGTH 1
	MSG NAME: WARTUNG_OK - WR data valid [0] invalid [1] valid, OFFSET 37, LENGTH 1
	MSG NAME: REST_WEG - (km(miles)) (Km (miles)) remaining distance, OFFSET 40, LENGTH 24
ECU NAME: ZGW_A5, ID: 0x001F. MSG COUNT: 39
	MSG NAME: LAND - Country-specific coding SA, OFFSET 0, LENGTH 4
	MSG NAME: LL_RL - Left / right-hand drive, OFFSET 6, LENGTH 2
	MSG NAME: GUARD_B4 - Special Protection Guard B4, OFFSET 8, LENGTH 1
	MSG NAME: BEHI_FZG - Conversion for disabled (only tester), OFFSET 9, LENGTH 1
	MSG NAME: TAXI_FUNKAUF - Radio override taxi, OFFSET 10, LENGTH 1
	MSG NAME: SO_FZG - special vehicle, OFFSET 11, LENGTH 1
	MSG NAME: TAXI_HIRU - Taxi call for help, OFFSET 12, LENGTH 1
	MSG NAME: TAXI_DZ - Connection for roof sign, OFFSET 13, LENGTH 1
	MSG NAME: TAXI_NOTALM - Taxi emergency alarm system, OFFSET 14, LENGTH 1
	MSG NAME: TAXI_INT - Taxi Power, OFFSET 15, LENGTH 1
	MSG NAME: KB_SPERR_KLA - Lock convection-touch control, OFFSET 16, LENGTH 1
	MSG NAME: KB_MAN_KLA - Mode convection Comfort Free automatically [0] manually [1], OFFSET 17, LENGTH 1
	MSG NAME: KB_AUTO - Mode Comfort Free manually [0] automatically [1], OFFSET 18, LENGTH 1
	MSG NAME: ZV_NOT_PAS - Emergency opening inactive (only tester), OFFSET 22, LENGTH 1
	MSG NAME: GUARD_B6 - Special Protection Guard B6 / 7, OFFSET 23, LENGTH 1
	MSG NAME: FCOD_KAR - Vehicle code body, OFFSET 24, LENGTH 3
	MSG NAME: FCOD_BR - Vehicle Code series, OFFSET 27, LENGTH 5
	MSG NAME: PRW_VH - Platt Roll Warner available, OFFSET 32, LENGTH 1
	MSG NAME: FCOD_MOT - Motor vehicle code, OFFSET 34, LENGTH 6
	MSG NAME: XEN_VH - Xenon light available, OFFSET 41, LENGTH 1
	MSG NAME: SRA_VH - Scheinw.-Reiniggs. system prev., OFFSET 42, LENGTH 1
	MSG NAME: KLA_VH - Air conditioning available, OFFSET 43, LENGTH 1
	MSG NAME: NAG_VH - available automatic transmission, OFFSET 44, LENGTH 1
	MSG NAME: KSG_VH - Comfort manual available, OFFSET 45, LENGTH 1
	MSG NAME: MEMORY_VH - Driver seat memory available, OFFSET 46, LENGTH 1
	MSG NAME: KP_VH - Communication platform available, OFFSET 47, LENGTH 1
	MSG NAME: ART_VH - SA ART available, OFFSET 48, LENGTH 1
	MSG NAME: STH_VH - SA auxiliary heating available, OFFSET 50, LENGTH 1
	MSG NAME: HFS_VH - SA remote boot lid closing, OFFSET 51, LENGTH 1
	MSG NAME: ALB_VH - SA automatic load floor available, OFFSET 52, LENGTH 1
	MSG NAME: CDC_VH - SA-CD Changer available, OFFSET 53, LENGTH 1
	MSG NAME: PTS_VH - Parktronic System, OFFSET 56, LENGTH 1
	MSG NAME: AHK_VH - Trailer hitch available, OFFSET 57, LENGTH 1
	MSG NAME: HR_VH - Rear blind available, OFFSET 58, LENGTH 1
	MSG NAME: EDW_VH - SA Car alarm available, OFFSET 59, LENGTH 1
	MSG NAME: IRS_VH - SA interior protection available, OFFSET 60, LENGTH 1
	MSG NAME: KG_VH - SA Keyless Go there, OFFSET 61, LENGTH 1
	MSG NAME: ERS_LICHT - Complete replacement of light allowed, OFFSET 62, LENGTH 1
	MSG NAME: WWSH_VH - Washing water hose heating RL or C490 [0], LL or C875 [1], OFFSET 63, LENGTH 1
ECU NAME: ZGW_A6, ID: 0x001E. MSG COUNT: 2
	MSG NAME: VER_JAHR - year specification, OFFSET 1, LENGTH 5
	MSG NAME: VER_AE - change year, OFFSET 6, LENGTH 2
ECU NAME: GW_C_B1, ID: 0x0002. MSG COUNT: 11
	MSG NAME: RIZ_VL - (Impulse) (Pulses) pulse ring counter left front wheel (48 per revolution), OFFSET 0, LENGTH 8
	MSG NAME: RIZ_VR - (Impulse) (Pulses) pulse ring counter right front wheel (48 per revolution), OFFSET 8, LENGTH 8
	MSG NAME: N_MOT - (1/min) (1 / min) engine speed, OFFSET 16, LENGTH 16
	MSG NAME: T_MOT - (°C) (° C) engine coolant temperature, OFFSET 32, LENGTH 8
	MSG NAME: LW_PA_GW - Steering angle parity bit (even parity), OFFSET 40, LENGTH 1
	MSG NAME: LW_OV_GW - Steering angle sensor: Overflow, OFFSET 41, LENGTH 1
	MSG NAME: LW_CF_GW - Steering angle sensor: Code Error, OFFSET 42, LENGTH 1
	MSG NAME: LW_INI_GW - Steering angle sensor: not initialized, OFFSET 43, LENGTH 1
	MSG NAME: LW_VZ_GW - Steering angle sign (right [0], left [1]), OFFSET 44, LENGTH 1
	MSG NAME: LW_GW - (°) (°) steering angle, OFFSET 45, LENGTH 11
	MSG NAME: T_OEL - (°C) (° C) Oil Temperature, OFFSET 56, LENGTH 8
ECU NAME: GW_C_B2, ID: 0x0003. MSG COUNT: 31
	MSG NAME: ART_ABW_AKT - ART-distance warning is switched on, OFFSET 0, LENGTH 1
	MSG NAME: KOMP_BAUS - turn air compressor: Acceleration, OFFSET 1, LENGTH 1
	MSG NAME: KOMP_NOTAUS - Air compressor Emergency Shutdown, OFFSET 2, LENGTH 1
	MSG NAME: LUEFT_MOT_KL - Motor fan defective indicator light, OFFSET 3, LENGTH 1
	MSG NAME: BRE_AKT_ESP - ESP brake intervention active, OFFSET 4, LENGTH 1
	MSG NAME: BLS_UNT - Brake light suppression, OFFSET 5, LENGTH 1
	MSG NAME: BLS_ST - Status Brake Light Switch, OFFSET 6, LENGTH 2
	MSG NAME: RG - engaged reverse gear (all transmission), OFFSET 8, LENGTH 1
	MSG NAME: P - Park position inserted, OFFSET 9, LENGTH 1
	MSG NAME: BELADUNG - loading, OFFSET 10, LENGTH 2
	MSG NAME: WHC - Gear selector lever position (NOS only), OFFSET 12, LENGTH 4
	MSG NAME: DRTGVL - Rotation direction left front wheel, OFFSET 16, LENGTH 2
	MSG NAME: DVL - (1/min) (1 / min) Left Front wheel, OFFSET 18, LENGTH 14
	MSG NAME: ST2_LED_DL - LED 2-stage switch continuous light, OFFSET 32, LENGTH 1
	MSG NAME: ST3_LEDR_BL - Right LED 3-position switch flashing light, OFFSET 33, LENGTH 1
	MSG NAME: ST3_LEDR_DL - Right LED 3-position switch continuous light, OFFSET 34, LENGTH 1
	MSG NAME: ST3_LEDL_BL - Left LED 3-stage switch indicator, OFFSET 35, LENGTH 1
	MSG NAME: ST3_LEDL_DL - Left LED 3-stage switch continuous light, OFFSET 36, LENGTH 1
	MSG NAME: INF_RFE_FSG - FSG: EHB ASG in fallback, OFFSET 37, LENGTH 1
	MSG NAME: KPL - clutch is pressed, OFFSET 38, LENGTH 1
	MSG NAME: LTG_CHK_POS - Line monitoring possible, OFFSET 39, LENGTH 1
	MSG NAME: WHST - Gear selector lever position (NAG, KSG, CVT), OFFSET 40, LENGTH 3
	MSG NAME: MBRE_ESP - (Nm) (Nm) Adjusted braking torque, OFFSET 44, LENGTH 12
	MSG NAME: ZWP_EIN_MS - Switch on auxiliary water pump, OFFSET 56, LENGTH 1
	MSG NAME: ZH_AUS_MS - Request from PTC Heaters, OFFSET 57, LENGTH 1
	MSG NAME: N_VRBT_SBCSH_AKT - SBC-S / H active ASG must not switch to "N", OFFSET 58, LENGTH 1
	MSG NAME: NOTBRE - Emergency braking (brake light flashing), OFFSET 59, LENGTH 1
	MSG NAME: ZVB_EIN_MS - Turn on additional consumer, OFFSET 60, LENGTH 1
	MSG NAME: SUB_ABL_L - Substitution low beam left, OFFSET 61, LENGTH 1
	MSG NAME: SUB_ABL_R - Substitution low beam right, OFFSET 62, LENGTH 1
	MSG NAME: LL_STBL - Idle is stable, OFFSET 63, LENGTH 1
ECU NAME: GW_C_B3, ID: 0x0222. MSG COUNT: 7
	MSG NAME: T_GET - (°C) (° C) transmission oil temperature, OFFSET 0, LENGTH 8
	MSG NAME: AY_S - (m/s²) (M / s²) Fahrzeugquerbeschleunig. the center of gravity (+ = left), OFFSET 8, LENGTH 8
	MSG NAME: FTK_BMI - Code acceleration type (> 100: dynamic), OFFSET 16, LENGTH 8
	MSG NAME: FTK_LMI - Code type lateral acceleration (> 100: dynamic), OFFSET 24, LENGTH 8
	MSG NAME: GIER_ROH - (°/s) (° / s) raw signal yaw rate without adjustment / filtration (+ = left), OFFSET 40, LENGTH 16
	MSG NAME: EHB_BN - EHB-board power status, OFFSET 56, LENGTH 2
	MSG NAME: HZL_ST - status heating, OFFSET 58, LENGTH 2
ECU NAME: GW_C_B4, ID: 0x0322. MSG COUNT: 7
	MSG NAME: PRESF_TGL - Presafe toggle, OFFSET 0, LENGTH 1
	MSG NAME: PRESF_R_SVR - Presafe-seat adjustment, front right, OFFSET 4, LENGTH 2
	MSG NAME: PRESF_L_SVL - Presafe-seat adjustment, front left, OFFSET 6, LENGTH 2
	MSG NAME: PRESF_R_FH - Presafe adjustment window front right, OFFSET 8, LENGTH 2
	MSG NAME: PRESF_L_FH - Presafe adjustment window front left, OFFSET 10, LENGTH 2
	MSG NAME: PRESF_R_SHD - Presafe adjustment slide / tilt sunroof, OFFSET 12, LENGTH 2
	MSG NAME: PRESF_L_SHD - Presafe adjustment slide / tilt sunroof, OFFSET 14, LENGTH 2
ECU NAME: GW_C_B5, ID: 0x010A. MSG COUNT: 7
	MSG NAME: RIZ_HL - (Impulse) (Pulses) pulse ring counter left rear wheel (48 per revolution), OFFSET 0, LENGTH 8
	MSG NAME: RIZ_HR - (Impulse) (Pulses) pulse ring counter right rear wheel (48 per revolution), OFFSET 8, LENGTH 8
	MSG NAME: DRTGHR - Direction of rotation right rear wheel, OFFSET 16, LENGTH 2
	MSG NAME: DHR - (1/min) (1 / min), rear right wheel speed, OFFSET 18, LENGTH 14
	MSG NAME: DRTGHL - Rotation direction left rear wheel, OFFSET 32, LENGTH 2
	MSG NAME: DHL - (1/min) (1 / min), rear left wheel speed, OFFSET 34, LENGTH 14
	MSG NAME: FMMOTMAX - Factor for fill value. d. Max. Mom with remo.. A.druck, OFFSET 48, LENGTH 8
ECU NAME: GW_C_B7, ID: 0x0005. MSG COUNT: 2
	MSG NAME: DRTGVR - Direction of rotation right front wheel, OFFSET 32, LENGTH 2
	MSG NAME: DVR - (1/min) (1 / min) the right front wheel speed, OFFSET 34, LENGTH 14
ECU NAME: GW_D_B1, ID: 0x018C. MSG COUNT: 2
	MSG NAME: AUT_STAT - Authorization Status: [0] not authorized authorized [1], OFFSET 3, LENGTH 1
	MSG NAME: LIVE_CP - Alive message CP, OFFSET 4, LENGTH 1
ECU NAME: GW_D_B2, ID: 0x00F2. MSG COUNT: 1
	MSG NAME: RDU - Remote door unlock, OFFSET 0, LENGTH 1
ECU NAME: TP_CP_EZS5, ID: 0x00F9. MSG COUNT: 1
	MSG NAME: TP_CP_EZS - Kommunikation CP zum EZS, OFFSET 0, LENGTH 64
ECU NAME: TP_CP_KOMBI4, ID: 0x01A1. MSG COUNT: 1
	MSG NAME: TP_CP_KOMBI - Kommunikation CP zum KOMBI, OFFSET 0, LENGTH 64
ECU NAME: TP_TELEAID_AGW6, ID: 0x01C0. MSG COUNT: 1
	MSG NAME: TP_TELEAID_AGW - Kommunikation TELEAID zum AGW, OFFSET 0, LENGTH 64
ECU NAME: TP_WR_KOMBI3, ID: 0x01A0. MSG COUNT: 1
	MSG NAME: TP_WR_KOMBI - Kommunikation WR zum KOMBI, OFFSET 0, LENGTH 64
ECU NAME: NM_ZGW, ID: 0x0404. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_SD, ID: 0x0538. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_ZGW, ID: 0x0764. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_AAG, ID: 0x0730. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_AGW, ID: 0x05D6. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_ALB, ID: 0x0561. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_ARMADA, ID: 0x06BC. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_BSG, ID: 0x0732. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_DBE, ID: 0x0667. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_EZS, ID: 0x04E0. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_FDSVL, ID: 0x06BE. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_FDSVR, ID: 0x06BF. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_HFS, ID: 0x0577. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_KLA, ID: 0x0791. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_KOMBI, ID: 0x05B4. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_LRK, ID: 0x06AF. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST0, ID: 0x0640. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST1, ID: 0x0641. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST10, ID: 0x064A. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST11, ID: 0x064B. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST12, ID: 0x064C. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST13, ID: 0x064D. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST14, ID: 0x064E. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST15, ID: 0x064F. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST16, ID: 0x0540. MSG COUNT: 0
ECU NAME: D_RQ_MOST17, ID: 0x0541. MSG COUNT: 0
ECU NAME: D_RQ_MOST18, ID: 0x0542. MSG COUNT: 0
ECU NAME: D_RQ_MOST19, ID: 0x0543. MSG COUNT: 0
ECU NAME: D_RQ_MOST2, ID: 0x0642. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST20, ID: 0x0544. MSG COUNT: 0
ECU NAME: D_RQ_MOST21, ID: 0x0545. MSG COUNT: 0
ECU NAME: D_RQ_MOST22, ID: 0x0546. MSG COUNT: 0
ECU NAME: D_RQ_MOST23, ID: 0x0547. MSG COUNT: 0
ECU NAME: D_RQ_MOST24, ID: 0x0548. MSG COUNT: 0
ECU NAME: D_RQ_MOST25, ID: 0x0549. MSG COUNT: 0
ECU NAME: D_RQ_MOST26, ID: 0x054A. MSG COUNT: 0
ECU NAME: D_RQ_MOST27, ID: 0x054B. MSG COUNT: 0
ECU NAME: D_RQ_MOST28, ID: 0x054C. MSG COUNT: 0
ECU NAME: D_RQ_MOST29, ID: 0x054D. MSG COUNT: 0
ECU NAME: D_RQ_MOST3, ID: 0x0643. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST30, ID: 0x054E. MSG COUNT: 0
ECU NAME: D_RQ_MOST31, ID: 0x054F. MSG COUNT: 0
ECU NAME: D_RQ_MOST4, ID: 0x0644. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST5, ID: 0x0645. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST6, ID: 0x0646. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST7, ID: 0x0647. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST8, ID: 0x0648. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MOST9, ID: 0x0649. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MRM, ID: 0x06D5. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_MSS, ID: 0x0726. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_OBF, ID: 0x06A5. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_PFDS, ID: 0x072E. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_PTS, ID: 0x0733. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_RDK, ID: 0x06B8. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_RWT, ID: 0x0560. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_SAM_B, ID: 0x0661. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_SAM_H, ID: 0x0563. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_SAM_V, ID: 0x0662. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_SB, ID: 0x06AD. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_SF, ID: 0x06AC. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_SHZ, ID: 0x057B. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_STH, ID: 0x0739. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_THL, ID: 0x0749. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_THR, ID: 0x074B. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_TVL, ID: 0x06C8. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_TVR, ID: 0x06CA. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_UBF, ID: 0x06BD. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_WSS, ID: 0x06A8. MSG COUNT: 1
	MSG NAME: D_RQ - KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: D_RQ_GLOBAL, ID: 0x001C. MSG COUNT: 1
	MSG NAME: D_RQ - Globaler KWP2000 Diagnose-Request, OFFSET 0, LENGTH 64
ECU NAME: KOMBI_A1, ID: 0x000C. MSG COUNT: 30
	MSG NAME: KL_58D_B - (%) (%) Brightness meter lighting, OFFSET 0, LENGTH 8
	MSG NAME: V_SIGNAL - (km/h) (Km / h) vehicle speed, OFFSET 8, LENGTH 8
	MSG NAME: DZ_EIN - Switch roof sign (taxi) a [1], [0], OFFSET 16, LENGTH 1
	MSG NAME: TFSM_B - Tank level minimum, OFFSET 17, LENGTH 1
	MSG NAME: AUTO_TUER - Automatic door locks: a [1], [0], OFFSET 18, LENGTH 1
	MSG NAME: T_C - Temperature unit "° C" [1], "° F" [0], OFFSET 19, LENGTH 1
	MSG NAME: TFL_EIN - daytime running lights, OFFSET 20, LENGTH 1
	MSG NAME: ANH_UEBW - Switch trailer monitoring, OFFSET 21, LENGTH 1
	MSG NAME: SCHLUE_ABH_EIN - Key-dependent storage: a [1], [0], OFFSET 22, LENGTH 1
	MSG NAME: SP_PARK_SPERR - Levels in the park position: closed [1], allowed [0], OFFSET 23, LENGTH 1
	MSG NAME: ESH_POS_SP - Seat longitudinal position for I / O help save, OFFSET 24, LENGTH 1
	MSG NAME: SP_ANKL_SPERR - Spiegelanklappen locked at lock Fzg. [1], allowed [0], OFFSET 25, LENGTH 1
	MSG NAME: FDS_B_CHAR - FDS characteristic passenger dominant [1], discreet [0], OFFSET 26, LENGTH 1
	MSG NAME: FDS_F_CHAR - FDS characteristic dominant driver [1], discreet [0], OFFSET 27, LENGTH 1
	MSG NAME: ESH_POS_STD - Sitzverstellweg at I / O help to default, OFFSET 28, LENGTH 1
	MSG NAME: ESH_SITZ_EIN - Seat adjustment for I / O help a [1], [0], OFFSET 29, LENGTH 1
	MSG NAME: ESH_LENK_EIN - Adjustable steering column for I / O help a [1], [0], OFFSET 30, LENGTH 1
	MSG NAME: ESH_AUTO_EIN - Easy Entry / automatic. Positionierg. a [1], [0], OFFSET 31, LENGTH 1
	MSG NAME: SLF - Memory Scan [1], tuning [0], OFFSET 32, LENGTH 1
	MSG NAME: RR_KM - Trip computer "km" [1], "miles" [0], OFFSET 33, LENGTH 1
	MSG NAME: FL_OK - High beam switch permits, OFFSET 34, LENGTH 1
	MSG NAME: UFB_EIN - Ambient lighting a, OFFSET 35, LENGTH 1
	MSG NAME: SPRACHE - language, OFFSET 36, LENGTH 4
	MSG NAME: STHL_EIN_KOMBI - / Off auxiliary heating independent ventilation, OFFSET 40, LENGTH 1
	MSG NAME: VWZ_AKT - Preset time is enabled (LED on), OFFSET 41, LENGTH 1
	MSG NAME: VWZ_AUS_MFL - Preselection time off (from LED) over MFL, OFFSET 42, LENGTH 1
	MSG NAME: AMB_LI - Light level ambient light, OFFSET 43, LENGTH 4
	MSG NAME: RDK_AKT - enable RDK, OFFSET 47, LENGTH 1
	MSG NAME: INLI_NLZ - (s) (S) Interior lighting afterglow, OFFSET 48, LENGTH 8
	MSG NAME: ABL_NLZ - (s) (S) standing or fog light afterglow (SWA), OFFSET 56, LENGTH 8
ECU NAME: KOMBI_A2, ID: 0x0038. MSG COUNT: 4
	MSG NAME: TAGE_ZAHL - (Tage) (Day) day cycle counter, OFFSET 0, LENGTH 16
	MSG NAME: TAG - (Tage) (Days) Day, OFFSET 16, LENGTH 8
	MSG NAME: MONAT - (Monate) (Months) Monthly, OFFSET 24, LENGTH 8
	MSG NAME: JAHR - (Jahre) (Years) Year, OFFSET 32, LENGTH 8
ECU NAME: KOMBI_A4, ID: 0x020C. MSG COUNT: 1
	MSG NAME: P_KI - Prioritäten am Kombi, OFFSET 5, LENGTH 3
ECU NAME: KOMBI_A5, ID: 0x01CA. MSG COUNT: 25
	MSG NAME: KI_STAT - status combi, OFFSET 0, LENGTH 8
	MSG NAME: BUTTON_4_2 - phone End, OFFSET 8, LENGTH 1
	MSG NAME: BUTTON_4_1 - phone Send, OFFSET 9, LENGTH 1
	MSG NAME: BUTTON_3_2 - "-" key, OFFSET 10, LENGTH 1
	MSG NAME: BUTTON_3_1 - "+" Key, OFFSET 11, LENGTH 1
	MSG NAME: BUTTON_2_2 - reserve, OFFSET 12, LENGTH 1
	MSG NAME: BUTTON_2_1 - reserve, OFFSET 13, LENGTH 1
	MSG NAME: BUTTON_1_2 - Previous display, OFFSET 14, LENGTH 1
	MSG NAME: BUTTON_1_1 - Next display, OFFSET 15, LENGTH 1
	MSG NAME: BUTTON_8_2 - reserve, OFFSET 16, LENGTH 1
	MSG NAME: BUTTON_8_1 - reserve, OFFSET 17, LENGTH 1
	MSG NAME: BUTTON_7_2 - reserve, OFFSET 18, LENGTH 1
	MSG NAME: BUTTON_7_1 - reserve, OFFSET 19, LENGTH 1
	MSG NAME: BUTTON_6_2 - reserve, OFFSET 20, LENGTH 1
	MSG NAME: BUTTON_6_1 - reserve, OFFSET 21, LENGTH 1
	MSG NAME: BUTTON_5_2 - reserve, OFFSET 22, LENGTH 1
	MSG NAME: BUTTON_5_1 - reserve, OFFSET 23, LENGTH 1
	MSG NAME: PTT_4_2 - reserve, OFFSET 24, LENGTH 1
	MSG NAME: PTT_4_1 - reserve, OFFSET 25, LENGTH 1
	MSG NAME: PTT_3_2 - reserve, OFFSET 26, LENGTH 1
	MSG NAME: PTT_3_1 - reserve, OFFSET 27, LENGTH 1
	MSG NAME: PTT_2_2 - reserve, OFFSET 28, LENGTH 1
	MSG NAME: PTT_2_1 - reserve, OFFSET 29, LENGTH 1
	MSG NAME: PTT_1_2 - disable Linguatronic, OFFSET 30, LENGTH 1
	MSG NAME: PTT_1_1 - Enable Linguatronic, OFFSET 31, LENGTH 1
ECU NAME: KOMBI_A6, ID: 0x009E. MSG COUNT: 2
	MSG NAME: SCHLUE_ID_KI - SchlüsselID from COMBI, OFFSET 0, LENGTH 32
	MSG NAME: KM_KI - (km) (Km) sailed derter mileage from COMBI, OFFSET 32, LENGTH 24
ECU NAME: KOMBI_A7, ID: 0x0194. MSG COUNT: 3
	MSG NAME: DISP_DIMM - (%) (%) Display dimming, OFFSET 0, LENGTH 8
	MSG NAME: HD_BEGRENZ - Tailgate limiting a, OFFSET 10, LENGTH 1
	MSG NAME: KOMBI_MW_OK - Combi is worth more capable, OFFSET 15, LENGTH 1
ECU NAME: KOMBI_A8, ID: 0x032A. MSG COUNT: 25
	MSG NAME: KI_STAT_MSS - status combi, OFFSET 0, LENGTH 8
	MSG NAME: BUTTON_4_2_MSS - phone End, OFFSET 8, LENGTH 1
	MSG NAME: BUTTON_4_1_MSS - phone Send, OFFSET 9, LENGTH 1
	MSG NAME: BUTTON_3_2_MSS - "-" key, OFFSET 10, LENGTH 1
	MSG NAME: BUTTON_3_1_MSS - "+" Key, OFFSET 11, LENGTH 1
	MSG NAME: BUTTON_2_2_MSS - reserve, OFFSET 12, LENGTH 1
	MSG NAME: BUTTON_2_1_MSS - reserve, OFFSET 13, LENGTH 1
	MSG NAME: BUTTON_1_2_MSS - Previous display, OFFSET 14, LENGTH 1
	MSG NAME: BUTTON_1_1_MSS - Next display, OFFSET 15, LENGTH 1
	MSG NAME: BUTTON_8_2_MSS - reserve, OFFSET 16, LENGTH 1
	MSG NAME: BUTTON_8_1_MSS - reserve, OFFSET 17, LENGTH 1
	MSG NAME: BUTTON_7_2_MSS - reserve, OFFSET 18, LENGTH 1
	MSG NAME: BUTTON_7_1_MSS - reserve, OFFSET 19, LENGTH 1
	MSG NAME: BUTTON_6_2_MSS - reserve, OFFSET 20, LENGTH 1
	MSG NAME: BUTTON_6_1_MSS - reserve, OFFSET 21, LENGTH 1
	MSG NAME: BUTTON_5_2_MSS - reserve, OFFSET 22, LENGTH 1
	MSG NAME: BUTTON_5_1_MSS - reserve, OFFSET 23, LENGTH 1
	MSG NAME: PTT_4_2_MSS - reserve, OFFSET 24, LENGTH 1
	MSG NAME: PTT_4_1_MSS - reserve, OFFSET 25, LENGTH 1
	MSG NAME: PTT_3_2_MSS - reserve, OFFSET 26, LENGTH 1
	MSG NAME: PTT_3_1_MSS - reserve, OFFSET 27, LENGTH 1
	MSG NAME: PTT_2_2_MSS - reserve, OFFSET 28, LENGTH 1
	MSG NAME: PTT_2_1_MSS - reserve, OFFSET 29, LENGTH 1
	MSG NAME: PTT_1_2_MSS - disable Linguatronic, OFFSET 30, LENGTH 1
	MSG NAME: PTT_1_1_MSS - Enable Linguatronic, OFFSET 31, LENGTH 1
ECU NAME: KOMBI_A9, ID: 0x01CB. MSG COUNT: 3
	MSG NAME: KOMBI_IPS_UPD - IPS update request, OFFSET 0, LENGTH 1
	MSG NAME: KOMBI_IPS_INDICATION - Icon confirmation, OFFSET 1, LENGTH 3
	MSG NAME: KOMBI_IPS_CONF - IPS Configuration, OFFSET 4, LENGTH 4
ECU NAME: TP_KOMBI_AGW1, ID: 0x01D0. MSG COUNT: 1
	MSG NAME: TP_KOMBI_AGW - Kommunikation KOMBI zum AGW, OFFSET 0, LENGTH 64
ECU NAME: TP_KOMBI_CP4, ID: 0x03E1. MSG COUNT: 1
	MSG NAME: TP_KOMBI_CP - Kommunikation KOMBI zur CP, OFFSET 0, LENGTH 64
ECU NAME: TP_KOMBI_MSS2, ID: 0x0330. MSG COUNT: 1
	MSG NAME: TP_KOMBI_MSS - Kommunikation KOMBI zum MSS, OFFSET 0, LENGTH 64
ECU NAME: TP_KOMBI_WR3, ID: 0x03E0. MSG COUNT: 1
	MSG NAME: TP_KOMBI_WR - Kommunikation KOMBI zum WR, OFFSET 0, LENGTH 64
ECU NAME: NM_KOMBI, ID: 0x0414. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_KOMBI, ID: 0x04F4. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_KOMBI, ID: 0x0774. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_KOMBI, ID: 0x07D4. MSG COUNT: 64
	MSG NAME: KOMBI_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: KOMBI_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: KOMBI_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: KOMBI_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: KOMBI_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: KOMBI_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: KOMBI_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: KOMBI_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: KOMBI_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: KOMBI_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: KOMBI_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: KOMBI_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: KOMBI_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: KOMBI_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: KOMBI_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: KOMBI_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: KOMBI_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: KOMBI_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: KOMBI_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: KOMBI_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: KOMBI_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: KOMBI_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: KOMBI_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: KOMBI_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: KOMBI_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: KOMBI_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: KOMBI_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: KOMBI_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: KOMBI_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: KOMBI_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: KOMBI_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: KOMBI_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: KOMBI_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: KOMBI_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: KOMBI_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: KOMBI_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: KOMBI_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: KOMBI_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: KOMBI_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: KOMBI_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: KOMBI_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: KOMBI_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: KOMBI_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: KOMBI_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: KOMBI_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: KOMBI_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: KOMBI_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: KOMBI_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: KOMBI_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: KOMBI_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: KOMBI_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: KOMBI_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: KOMBI_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: KOMBI_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: KOMBI_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: KOMBI_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: KOMBI_PGV08 - State variable 08h, OFFSET 56, LENGTH 1
	MSG NAME: KOMBI_PGV07 - State variable 07h, OFFSET 57, LENGTH 1
	MSG NAME: KOMBI_PGV06 - State variable 06h, OFFSET 58, LENGTH 1
	MSG NAME: KOMBI_PGV05 - State variable 05h, OFFSET 59, LENGTH 1
	MSG NAME: KOMBI_PGV04 - State variable 04h, OFFSET 60, LENGTH 1
	MSG NAME: KOMBI_PGV03 - State variable 03h, OFFSET 61, LENGTH 1
	MSG NAME: KOMBI_PGV02 - State variable 02h, OFFSET 62, LENGTH 1
	MSG NAME: KOMBI_PGV01 - State variable 01h, OFFSET 63, LENGTH 1
ECU NAME: MRM_A1, ID: 0x0006. MSG COUNT: 18
	MSG NAME: SGH_EIN_LR - Switch Bugle, OFFSET 0, LENGTH 1
	MSG NAME: LHP_EIN - turn flasher, OFFSET 1, LENGTH 1
	MSG NAME: FL_EIN - High beam switch (requirement), OFFSET 2, LENGTH 1
	MSG NAME: BLI_RE - Directional blinking right (requirement), OFFSET 3, LENGTH 1
	MSG NAME: BLI_LI - Direction flashing left (requirement), OFFSET 4, LENGTH 1
	MSG NAME: SCH_WI_2 - LSS in position III (step 2, requirement), OFFSET 8, LENGTH 1
	MSG NAME: SCH_WI_1 - LSS in position II (stage 1, requirement), OFFSET 9, LENGTH 1
	MSG NAME: SCH_WI_INT - LSS in position I (the rain sensor operation), OFFSET 10, LENGTH 1
	MSG NAME: WASCHEN - washing actuated, OFFSET 11, LENGTH 1
	MSG NAME: TIPP_WISCH - Brief wipe (not W211) is operated, OFFSET 12, LENGTH 1
	MSG NAME: SBS_EIN - Switch on voice control, OFFSET 22, LENGTH 1
	MSG NAME: SBS_AUS - Switch off voice control, OFFSET 23, LENGTH 1
	MSG NAME: LW_PA_B - Steering angle parity bit (even parity), OFFSET 24, LENGTH 1
	MSG NAME: LW_OV_B - Steering angle sensor: Overflow, OFFSET 25, LENGTH 1
	MSG NAME: LW_CF_B - Steering angle sensor: Code Error, OFFSET 26, LENGTH 1
	MSG NAME: LW_INI_B - Steering angle sensor: not initialized, OFFSET 27, LENGTH 1
	MSG NAME: LW_VZ_B - Steering angle sign (right [0], left [1]), OFFSET 28, LENGTH 1
	MSG NAME: LW_B - (°) (°) steering angle, OFFSET 29, LENGTH 11
ECU NAME: MRM_A2, ID: 0x01A8. MSG COUNT: 16
	MSG NAME: WIPPE_4_2 - Button on the bottom right to bottom, OFFSET 0, LENGTH 1
	MSG NAME: WIPPE_4_1 - Button on the right bottom to top, OFFSET 1, LENGTH 1
	MSG NAME: WIPPE_3_2 - Button on the right top to bottom, OFFSET 2, LENGTH 1
	MSG NAME: WIPPE_3_1 - Button on the top right to the top, OFFSET 3, LENGTH 1
	MSG NAME: WIPPE_2_2 - Button on the bottom left to bottom, OFFSET 4, LENGTH 1
	MSG NAME: WIPPE_2_1 - Button on the left bottom to top, OFFSET 5, LENGTH 1
	MSG NAME: WIPPE_1_2 - Button top left to bottom, OFFSET 6, LENGTH 1
	MSG NAME: WIPPE_1_1 - Button top left to top, OFFSET 7, LENGTH 1
	MSG NAME: WIPPE_8_2 - reserve, OFFSET 8, LENGTH 1
	MSG NAME: WIPPE_8_1 - reserve, OFFSET 9, LENGTH 1
	MSG NAME: WIPPE_7_2 - reserve, OFFSET 10, LENGTH 1
	MSG NAME: WIPPE_7_1 - reserve, OFFSET 11, LENGTH 1
	MSG NAME: WIPPE_6_2 - reserve, OFFSET 12, LENGTH 1
	MSG NAME: WIPPE_6_1 - reserve, OFFSET 13, LENGTH 1
	MSG NAME: WIPPE_5_2 - reserve, OFFSET 14, LENGTH 1
	MSG NAME: WIPPE_5_1 - reserve, OFFSET 15, LENGTH 1
ECU NAME: MRM_A3, ID: 0x0296. MSG COUNT: 18
	MSG NAME: LS_ZUR_MRM - Steering column to the rear (toward the driver), OFFSET 0, LENGTH 1
	MSG NAME: LS_VOR_MRM - Steering column to the front, OFFSET 1, LENGTH 1
	MSG NAME: LS_AB_MRM - Steering column downward, OFFSET 2, LENGTH 1
	MSG NAME: LS_AUF_MRM - Steering column according to above, OFFSET 3, LENGTH 1
	MSG NAME: LSVH_UN - Lenksäulenverstellhebel turned down, OFFSET 4, LENGTH 1
	MSG NAME: LSVH_OB - Lenksäulenverstellhebel turned upward, OFFSET 5, LENGTH 1
	MSG NAME: DTC8_ELK - Error code $ 9073, OFFSET 16, LENGTH 1
	MSG NAME: DTC7_ELK - Error code $ 9072, OFFSET 17, LENGTH 1
	MSG NAME: DTC6_ELK - Error code $ 9071, OFFSET 18, LENGTH 1
	MSG NAME: DTC5_ELK - Error code $ 9070, OFFSET 19, LENGTH 1
	MSG NAME: DTC4_ELK - Error code $ 9063, OFFSET 20, LENGTH 1
	MSG NAME: DTC3_ELK - Error code $ 9062, OFFSET 21, LENGTH 1
	MSG NAME: DTC2_ELK - Error code $ 9061, OFFSET 22, LENGTH 1
	MSG NAME: DTC1_ELK - Error code $ 9060, OFFSET 23, LENGTH 1
	MSG NAME: ELH_DEF - ELH defective, OFFSET 24, LENGTH 1
	MSG NAME: DTC11_ELK - Error code $ 9076, OFFSET 29, LENGTH 1
	MSG NAME: DTC10_ELK - Error code $ 9075, OFFSET 30, LENGTH 1
	MSG NAME: DTC9_ELK - Error code $ 9074, OFFSET 31, LENGTH 1
ECU NAME: NM_MRM, ID: 0x0415. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MRM, ID: 0x04F5. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_MRM, ID: 0x0775. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_MRM, ID: 0x07D5. MSG COUNT: 56
	MSG NAME: MRM_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: MRM_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: MRM_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: MRM_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: MRM_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: MRM_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: MRM_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: MRM_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: MRM_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: MRM_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: MRM_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: MRM_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: MRM_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: MRM_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: MRM_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: MRM_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: MRM_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: MRM_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: MRM_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: MRM_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: MRM_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: MRM_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: MRM_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: MRM_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: MRM_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: MRM_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: MRM_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: MRM_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: MRM_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: MRM_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: MRM_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: MRM_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: MRM_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: MRM_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: MRM_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: MRM_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: MRM_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: MRM_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: MRM_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: MRM_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: MRM_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: MRM_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: MRM_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: MRM_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: MRM_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: MRM_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: MRM_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: MRM_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: MRM_PGV08 - State variable 08h, OFFSET 48, LENGTH 1
	MSG NAME: MRM_PGV07 - State variable 07h, OFFSET 49, LENGTH 1
	MSG NAME: MRM_PGV06 - State variable 06h, OFFSET 50, LENGTH 1
	MSG NAME: MRM_PGV05 - State variable 05h, OFFSET 51, LENGTH 1
	MSG NAME: MRM_PGV04 - State variable 04h, OFFSET 52, LENGTH 1
	MSG NAME: MRM_PGV03 - State variable 03h, OFFSET 53, LENGTH 1
	MSG NAME: MRM_PGV02 - State variable 02h, OFFSET 54, LENGTH 1
	MSG NAME: MRM_PGV01 - State variable 01h, OFFSET 55, LENGTH 1
ECU NAME: LRK_A1, ID: 0x0288. MSG COUNT: 5
	MSG NAME: LLFT_LED_EIN - Switch LED wheel ventilation, OFFSET 0, LENGTH 1
	MSG NAME: LHZG_LED_EIN - Switch LED steering wheel heating, OFFSET 1, LENGTH 1
	MSG NAME: LRK_STOERG - LEDs blink LRK wg. disorder, OFFSET 2, LENGTH 1
	MSG NAME: LLFT_EIN - Turn the steering wheel ventilation, OFFSET 3, LENGTH 1
	MSG NAME: LHZG_EIN - Turn steering wheel heating, OFFSET 4, LENGTH 1
ECU NAME: NM_LRK, ID: 0x040F. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_LRK, ID: 0x04EF. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_LRK, ID: 0x076F. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_LRK, ID: 0x07CF. MSG COUNT: 40
	MSG NAME: LRK_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: LRK_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: LRK_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: LRK_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: LRK_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: LRK_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: LRK_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: LRK_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: LRK_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: LRK_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: LRK_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: LRK_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: LRK_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: LRK_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: LRK_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: LRK_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: LRK_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: LRK_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: LRK_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: LRK_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: LRK_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: LRK_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: LRK_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: LRK_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: LRK_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: LRK_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: LRK_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: LRK_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: LRK_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: LRK_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: LRK_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: LRK_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: LRK_PGV08 - State variable 08h, OFFSET 32, LENGTH 1
	MSG NAME: LRK_PGV07 - State variable 07h, OFFSET 33, LENGTH 1
	MSG NAME: LRK_PGV06 - State variable 06h, OFFSET 34, LENGTH 1
	MSG NAME: LRK_PGV05 - State variable 05h, OFFSET 35, LENGTH 1
	MSG NAME: LRK_PGV04 - State variable 04h, OFFSET 36, LENGTH 1
	MSG NAME: LRK_PGV03 - State variable 03h, OFFSET 37, LENGTH 1
	MSG NAME: LRK_PGV02 - State variable 02h, OFFSET 38, LENGTH 1
	MSG NAME: LRK_PGV01 - State variable 01h, OFFSET 39, LENGTH 1
ECU NAME: SAM_V_A1, ID: 0x000A. MSG COUNT: 50
	MSG NAME: KL_61_EIN - terminal 61, OFFSET 0, LENGTH 1
	MSG NAME: SWA_AKT - Injection active headlamps, OFFSET 1, LENGTH 1
	MSG NAME: KL_15R_KG_V - Kl15R a, OFFSET 2, LENGTH 1
	MSG NAME: KL_15_KG_V - F15 / 87 FW one, OFFSET 3, LENGTH 1
	MSG NAME: SGH_ST_EIN - Signal horn is activated, OFFSET 4, LENGTH 1
	MSG NAME: FL_ST_EIN - High beam is turned on, OFFSET 5, LENGTH 1
	MSG NAME: NSW_ST_EIN - Fog lights are turned on, OFFSET 6, LENGTH 1
	MSG NAME: AFL_AKT - Outside light activated by light sensor, OFFSET 7, LENGTH 1
	MSG NAME: NSL_EIN - Switch rear fog light, OFFSET 8, LENGTH 1
	MSG NAME: NSW_EIN - switch fog lights, OFFSET 9, LENGTH 1
	MSG NAME: ABL_EIN - switch on low beam, OFFSET 10, LENGTH 1
	MSG NAME: STL_EIN - Switch on parking lights, OFFSET 11, LENGTH 1
	MSG NAME: DIMM2 - External light dimmed with threshold 2, OFFSET 12, LENGTH 1
	MSG NAME: PL_RE_EIN - Turn right parking light, OFFSET 13, LENGTH 1
	MSG NAME: PL_LI_EIN - Left parking light switch, OFFSET 14, LENGTH 1
	MSG NAME: FL_EIN_SAM_V - Turn on high beams, OFFSET 15, LENGTH 1
	MSG NAME: TFL_EIN_ECE - daytime running lights, OFFSET 16, LENGTH 1
	MSG NAME: KOMP_LFT - Refrigeration compressor runs, OFFSET 17, LENGTH 1
	MSG NAME: HAS_KL - Hand brake applied (control light), OFFSET 18, LENGTH 1
	MSG NAME: KOMP_EIN - Air compressor switched, OFFSET 19, LENGTH 1
	MSG NAME: KOMP_DEF - C compressor drive current output defective, OFFSET 20, LENGTH 1
	MSG NAME: DIAG_15_EIN - Terminal 15 is activated via diagnostics, OFFSET 21, LENGTH 1
	MSG NAME: DIAG_15R_EIN - Terminal 15R via diagnostic activated, OFFSET 22, LENGTH 1
	MSG NAME: BBV_KL - Brake pad wear warning light, OFFSET 23, LENGTH 1
	MSG NAME: BFL_KL - Brake fluid level warning light, OFFSET 24, LENGTH 1
	MSG NAME: WWS_KL - Wash water level too low pilot light, OFFSET 25, LENGTH 1
	MSG NAME: KWS_KL - Cooling water level too low pilot light, OFFSET 26, LENGTH 1
	MSG NAME: MW_AKT_SAM_V - SBC added value: Overrun active, OFFSET 27, LENGTH 1
	MSG NAME: VSTAT_A - SAM / x: v-signal from the EHB ASG, x = B (230), V (211), F (240), OFFSET 28, LENGTH 1
	MSG NAME: SAM_V_PAS - SAM / V passive, OFFSET 29, LENGTH 1
	MSG NAME: BLS_A - SAM / x: brake light switch output EHB ASG, x = B (230), V (211), F (240), OFFSET 30, LENGTH 1
	MSG NAME: INF_RFE_SAM - SAM / x: EHB ASG in fallback mode, x = B (230), V (211,164,251), F (240), OFFSET 31, LENGTH 1
	MSG NAME: NSW_DEF_F - Fog lights defective driver's side, OFFSET 32, LENGTH 1
	MSG NAME: FL_DEF_F - High beam driver's side defective, OFFSET 33, LENGTH 1
	MSG NAME: ABL_DEF_F - Low beam driver's side defective, OFFSET 34, LENGTH 1
	MSG NAME: PL_DEF_VF - front parking light defective driver's side, OFFSET 35, LENGTH 1
	MSG NAME: BLI_DEF_VF - Indicator front defective driver's side, OFFSET 36, LENGTH 1
	MSG NAME: SM_DEF_VF - Side Marker front defective driver's side, OFFSET 37, LENGTH 1
	MSG NAME: SM_DEF_VBF - Side Marker front passenger side defective, OFFSET 38, LENGTH 1
	MSG NAME: INSTR_AUS - Instrument illumination from, OFFSET 39, LENGTH 1
	MSG NAME: BLI_ERS_VF - Replacement Indicator front driver's side active, OFFSET 40, LENGTH 1
	MSG NAME: PL_ERS_VF - Replacement parking light front driver's side active, OFFSET 41, LENGTH 1
	MSG NAME: DIAG_X4_F - Start Xenon4 diagnostic procedure driver's side, OFFSET 42, LENGTH 1
	MSG NAME: BBV_V_50 - Brake lining wear remaining 50%, OFFSET 48, LENGTH 1
	MSG NAME: BBV_V_100 - Brake pad wear front 100%, OFFSET 49, LENGTH 1
	MSG NAME: BBV_H_50 - Brake pad wear rear 50%, OFFSET 50, LENGTH 1
	MSG NAME: BBV_H_100 - Brake pad wear back 100%, OFFSET 51, LENGTH 1
	MSG NAME: EHB_BEH - EHB Behelfsspannungsversorgung, OFFSET 52, LENGTH 2
	MSG NAME: KL15R_ST_RL - Readback signal Kl15R, OFFSET 54, LENGTH 1
	MSG NAME: KL15_ST_RL - Readback signal KL15, OFFSET 55, LENGTH 1
ECU NAME: SAM_V_A2, ID: 0x0017. MSG COUNT: 4
	MSG NAME: T_AUSSEN_B - (°C) (° C) Outside air temperature, OFFSET 0, LENGTH 8
	MSG NAME: P_KAELTE - (bar) (Bar) pressure refrigerant R134a, OFFSET 8, LENGTH 16
	MSG NAME: T_KAELTE - (°C) (° C) temperature refrigerant R134a, OFFSET 24, LENGTH 16
	MSG NAME: I_KOMP - (mA) (MA) current compressor main control valve, OFFSET 40, LENGTH 8
ECU NAME: SAM_V_A3, ID: 0x0070. MSG COUNT: 6
	MSG NAME: DIAG_RS - Diagnosis rain sensor, OFFSET 2, LENGTH 1
	MSG NAME: SCH_WI_1_RS - Steering column switch in stage 1, OFFSET 3, LENGTH 1
	MSG NAME: SAM_V_INIT - SAM_V initialization, OFFSET 4, LENGTH 1
	MSG NAME: KL_86_RS - washing actuated, OFFSET 5, LENGTH 1
	MSG NAME: KL_31B_RS - Wiper outside parking position, OFFSET 6, LENGTH 1
	MSG NAME: RS_INT - Rain sensor on / off (position interval), OFFSET 7, LENGTH 1
ECU NAME: NM_SAM_V, ID: 0x0402. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_SAM_V, ID: 0x04E2. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_SAM_V, ID: 0x0762. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_SAM_V, ID: 0x07C2. MSG COUNT: 19
	MSG NAME: SAM_V_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: SAM_V_PGV07 - State variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: SAM_V_PGV06 - State variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: SAM_V_PGV05 - State variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: SAM_V_PGV04 - State variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: SAM_V_PGV03 - State variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: SAM_V_PGV02 - State variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: SAM_V_PGV01 - State variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: SAM_V_FM01 - Error message 01h, OFFSET 8, LENGTH 16
	MSG NAME: SAM_V_FM02 - Error message 02h, OFFSET 24, LENGTH 16
	MSG NAME: SAM_V_FM03 - Error message 03h, OFFSET 40, LENGTH 16
	MSG NAME: SAM_V_PGV0F - State variable 0Fh, OFFSET 56, LENGTH 1
	MSG NAME: SAM_V_PGV0E - State variable 0Eh, OFFSET 57, LENGTH 1
	MSG NAME: SAM_V_PGV0D - State variable 0Dh, OFFSET 58, LENGTH 1
	MSG NAME: SAM_V_PGV0C - State variable 0Ch, OFFSET 59, LENGTH 1
	MSG NAME: SAM_V_PGV0B - State variable 0Bh, OFFSET 60, LENGTH 1
	MSG NAME: SAM_V_PGV0A - State variable 0Ah, OFFSET 61, LENGTH 1
	MSG NAME: SAM_V_PGV09 - State variable 09h, OFFSET 62, LENGTH 1
	MSG NAME: SAM_V_PGV08 - State variable 08h, OFFSET 63, LENGTH 1
ECU NAME: SAM_B_A1, ID: 0x008C. MSG COUNT: 16
	MSG NAME: RG_SAM_B - engaged reverse gear (manual transmission only), OFFSET 0, LENGTH 1
	MSG NAME: ZWP_LFT - Auxiliary water pump runs, OFFSET 1, LENGTH 1
	MSG NAME: KL_15R_KG_B - Kl15R a, OFFSET 4, LENGTH 1
	MSG NAME: KL_15_KG_B - F15 / 87 FW one, OFFSET 5, LENGTH 1
	MSG NAME: KL_15R_KG_DEF - Driver error for relay Kl15R, OFFSET 6, LENGTH 1
	MSG NAME: KL_15_KG_DEF - Driver error for relay F15 / 87FW, OFFSET 7, LENGTH 1
	MSG NAME: NSW_DEF_BF - Fog lights passenger side defective, OFFSET 8, LENGTH 1
	MSG NAME: FL_DEF_BF - Highbeam passenger side defective, OFFSET 9, LENGTH 1
	MSG NAME: ABL_DEF_BF - Dipped passenger side defective, OFFSET 10, LENGTH 1
	MSG NAME: PL_DEF_VBF - front parking light passenger side defective, OFFSET 11, LENGTH 1
	MSG NAME: BLI_DEF_VBF - Indicator front passenger side defective, OFFSET 12, LENGTH 1
	MSG NAME: BLI_ERS_VBF - Replacement light Indicator front Beif.seite active, OFFSET 16, LENGTH 1
	MSG NAME: PL_ERS_VBF - Replacement light Parkl. front Beif.seite active, OFFSET 17, LENGTH 1
	MSG NAME: DIAG_X4_B - Start Xenon4 diagnostic procedure passenger side, OFFSET 18, LENGTH 1
	MSG NAME: GWHST_P_SAM_B - Gear selector lever position "P" detected, OFFSET 25, LENGTH 1
	MSG NAME: KL_30A_EIN - 2. Battery switch, OFFSET 26, LENGTH 1
ECU NAME: SAM_B_A2, ID: 0x0260. MSG COUNT: 2
	MSG NAME: HUPE_EIN - Trigger the horn warning, OFFSET 7, LENGTH 1
	MSG NAME: HUPEN_EIN_ZEIT - (ms) (Ms) time of the horn actuation, OFFSET 8, LENGTH 8
ECU NAME: NM_SAM_B, ID: 0x0401. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_SAM_B, ID: 0x04E1. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_SAM_B, ID: 0x0761. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_SAM_B, ID: 0x07C1. MSG COUNT: 48
	MSG NAME: SAM_B_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: SAM_B_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: SAM_B_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: SAM_B_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: SAM_B_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: SAM_B_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: SAM_B_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: SAM_B_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: SAM_B_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: SAM_B_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: SAM_B_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: SAM_B_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: SAM_B_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: SAM_B_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: SAM_B_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: SAM_B_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: SAM_B_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: SAM_B_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: SAM_B_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: SAM_B_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: SAM_B_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: SAM_B_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: SAM_B_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: SAM_B_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: SAM_B_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: SAM_B_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: SAM_B_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: SAM_B_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: SAM_B_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: SAM_B_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: SAM_B_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: SAM_B_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: SAM_B_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: SAM_B_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: SAM_B_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: SAM_B_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: SAM_B_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: SAM_B_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: SAM_B_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: SAM_B_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: SAM_B_PGV08 - State variable 08h, OFFSET 40, LENGTH 1
	MSG NAME: SAM_B_PGV07 - State variable 07h, OFFSET 41, LENGTH 1
	MSG NAME: SAM_B_PGV06 - State variable 06h, OFFSET 42, LENGTH 1
	MSG NAME: SAM_B_PGV05 - State variable 05h, OFFSET 43, LENGTH 1
	MSG NAME: SAM_B_PGV04 - State variable 04h, OFFSET 44, LENGTH 1
	MSG NAME: SAM_B_PGV03 - State variable 03h, OFFSET 45, LENGTH 1
	MSG NAME: SAM_B_PGV02 - State variable 02h, OFFSET 46, LENGTH 1
	MSG NAME: SAM_B_PGV01 - State variable 01h, OFFSET 47, LENGTH 1
ECU NAME: SAM_H_A1, ID: 0x0004. MSG COUNT: 51
	MSG NAME: PNK_AKT - Panic alarm is active, OFFSET 0, LENGTH 1
	MSG NAME: KL54_RM - Terminal 54 Hardware enabled, OFFSET 1, LENGTH 1
	MSG NAME: HDK_BET - down tailgate Contact, OFFSET 2, LENGTH 1
	MSG NAME: HD_AUF - Boot lid is on, OFFSET 3, LENGTH 1
	MSG NAME: THR_AUF - Rear door is right, OFFSET 4, LENGTH 1
	MSG NAME: THL_AUF - Door rear left on, OFFSET 5, LENGTH 1
	MSG NAME: TVR_AUF - Front door is right, OFFSET 6, LENGTH 1
	MSG NAME: TVL_AUF - Door front left, OFFSET 7, LENGTH 1
	MSG NAME: MOT_AUF - Bonnet is on, OFFSET 8, LENGTH 1
	MSG NAME: HHS_ST_USPG - Heizb. Rear window is switched off due to undervoltage., OFFSET 11, LENGTH 1
	MSG NAME: HHS_ST_EIN - Heated rear window is on, OFFSET 12, LENGTH 1
	MSG NAME: HSCHL_ZU - Rear lock in 90 ° position,, OFFSET 14, LENGTH 1
	MSG NAME: SAM_H_PAS - SAM / passive H, OFFSET 15, LENGTH 1
	MSG NAME: EDW_IL_EIN - Switch EDW interior light, OFFSET 16, LENGTH 1
	MSG NAME: EDW_AKT - EDW sharpened, OFFSET 17, LENGTH 1
	MSG NAME: EDW_IRS_AKT - Enable EDW interior protection, OFFSET 18, LENGTH 1
	MSG NAME: EDW_AAG_AKT - Enable EDW-trailer monitoring, OFFSET 19, LENGTH 1
	MSG NAME: EDW_ALARM - EDW alarm triggered, OFFSET 20, LENGTH 1
	MSG NAME: EDW_FT_ENT - EDW enabled driver's door open, OFFSET 21, LENGTH 1
	MSG NAME: EDW_AUTO_AKTIV - EDW self-sharpening "Belgium" active, OFFSET 22, LENGTH 1
	MSG NAME: KZL_DEF_L - Plate light left broken, OFFSET 24, LENGTH 1
	MSG NAME: RFL_DEF_L - Reversing light Left defective, OFFSET 25, LENGTH 1
	MSG NAME: BL_DEF_L - Left brake light is defective, OFFSET 26, LENGTH 1
	MSG NAME: SL_DEF_L - Bottom left defective, OFFSET 27, LENGTH 1
	MSG NAME: BLI_DEF_HL - Indicator rear left defective, OFFSET 28, LENGTH 1
	MSG NAME: NSL_DEF_L - Rear fog light left broken, OFFSET 29, LENGTH 1
	MSG NAME: BL3_DEF - 3rd brake light is defective, OFFSET 30, LENGTH 1
	MSG NAME: KL_54_DEF - Terminal 54 errors, OFFSET 31, LENGTH 1
	MSG NAME: KZL_DEF_R - Plate light right defective, OFFSET 32, LENGTH 1
	MSG NAME: RFL_DEF_R - Reversing light Right defective, OFFSET 33, LENGTH 1
	MSG NAME: BL_DEF_R - Stoplight right defective, OFFSET 34, LENGTH 1
	MSG NAME: SL_DEF_R - Bottom right defective, OFFSET 35, LENGTH 1
	MSG NAME: BLI_DEF_HR - Rear right turn signal defective, OFFSET 36, LENGTH 1
	MSG NAME: NSL_DEF_R - Rear fog light, right defective, OFFSET 37, LENGTH 1
	MSG NAME: BL_ERS_HR - Replacement light brake light, rear right, OFFSET 41, LENGTH 1
	MSG NAME: SL_ERS_HR - Replacement light tail light, rear right active, OFFSET 42, LENGTH 1
	MSG NAME: BLI_ERS_HR - Replacement light Rear right turn signal active, OFFSET 43, LENGTH 1
	MSG NAME: BL_ERS_HL - Replacement light brake light, rear left, OFFSET 45, LENGTH 1
	MSG NAME: SL_ERS_HL - Replacement light rear lights, left active, OFFSET 46, LENGTH 1
	MSG NAME: BLI_ERS_HL - Replacement light Indicator rear left active, OFFSET 47, LENGTH 1
	MSG NAME: HFS_SB_EIN - Switch HFS search lights, OFFSET 51, LENGTH 1
	MSG NAME: FS_VER_R - Rear seat locked right, OFFSET 52, LENGTH 1
	MSG NAME: FS_VER_L - locked rear seat left, OFFSET 53, LENGTH 1
	MSG NAME: FS_ENT_R - Rear seat unlocked right, OFFSET 54, LENGTH 1
	MSG NAME: FS_ENT_L - unlocked rear seat left, OFFSET 55, LENGTH 1
	MSG NAME: NSL_R_D_EIN - Turn right fog light dimmed, OFFSET 58, LENGTH 1
	MSG NAME: NSL_L_D_EIN - Switch dim fog light left, OFFSET 59, LENGTH 1
	MSG NAME: NSL_R_EIN - The rear fog light right, OFFSET 60, LENGTH 1
	MSG NAME: NSL_L_EIN - Turn left fog light, OFFSET 61, LENGTH 1
	MSG NAME: RFL_R_EIN - Switch reverse light right, OFFSET 62, LENGTH 1
	MSG NAME: RFL_L_EIN - Switch reverse light left, OFFSET 63, LENGTH 1
ECU NAME: SAM_H_A2, ID: 0x0090. MSG COUNT: 3
	MSG NAME: TANK_FS_B - (%) (%) Tank Level, OFFSET 0, LENGTH 8
	MSG NAME: TANK_GE_RE - (%) (%) Tank encoder value right, OFFSET 8, LENGTH 8
	MSG NAME: TANK_GE_LI - (%) (%) Tank timer value left, OFFSET 16, LENGTH 8
ECU NAME: SAM_H_A3, ID: 0x000E. MSG COUNT: 4
	MSG NAME: BLI_RE_EIN - Turn Right indicator, OFFSET 0, LENGTH 1
	MSG NAME: BLI_LI_EIN - Turn left turn signal, OFFSET 1, LENGTH 1
	MSG NAME: WARN_AKT - Hazard lights active, OFFSET 2, LENGTH 1
	MSG NAME: HELL_BLINK - (ms) (Ms) Flashing-light light phase, OFFSET 8, LENGTH 8
ECU NAME: SAM_H_A4, ID: 0x0041. MSG COUNT: 1
	MSG NAME: ZV_NOTOEFF - ZV Notöffnung, OFFSET 7, LENGTH 1
ECU NAME: SAM_H_A5, ID: 0x0230. MSG COUNT: 4
	MSG NAME: NSW_EIN_EDW - switch fog lights, OFFSET 0, LENGTH 1
	MSG NAME: ABL_EIN_EDW - switch on low beam, OFFSET 1, LENGTH 1
	MSG NAME: SL_EIN_EDW - Turn tail light, OFFSET 2, LENGTH 1
	MSG NAME: HELL_EDW - (ms) (Ms) continuous light light phase, OFFSET 8, LENGTH 8
ECU NAME: SAM_H_A6, ID: 0x00CC. MSG COUNT: 1
	MSG NAME: ZBC_SAM_H - Code Zugangberechtigung, OFFSET 0, LENGTH 64
ECU NAME: SAM_H_A7, ID: 0x016C. MSG COUNT: 2
	MSG NAME: TST_HFS_SCHL - Close button tailgate, OFFSET 6, LENGTH 1
	MSG NAME: TST_HFS_OEFF - Open button tailgate, OFFSET 7, LENGTH 1
ECU NAME: NM_SAM_H, ID: 0x0403. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_SAM_H, ID: 0x04E3. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_SAM_H, ID: 0x0763. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_SAM_H, ID: 0x07C3. MSG COUNT: 19
	MSG NAME: SAM_H_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: SAM_H_PGV07 - State variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: SAM_H_PGV06 - State variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: SAM_H_PGV05 - State variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: SAM_H_PGV04 - State variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: SAM_H_PGV03 - State variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: SAM_H_PGV02 - State variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: SAM_H_PGV01 - State variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: SAM_H_FM01 - Error message 01h, OFFSET 8, LENGTH 16
	MSG NAME: SAM_H_FM02 - Error message 02h, OFFSET 24, LENGTH 16
	MSG NAME: SAM_H_FM03 - Error message 03h, OFFSET 40, LENGTH 16
	MSG NAME: SAM_H_PGV0F - State variable 0Fh, OFFSET 56, LENGTH 1
	MSG NAME: SAM_H_PGV0E - State variable 0Eh, OFFSET 57, LENGTH 1
	MSG NAME: SAM_H_PGV0D - State variable 0Dh, OFFSET 58, LENGTH 1
	MSG NAME: SAM_H_PGV0C - State variable 0Ch, OFFSET 59, LENGTH 1
	MSG NAME: SAM_H_PGV0B - State variable 0Bh, OFFSET 60, LENGTH 1
	MSG NAME: SAM_H_PGV0A - State variable 0Ah, OFFSET 61, LENGTH 1
	MSG NAME: SAM_H_PGV09 - State variable 09h, OFFSET 62, LENGTH 1
	MSG NAME: SAM_H_PGV08 - State variable 08h, OFFSET 63, LENGTH 1
ECU NAME: AAG_A1, ID: 0x0130. MSG COUNT: 9
	MSG NAME: ANH_ERK - Towing recognized, OFFSET 0, LENGTH 1
	MSG NAME: AHK_NOK - not locked trailer coupling, OFFSET 1, LENGTH 1
	MSG NAME: ANHKL_54_DEF - Trailer Terminal 54 errors, OFFSET 2, LENGTH 1
	MSG NAME: EDW_ANH_ALM - EDW trailer monitoring alarm triggered, OFFSET 3, LENGTH 1
	MSG NAME: ANHSL_DEF_L - Trailer left tail light broken, OFFSET 8, LENGTH 1
	MSG NAME: ANHBLI_DEF_L - Trailer left turn signal defective, OFFSET 9, LENGTH 1
	MSG NAME: ANHBL_DEF - Trailer brake light broken, OFFSET 11, LENGTH 1
	MSG NAME: ANHSL_DEF_R - Trailer tail lamp right defective, OFFSET 12, LENGTH 1
	MSG NAME: ANHBLI_DEF_R - Trailer right turn signal defective, OFFSET 13, LENGTH 1
ECU NAME: NM_AAG, ID: 0x0410. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_AAG, ID: 0x04F0. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_AAG, ID: 0x0770. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_AAG, ID: 0x07D0. MSG COUNT: 32
	MSG NAME: AAG_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: AAG_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: AAG_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: AAG_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: AAG_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: AAG_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: AAG_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: AAG_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: AAG_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: AAG_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: AAG_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: AAG_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: AAG_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: AAG_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: AAG_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: AAG_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: AAG_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: AAG_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: AAG_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: AAG_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: AAG_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: AAG_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: AAG_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: AAG_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: AAG_PG08 - Process variable 08h, OFFSET 24, LENGTH 1
	MSG NAME: AAG_PG07 - Process variable 07h, OFFSET 25, LENGTH 1
	MSG NAME: AAG_PG06 - Process variable 06h, OFFSET 26, LENGTH 1
	MSG NAME: AAG_PG05 - Process variable 05h, OFFSET 27, LENGTH 1
	MSG NAME: AAG_PG04 - Process variable 04h, OFFSET 28, LENGTH 1
	MSG NAME: AAG_PG03 - Process variable 03h, OFFSET 29, LENGTH 1
	MSG NAME: AAG_PG02 - Process variable 02h, OFFSET 30, LENGTH 1
	MSG NAME: AAG_PG01 - Process variable 01h, OFFSET 31, LENGTH 1
ECU NAME: TVL_A1, ID: 0x028C. MSG COUNT: 31
	MSG NAME: SVL_TGL - Sitting front left - toggle, OFFSET 0, LENGTH 1
	MSG NAME: SVL_SITZ_BET - Seat left front - operated, OFFSET 1, LENGTH 1
	MSG NAME: SVL_HI_AB - Sitting front left - rear height from, OFFSET 4, LENGTH 1
	MSG NAME: SVL_HI_AUF - Sitting front left - rear height on, OFFSET 5, LENGTH 1
	MSG NAME: SVL_ZUR - Seat left front - along back, OFFSET 6, LENGTH 1
	MSG NAME: SVL_VOR - Seat left front - along ago, OFFSET 7, LENGTH 1
	MSG NAME: SVL_KST_AB - Seat left front - head restraint down, OFFSET 8, LENGTH 1
	MSG NAME: SVL_KST_AUF - Seat left front - head restraint upwards, OFFSET 9, LENGTH 1
	MSG NAME: SVL_VO_AB - Sitting front left - front height from, OFFSET 10, LENGTH 1
	MSG NAME: SVL_VO_AUF - Sitting front left - front height, OFFSET 11, LENGTH 1
	MSG NAME: SVL_LE_ZUR - Seat left front - back to back, OFFSET 12, LENGTH 1
	MSG NAME: SVL_LE_VOR - Sitting front left - back forward, OFFSET 13, LENGTH 1
	MSG NAME: LS_ZURUECK_LL - Steering column to the rear (toward the driver), OFFSET 16, LENGTH 1
	MSG NAME: LS_VOR_LL - Steering column to the front, OFFSET 17, LENGTH 1
	MSG NAME: LS_AB_LL - Steering column downward, OFFSET 18, LENGTH 1
	MSG NAME: LS_AUF_LL - Steering column according to above, OFFSET 19, LENGTH 1
	MSG NAME: MVL_TGL - Memory left front - toggle, OFFSET 24, LENGTH 1
	MSG NAME: SPI_RE_SP - Mirrors operated right memory button, OFFSET 25, LENGTH 1
	MSG NAME: MVL_P3_SP - Memory front left - save position 3, OFFSET 26, LENGTH 1
	MSG NAME: MVL_P2_SP - Memory left front - Save position 2, OFFSET 27, LENGTH 1
	MSG NAME: MVL_P1_SP - Memory front left - save position 1, OFFSET 28, LENGTH 1
	MSG NAME: MVL_P3_EN - Memory left front - taking position 3, OFFSET 29, LENGTH 1
	MSG NAME: MVL_P2_EN - Memory left front - taking position 2, OFFSET 30, LENGTH 1
	MSG NAME: MVL_P1_EN - Memory left front - occupy position 1, OFFSET 31, LENGTH 1
	MSG NAME: SPVS_BET_LL - mirror adjustment operated, OFFSET 32, LENGTH 1
	MSG NAME: SPI_RE_FAHREN - Mirrors right to drive position, OFFSET 34, LENGTH 1
	MSG NAME: SPI_RE_GARAGE - Mirrors right to Garage position, OFFSET 35, LENGTH 1
	MSG NAME: SPI_RE_N_UN - Mirrors right down, OFFSET 36, LENGTH 1
	MSG NAME: SPI_RE_N_OB - Mirrors right to top, OFFSET 37, LENGTH 1
	MSG NAME: SPI_RE_N_RE - Mirrors right to right, OFFSET 38, LENGTH 1
	MSG NAME: SPI_RE_N_LI - Mirrors right to left, OFFSET 39, LENGTH 1
ECU NAME: TVL_A2, ID: 0x0044. MSG COUNT: 19
	MSG NAME: FHR_TVL - rear window open / close right, OFFSET 8, LENGTH 1
	MSG NAME: FHL_TVL - Open windows, rear left / Close, OFFSET 9, LENGTH 1
	MSG NAME: FVR_TVL - Front windows open / close right, OFFSET 10, LENGTH 1
	MSG NAME: FVL_TVL - Open windows front left / Close, OFFSET 11, LENGTH 1
	MSG NAME: SHD_TVL - Open / close SHD / top, OFFSET 12, LENGTH 1
	MSG NAME: KB_RI_TVL - Direction touch control: open [0], close [1], OFFSET 13, LENGTH 1
	MSG NAME: KB_MOD_TVL - Touch control automatic operation [1] Manual [0], OFFSET 14, LENGTH 1
	MSG NAME: FHR_AS_LL - automatically close - window rear right, OFFSET 16, LENGTH 1
	MSG NAME: FHR_MS_LL - manually close - window rear right, OFFSET 17, LENGTH 1
	MSG NAME: FHR_MOE_LL - manually open - window rear right, OFFSET 18, LENGTH 1
	MSG NAME: FHR_AOE_LL - Automatically open - window rear right, OFFSET 19, LENGTH 1
	MSG NAME: FHL_AS_LL - Left rear windows - automatically close, OFFSET 20, LENGTH 1
	MSG NAME: FHL_MS_LL - rear left window - manually close, OFFSET 21, LENGTH 1
	MSG NAME: FHL_MOE_LL - Left rear window - manually open, OFFSET 22, LENGTH 1
	MSG NAME: FHL_AOE_LL - Left rear windows - automatically open, OFFSET 23, LENGTH 1
	MSG NAME: FVR_AS - automatically close - window front right, OFFSET 24, LENGTH 1
	MSG NAME: FVR_MS - manually close - window front right, OFFSET 25, LENGTH 1
	MSG NAME: FVR_MOE - manually open - window front right, OFFSET 26, LENGTH 1
	MSG NAME: FVR_AOE - Automatically Open - front right window, OFFSET 27, LENGTH 1
ECU NAME: TVL_A3, ID: 0x0018. MSG COUNT: 8
	MSG NAME: SPVS_BF_LL - Mirror adjustment in position right, OFFSET 0, LENGTH 1
	MSG NAME: HFE_LL - Heckdeckelfernentriegelung, OFFSET 1, LENGTH 1
	MSG NAME: KISI_EIN_LL - Parental Control, OFFSET 2, LENGTH 1
	MSG NAME: ZBLL_DEF - Additional left turn signal defective, OFFSET 3, LENGTH 1
	MSG NAME: HFS_LL - Remote boot lid closing, OFFSET 4, LENGTH 1
	MSG NAME: FVL_NORM - normalized window front left, OFFSET 8, LENGTH 1
	MSG NAME: FVL_BLOCK - blocked windows front left, OFFSET 9, LENGTH 1
	MSG NAME: FESTE_VL - (1/Ankerumdre) (1 / Ankerumdre) window position front left, OFFSET 12, LENGTH 12
ECU NAME: TVL_A4, ID: 0x00E8. MSG COUNT: 1
	MSG NAME: ZBC_TVL - Code Zugangberechtigung, OFFSET 0, LENGTH 64
ECU NAME: NM_TVL, ID: 0x0408. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_TVL, ID: 0x04E8. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_TVL, ID: 0x0768. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_TVL, ID: 0x07C8. MSG COUNT: 64
	MSG NAME: TVL_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: TVL_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: TVL_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: TVL_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: TVL_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: TVL_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: TVL_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: TVL_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: TVL_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: TVL_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: TVL_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: TVL_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: TVL_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: TVL_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: TVL_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: TVL_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: TVL_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: TVL_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: TVL_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: TVL_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: TVL_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: TVL_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: TVL_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: TVL_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: TVL_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: TVL_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: TVL_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: TVL_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: TVL_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: TVL_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: TVL_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: TVL_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: TVL_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: TVL_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: TVL_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: TVL_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: TVL_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: TVL_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: TVL_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: TVL_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: TVL_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: TVL_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: TVL_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: TVL_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: TVL_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: TVL_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: TVL_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: TVL_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: TVL_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: TVL_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: TVL_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: TVL_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: TVL_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: TVL_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: TVL_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: TVL_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: TVL_PGV04 - State variable 04h, OFFSET 56, LENGTH 1
	MSG NAME: TVL_PGV03 - State variable 03h, OFFSET 57, LENGTH 1
	MSG NAME: TVL_PGV02 - State variable 02h, OFFSET 58, LENGTH 1
	MSG NAME: TVL_PGV01 - State variable 01h, OFFSET 59, LENGTH 1
	MSG NAME: TVL_FV3B - Error vector 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: TVL_FV3A - Error vector 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: TVL_FV39 - Error vector 39h, OFFSET 62, LENGTH 1
	MSG NAME: TVL_FV38 - Error vector 38h, OFFSET 63, LENGTH 1
ECU NAME: TVR_A1, ID: 0x0290. MSG COUNT: 31
	MSG NAME: SVR_TGL - Seat front right - toggle, OFFSET 0, LENGTH 1
	MSG NAME: SVR_SITZ_BET - Seat front right - operated, OFFSET 1, LENGTH 1
	MSG NAME: SVR_HI_AB - Seat front right - rear height from, OFFSET 4, LENGTH 1
	MSG NAME: SVR_HI_AUF - Seat front right - rear height on, OFFSET 5, LENGTH 1
	MSG NAME: SVR_ZUR - Seat front right - along back, OFFSET 6, LENGTH 1
	MSG NAME: SVR_VOR - Seat front right - along ago, OFFSET 7, LENGTH 1
	MSG NAME: SVR_KST_AB - Seat front right - the head restraint down, OFFSET 8, LENGTH 1
	MSG NAME: SVR_KST_AUF - Seat front right - head restraint upwards, OFFSET 9, LENGTH 1
	MSG NAME: SVR_VO_AB - Seat front right - front height from, OFFSET 10, LENGTH 1
	MSG NAME: SVR_VO_AUF - Seat front right - front height, OFFSET 11, LENGTH 1
	MSG NAME: SVR_LE_ZUR - Seat front right - back to back, OFFSET 12, LENGTH 1
	MSG NAME: SVR_LE_VOR - Seat front right - back forward, OFFSET 13, LENGTH 1
	MSG NAME: LS_ZURUECK_RL - Steering column to the rear (toward the driver), OFFSET 16, LENGTH 1
	MSG NAME: LS_VOR_RL - Steering column to the front, OFFSET 17, LENGTH 1
	MSG NAME: LS_AB_RL - Steering column downward, OFFSET 18, LENGTH 1
	MSG NAME: LS_AUF_RL - Steering column according to above, OFFSET 19, LENGTH 1
	MSG NAME: MVR_TGL - Memory Front right - toggle, OFFSET 24, LENGTH 1
	MSG NAME: SPI_LI_SP - Exterior mirrors memory key is pressed, OFFSET 25, LENGTH 1
	MSG NAME: MVR_P3_SP - Memory front right - save position 3, OFFSET 26, LENGTH 1
	MSG NAME: MVR_P2_SP - Memory front right - save position 2, OFFSET 27, LENGTH 1
	MSG NAME: MVR_P1_SP - Memory front right - save position 1, OFFSET 28, LENGTH 1
	MSG NAME: MVR_P3_EN - Memory Front right - taking position 3, OFFSET 29, LENGTH 1
	MSG NAME: MVR_P2_EN - Memory Front right - taking position 2, OFFSET 30, LENGTH 1
	MSG NAME: MVR_P1_EN - Memory Front right - occupy position 1, OFFSET 31, LENGTH 1
	MSG NAME: SPVS_BET_RL - mirror adjustment operated, OFFSET 32, LENGTH 1
	MSG NAME: SPI_LI_FAHREN - Mirrors left to driving position, OFFSET 34, LENGTH 1
	MSG NAME: SPI_LI_GARAGE - Mirrors left to Garage position, OFFSET 35, LENGTH 1
	MSG NAME: SPI_LI_N_UN - Mirrors left to bottom, OFFSET 36, LENGTH 1
	MSG NAME: SPI_LI_N_OB - Mirrors left to top, OFFSET 37, LENGTH 1
	MSG NAME: SPI_LI_N_RE - Mirrors left to right, OFFSET 38, LENGTH 1
	MSG NAME: SPI_LI_N_LI - Exterior mirrors left, OFFSET 39, LENGTH 1
ECU NAME: TVR_A2, ID: 0x0045. MSG COUNT: 19
	MSG NAME: FHR_TVR - rear window open / close right, OFFSET 8, LENGTH 1
	MSG NAME: FHL_TVR - Open windows, rear left / Close, OFFSET 9, LENGTH 1
	MSG NAME: FVR_TVR - Front windows open / close right, OFFSET 10, LENGTH 1
	MSG NAME: FVL_TVR - Open windows front left / Close, OFFSET 11, LENGTH 1
	MSG NAME: SHD_TVR - Open / close SHD / top, OFFSET 12, LENGTH 1
	MSG NAME: KB_RI_TVR - Direction touch control: open [0], close [1], OFFSET 13, LENGTH 1
	MSG NAME: KB_MOD_TVR - Touch control automatic operation [1] Manual [0], OFFSET 14, LENGTH 1
	MSG NAME: FHR_AS_RL - automatically close - window rear right, OFFSET 16, LENGTH 1
	MSG NAME: FHR_MS_RL - manually close - window rear right, OFFSET 17, LENGTH 1
	MSG NAME: FHR_MOE_RL - manually open - window rear right, OFFSET 18, LENGTH 1
	MSG NAME: FHR_AOE_RL - Automatically open - window rear right, OFFSET 19, LENGTH 1
	MSG NAME: FHL_AS_RL - Left rear windows - automatically close, OFFSET 20, LENGTH 1
	MSG NAME: FHL_MS_RL - rear left window - manually close, OFFSET 21, LENGTH 1
	MSG NAME: FHL_MOE_RL - Left rear window - manually open, OFFSET 22, LENGTH 1
	MSG NAME: FHL_AOE_RL - Left rear windows - automatically open, OFFSET 23, LENGTH 1
	MSG NAME: FVL_AS - the left window front - automatically close, OFFSET 28, LENGTH 1
	MSG NAME: FVL_MS - the left window front - manually close, OFFSET 29, LENGTH 1
	MSG NAME: FVL_MOE - the left window front - manually open, OFFSET 30, LENGTH 1
	MSG NAME: FVL_AOE - the left window front - automatically open, OFFSET 31, LENGTH 1
ECU NAME: TVR_A3, ID: 0x0019. MSG COUNT: 8
	MSG NAME: SPVS_BF_RL - Mirror adjustment in position left, OFFSET 0, LENGTH 1
	MSG NAME: HFE_RL - Heckdeckelfernentriegelung, OFFSET 1, LENGTH 1
	MSG NAME: KISI_EIN_RL - Parental Control, OFFSET 2, LENGTH 1
	MSG NAME: ZBLR_DEF - Additional right turn signal defective, OFFSET 3, LENGTH 1
	MSG NAME: HFS_RL - Remote boot lid closing, OFFSET 4, LENGTH 1
	MSG NAME: FVR_NORM - Window normalized front right, OFFSET 8, LENGTH 1
	MSG NAME: FVR_BLOCK - Front windows blocked right, OFFSET 9, LENGTH 1
	MSG NAME: FESTE_VR - (1/Ankerumdre) (1 / Ankerumdre) Window position front right, OFFSET 12, LENGTH 12
ECU NAME: TVR_A4, ID: 0x00EC. MSG COUNT: 1
	MSG NAME: ZBC_TVR - Code Zugangberechtigung, OFFSET 0, LENGTH 64
ECU NAME: NM_TVR, ID: 0x040A. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_TVR, ID: 0x04EA. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_TVR, ID: 0x076A. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_TVR, ID: 0x07CA. MSG COUNT: 64
	MSG NAME: TVR_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: TVR_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: TVR_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: TVR_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: TVR_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: TVR_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: TVR_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: TVR_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: TVR_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: TVR_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: TVR_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: TVR_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: TVR_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: TVR_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: TVR_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: TVR_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: TVR_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: TVR_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: TVR_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: TVR_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: TVR_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: TVR_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: TVR_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: TVR_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: TVR_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: TVR_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: TVR_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: TVR_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: TVR_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: TVR_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: TVR_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: TVR_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: TVR_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: TVR_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: TVR_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: TVR_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: TVR_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: TVR_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: TVR_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: TVR_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: TVR_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: TVR_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: TVR_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: TVR_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: TVR_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: TVR_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: TVR_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: TVR_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: TVR_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: TVR_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: TVR_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: TVR_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: TVR_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: TVR_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: TVR_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: TVR_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: TVR_PGV04 - State variable 04h, OFFSET 56, LENGTH 1
	MSG NAME: TVR_PGV03 - State variable 03h, OFFSET 57, LENGTH 1
	MSG NAME: TVR_PGV02 - State variable 02h, OFFSET 58, LENGTH 1
	MSG NAME: TVR_PGV01 - State variable 01h, OFFSET 59, LENGTH 1
	MSG NAME: TVR_FV3B - Error vector 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: TVR_FV3A - Error vector 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: TVR_FV39 - Error vector 39h, OFFSET 62, LENGTH 1
	MSG NAME: TVR_FV38 - Error vector 38h, OFFSET 63, LENGTH 1
ECU NAME: THL_A1, ID: 0x009A. MSG COUNT: 3
	MSG NAME: FHL_NORM - normalized power windows, rear left, OFFSET 0, LENGTH 1
	MSG NAME: FHL_BLOCK - Rear windows blocked the left, OFFSET 1, LENGTH 1
	MSG NAME: FESTE_HL - (1/Ankerumdre) (1 / Ankerumdre) window position rear left, OFFSET 4, LENGTH 12
ECU NAME: THL_A2, ID: 0x0178. MSG COUNT: 1
	MSG NAME: SHZ_HL_NS - Sitzhzg. hinten links nächste Stufe, OFFSET 0, LENGTH 1
ECU NAME: NM_THL, ID: 0x0409. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_THL, ID: 0x04E9. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_THL, ID: 0x0769. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_THL, ID: 0x07C9. MSG COUNT: 64
	MSG NAME: THL_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: THL_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: THL_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: THL_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: THL_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: THL_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: THL_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: THL_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: THL_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: THL_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: THL_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: THL_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: THL_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: THL_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: THL_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: THL_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: THL_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: THL_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: THL_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: THL_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: THL_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: THL_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: THL_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: THL_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: THL_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: THL_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: THL_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: THL_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: THL_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: THL_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: THL_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: THL_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: THL_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: THL_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: THL_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: THL_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: THL_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: THL_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: THL_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: THL_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: THL_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: THL_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: THL_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: THL_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: THL_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: THL_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: THL_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: THL_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: THL_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: THL_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: THL_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: THL_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: THL_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: THL_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: THL_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: THL_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: THL_PGV04 - State variable 04h, OFFSET 56, LENGTH 1
	MSG NAME: THL_PGV03 - State variable 03h, OFFSET 57, LENGTH 1
	MSG NAME: THL_PGV02 - State variable 02h, OFFSET 58, LENGTH 1
	MSG NAME: THL_PGV01 - State variable 01h, OFFSET 59, LENGTH 1
	MSG NAME: THL_FV3B - Error vector 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: THL_FV3A - Error vector 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: THL_FV39 - Error vector 39h, OFFSET 62, LENGTH 1
	MSG NAME: THL_FV38 - Error vector 38h, OFFSET 63, LENGTH 1
ECU NAME: THR_A1, ID: 0x009C. MSG COUNT: 3
	MSG NAME: FHR_NORM - Windows normalized rear right, OFFSET 0, LENGTH 1
	MSG NAME: FHR_BLOCK - Rear windows blocked right, OFFSET 1, LENGTH 1
	MSG NAME: FESTE_HR - (1/Ankerumdre) (1 / Ankerumdre) Window position rear right, OFFSET 4, LENGTH 12
ECU NAME: THR_A2, ID: 0x017C. MSG COUNT: 1
	MSG NAME: SHZ_HR_NS - Sitzhzg. hinten rechts nächste Stufe, OFFSET 0, LENGTH 1
ECU NAME: NM_THR, ID: 0x040B. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_THR, ID: 0x04EB. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_THR, ID: 0x076B. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_THR, ID: 0x07CB. MSG COUNT: 64
	MSG NAME: THR_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: THR_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: THR_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: THR_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: THR_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: THR_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: THR_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: THR_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: THR_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: THR_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: THR_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: THR_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: THR_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: THR_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: THR_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: THR_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: THR_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: THR_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: THR_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: THR_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: THR_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: THR_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: THR_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: THR_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: THR_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: THR_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: THR_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: THR_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: THR_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: THR_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: THR_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: THR_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: THR_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: THR_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: THR_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: THR_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: THR_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: THR_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: THR_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: THR_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: THR_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: THR_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: THR_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: THR_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: THR_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: THR_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: THR_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: THR_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: THR_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: THR_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: THR_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: THR_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: THR_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: THR_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: THR_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: THR_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: THR_PGV04 - State variable 04h, OFFSET 56, LENGTH 1
	MSG NAME: THR_PGV03 - State variable 03h, OFFSET 57, LENGTH 1
	MSG NAME: THR_PGV02 - State variable 02h, OFFSET 58, LENGTH 1
	MSG NAME: THR_PGV01 - State variable 01h, OFFSET 59, LENGTH 1
	MSG NAME: THR_FV3B - Error vector 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: THR_FV3A - Error vector 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: THR_FV39 - Error vector 39h, OFFSET 62, LENGTH 1
	MSG NAME: THR_FV38 - Error vector 38h, OFFSET 63, LENGTH 1
ECU NAME: RWT_A1, ID: 0x0011. MSG COUNT: 25
	MSG NAME: KG_RWTAT_BET - KeylessGo rear door outer button operated, OFFSET 0, LENGTH 1
	MSG NAME: ALB_AUT_RAUS - Loading platform operated car exit, OFFSET 1, LENGTH 1
	MSG NAME: ALB_REIN - Retract charging Bode, OFFSET 2, LENGTH 1
	MSG NAME: ALB_RAUS - Loading platform operated manually exit, OFFSET 3, LENGTH 1
	MSG NAME: RWTS_ST - Status rear door lock, OFFSET 4, LENGTH 2
	MSG NAME: RW_TAG_BET - Rear outside door handle operated, OFFSET 6, LENGTH 1
	MSG NAME: RW_TIG_BET - Rear door inside handle operated, OFFSET 7, LENGTH 1
	MSG NAME: HW_INT_AKT - Rear wiper interval operation, OFFSET 8, LENGTH 1
	MSG NAME: KISI_AKT_RWT - Child safety rear door activated, OFFSET 9, LENGTH 1
	MSG NAME: SK_ANGEF - Pawl requested, OFFSET 10, LENGTH 1
	MSG NAME: ALB_AUT_REIN - Loading floor operated auto retract, OFFSET 11, LENGTH 1
	MSG NAME: HDI_SKG_RWT - Close rear lid and secure actuated, OFFSET 14, LENGTH 1
	MSG NAME: HDI_S_RWT - operated close boot lid, OFFSET 15, LENGTH 1
	MSG NAME: NSL_DEF_RWT_R - Rear fog light right defective, OFFSET 18, LENGTH 1
	MSG NAME: NSL_DEF_RWT_L - Rear fog light, left, defective, OFFSET 19, LENGTH 1
	MSG NAME: KZL_DEF_RWT_R - License plate light right defective, OFFSET 20, LENGTH 1
	MSG NAME: KZL_DEF_RWT_L - Number plate light left broken, OFFSET 21, LENGTH 1
	MSG NAME: RFL_DEF_RWT_R - Reversing light Right defective, OFFSET 22, LENGTH 1
	MSG NAME: RFL_DEF_RWT_L - Reversing light Left defective, OFFSET 23, LENGTH 1
	MSG NAME: SL_ERS_R - Replacement light tail light right, OFFSET 26, LENGTH 1
	MSG NAME: SL_ERS_L - Replacement light left tail light, OFFSET 27, LENGTH 1
	MSG NAME: BLI_HI_ERS_R - Replacement light blinker rear right, OFFSET 28, LENGTH 1
	MSG NAME: BLI_HI_ERS_L - Replacement light Indicator rear left, OFFSET 29, LENGTH 1
	MSG NAME: BL_ERS_R - Spare Stoplight right active, OFFSET 30, LENGTH 1
	MSG NAME: BL_ERS_L - Replacement Light Brake Light left active, OFFSET 31, LENGTH 1
ECU NAME: NM_RWT, ID: 0x0420. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_RWT, ID: 0x04C0. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_RWT, ID: 0x0700. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_RWT, ID: 0x07E0. MSG COUNT: 64
	MSG NAME: RWT_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: RWT_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: RWT_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: RWT_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: RWT_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: RWT_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: RWT_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: RWT_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: RWT_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: RWT_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: RWT_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: RWT_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: RWT_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: RWT_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: RWT_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: RWT_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: RWT_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: RWT_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: RWT_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: RWT_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: RWT_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: RWT_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: RWT_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: RWT_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: RWT_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: RWT_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: RWT_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: RWT_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: RWT_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: RWT_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: RWT_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: RWT_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: RWT_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: RWT_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: RWT_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: RWT_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: RWT_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: RWT_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: RWT_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: RWT_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: RWT_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: RWT_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: RWT_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: RWT_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: RWT_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: RWT_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: RWT_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: RWT_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: RWT_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: RWT_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: RWT_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: RWT_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: RWT_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: RWT_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: RWT_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: RWT_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: RWT_PGV08 - State variable 08h, OFFSET 56, LENGTH 1
	MSG NAME: RWT_PGV07 - State variable 07h, OFFSET 57, LENGTH 1
	MSG NAME: RWT_PGV06 - State variable 06h, OFFSET 58, LENGTH 1
	MSG NAME: RWT_PGV05 - State variable 05h, OFFSET 59, LENGTH 1
	MSG NAME: RWT_PGV04 - State variable 04h, OFFSET 60, LENGTH 1
	MSG NAME: RWT_PGV03 - State variable 03h, OFFSET 61, LENGTH 1
	MSG NAME: RWT_PGV02 - State variable 02h, OFFSET 62, LENGTH 1
	MSG NAME: RWT_PGV01 - State variable 01h, OFFSET 63, LENGTH 1
ECU NAME: HFS_A1, ID: 0x0078. MSG COUNT: 4
	MSG NAME: HD_ST - Status tailgate, OFFSET 0, LENGTH 3
	MSG NAME: HDI_SKG_HFS - Close rear lid and secure actuated, OFFSET 3, LENGTH 1
	MSG NAME: HDI_S_HFS - operated close boot lid, OFFSET 4, LENGTH 1
	MSG NAME: ALB_WARN - Warning cargo floor, OFFSET 7, LENGTH 1
ECU NAME: NM_HFS, ID: 0x0417. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_HFS, ID: 0x04F7. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_HFS, ID: 0x0777. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_HFS, ID: 0x07D7. MSG COUNT: 24
	MSG NAME: HFS_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: HFS_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: HFS_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: HFS_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: HFS_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: HFS_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: HFS_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: HFS_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: HFS_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: HFS_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: HFS_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: HFS_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: HFS_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: HFS_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: HFS_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: HFS_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: HFS_PGV08 - State variable 08h, OFFSET 16, LENGTH 1
	MSG NAME: HFS_PGV07 - State variable 07h, OFFSET 17, LENGTH 1
	MSG NAME: HFS_PGV06 - State variable 06h, OFFSET 18, LENGTH 1
	MSG NAME: HFS_PGV05 - State variable 05h, OFFSET 19, LENGTH 1
	MSG NAME: HFS_PGV04 - State variable 04h, OFFSET 20, LENGTH 1
	MSG NAME: HFS_PGV03 - State variable 03h, OFFSET 21, LENGTH 1
	MSG NAME: HFS_PGV02 - State variable 02h, OFFSET 22, LENGTH 1
	MSG NAME: HFS_PGV01 - State variable 01h, OFFSET 23, LENGTH 1
ECU NAME: ALB_A1, ID: 0x0171. MSG COUNT: 1
	MSG NAME: ALB_ST - Status Ladeboden, OFFSET 5, LENGTH 3
ECU NAME: NM_ALB, ID: 0x0421. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_ALB, ID: 0x04C1. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_ALB, ID: 0x0701. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_ALB, ID: 0x07E1. MSG COUNT: 64
	MSG NAME: ALB_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: ALB_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: ALB_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: ALB_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: ALB_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: ALB_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: ALB_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: ALB_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: ALB_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: ALB_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: ALB_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: ALB_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: ALB_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: ALB_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: ALB_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: ALB_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: ALB_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: ALB_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: ALB_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: ALB_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: ALB_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: ALB_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: ALB_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: ALB_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: ALB_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: ALB_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: ALB_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: ALB_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: ALB_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: ALB_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: ALB_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: ALB_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: ALB_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: ALB_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: ALB_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: ALB_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: ALB_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: ALB_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: ALB_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: ALB_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: ALB_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: ALB_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: ALB_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: ALB_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: ALB_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: ALB_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: ALB_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: ALB_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: ALB_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: ALB_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: ALB_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: ALB_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: ALB_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: ALB_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: ALB_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: ALB_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: ALB_PGV08 - State variable 08h, OFFSET 56, LENGTH 1
	MSG NAME: ALB_PGV07 - State variable 07h, OFFSET 57, LENGTH 1
	MSG NAME: ALB_PGV06 - State variable 06h, OFFSET 58, LENGTH 1
	MSG NAME: ALB_PGV05 - State variable 05h, OFFSET 59, LENGTH 1
	MSG NAME: ALB_PGV04 - State variable 04h, OFFSET 60, LENGTH 1
	MSG NAME: ALB_PGV03 - State variable 03h, OFFSET 61, LENGTH 1
	MSG NAME: ALB_PGV02 - State variable 02h, OFFSET 62, LENGTH 1
	MSG NAME: ALB_PGV01 - State variable 01h, OFFSET 63, LENGTH 1
ECU NAME: DBE_A1, ID: 0x0014. MSG COUNT: 27
	MSG NAME: AL_VL - Turn courtesy lamp front left, OFFSET 0, LENGTH 1
	MSG NAME: AL_VR - Exit light switch, front right, OFFSET 1, LENGTH 1
	MSG NAME: AL_HL - Turn courtesy lamp, rear left, OFFSET 2, LENGTH 1
	MSG NAME: AL_HR - Exit light switch, rear right, OFFSET 3, LENGTH 1
	MSG NAME: WL_VL - front warning light turn left, OFFSET 4, LENGTH 1
	MSG NAME: WL_VR - front warning light turn right, OFFSET 5, LENGTH 1
	MSG NAME: WL_HL - Warning light, rear turn left, OFFSET 6, LENGTH 1
	MSG NAME: WL_HR - Warning light, rear turn right, OFFSET 7, LENGTH 1
	MSG NAME: T_INNEN - (°C) (° C) indoor temperature, OFFSET 8, LENGTH 8
	MSG NAME: AFL_ABL_EIN - Low beam switch (request from the light sensor), OFFSET 16, LENGTH 1
	MSG NAME: NACHT - Value Light Sensor: day [0]; Night [1], OFFSET 17, LENGTH 1
	MSG NAME: LISR_DEF - Light sensor defective, OFFSET 18, LENGTH 1
	MSG NAME: TUNNEL - Light sensor: Tunnel, OFFSET 19, LENGTH 1
	MSG NAME: LADE_EIN - Switch charging light, OFFSET 27, LENGTH 1
	MSG NAME: SHD_ST - Sunroof status, OFFSET 29, LENGTH 3
	MSG NAME: IRS_ALM - Interior protection triggered, OFFSET 32, LENGTH 1
	MSG NAME: IRS_GB - triggered interior protection glass breakage, OFFSET 33, LENGTH 1
	MSG NAME: EDW_AS_ABW - deselect EDW tow-away protection, OFFSET 34, LENGTH 1
	MSG NAME: EDW_IRS_ABW - deselect EDW interior protection, OFFSET 35, LENGTH 1
	MSG NAME: EINSTIEG_R_EIN - Turn courtesy lighting right, OFFSET 36, LENGTH 1
	MSG NAME: EINSTIEG_L_EIN - Turn courtesy lighting left, OFFSET 37, LENGTH 1
	MSG NAME: IFG_LFT - Room sensor blower runs, OFFSET 39, LENGTH 1
	MSG NAME: FRBL_VL - Footwell lighting front on the left, OFFSET 52, LENGTH 1
	MSG NAME: FRBL_VR - Footwell lighting front right one, OFFSET 53, LENGTH 1
	MSG NAME: FRBL_HL - Footwell lighting behind the left, OFFSET 54, LENGTH 1
	MSG NAME: FRBL_HR - Footwell lighting, rear right one, OFFSET 55, LENGTH 1
	MSG NAME: FRBL_HELL - (%) (%) Brightness footwell lighting, OFFSET 56, LENGTH 8
ECU NAME: DBE_A2, ID: 0x0270. MSG COUNT: 8
	MSG NAME: KENN_RS - A byte code rain sensor, OFFSET 0, LENGTH 1
	MSG NAME: RS_DEF - Rain sensor defective, OFFSET 1, LENGTH 1
	MSG NAME: SCHWALL - Schwall recognition, OFFSET 3, LENGTH 1
	MSG NAME: WISCHER_ST - (Stufen) (Stages) wiper stages, OFFSET 4, LENGTH 4
	MSG NAME: RLS_UNPLAUS - Readings unavailable from RLS, OFFSET 12, LENGTH 1
	MSG NAME: SAM_V_A3_TO - Timeout for SAM_V_A3 Embassy, OFFSET 13, LENGTH 1
	MSG NAME: KOM_RLS_FEHL - Communication error to rain / light sensor, OFFSET 14, LENGTH 1
	MSG NAME: DIAG_RLS_EIN - Diagnosis rain / light sensor, a, OFFSET 15, LENGTH 1
ECU NAME: DBE_A3, ID: 0x02D4. MSG COUNT: 1
	MSG NAME: SP_ABBLEND - (Stufen) Spiegel-Abblendung, OFFSET 3, LENGTH 5
ECU NAME: DBE_A4, ID: 0x0174. MSG COUNT: 2
	MSG NAME: SHD_ZU_RS - A roof for rain, OFFSET 0, LENGTH 1
	MSG NAME: ISP_BET - Interior mirror operated, OFFSET 1, LENGTH 1
ECU NAME: NM_DBE, ID: 0x0407. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_DBE, ID: 0x04E7. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_DBE, ID: 0x0767. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_DBE, ID: 0x07C7. MSG COUNT: 19
	MSG NAME: DBE_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: DBE_PGV07 - State variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: DBE_PGV06 - State variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: DBE_PGV05 - State variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: DBE_PGV04 - State variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: DBE_PGV03 - State variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: DBE_PGV02 - State variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: DBE_PGV01 - State variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: DBE_FM01 - Error message 01h, OFFSET 8, LENGTH 16
	MSG NAME: DBE_FM02 - Error message 02h, OFFSET 24, LENGTH 16
	MSG NAME: DBE_FM03 - Error message 03h, OFFSET 40, LENGTH 16
	MSG NAME: DBE_PGV0F - State variable 0Fh, OFFSET 56, LENGTH 1
	MSG NAME: DBE_PGV0E - State variable 0Eh, OFFSET 57, LENGTH 1
	MSG NAME: DBE_PGV0D - State variable 0Dh, OFFSET 58, LENGTH 1
	MSG NAME: DBE_PGV0C - State variable 0Ch, OFFSET 59, LENGTH 1
	MSG NAME: DBE_PGV0B - State variable 0Bh, OFFSET 60, LENGTH 1
	MSG NAME: DBE_PGV0A - State variable 0Ah, OFFSET 61, LENGTH 1
	MSG NAME: DBE_PGV09 - State variable 09h, OFFSET 62, LENGTH 1
	MSG NAME: DBE_PGV08 - State variable 08h, OFFSET 63, LENGTH 1
ECU NAME: OBF_A1, ID: 0x002C. MSG COUNT: 20
	MSG NAME: ZV_VERRI_IS - ZV lock (internal switch operated), OFFSET 0, LENGTH 1
	MSG NAME: ZV_ENTRI_IS - ZV unlock (internal switch operated), OFFSET 1, LENGTH 1
	MSG NAME: HR_BET - Rear blind button actuated, OFFSET 2, LENGTH 1
	MSG NAME: FKS_BET - Headrest rear lift / lower actuated, OFFSET 4, LENGTH 1
	MSG NAME: ESP_BET - ESP button pressed, OFFSET 6, LENGTH 1
	MSG NAME: HECK_INT - Rear window Intermittent wipe, OFFSET 8, LENGTH 1
	MSG NAME: HECK_WISCH - Rear window wipe / wash, OFFSET 9, LENGTH 1
	MSG NAME: WBL_EIN - Hazard lights a, OFFSET 10, LENGTH 1
	MSG NAME: ASG_SPORT_BET - ASG Sport mode on / off operated (ST2_LED_DL when ABC available), OFFSET 12, LENGTH 1
	MSG NAME: SHZ_VR_NS - Sitzhzg. front right next level, OFFSET 16, LENGTH 1
	MSG NAME: SBL_VR_NS - Seat ventilation, front right - next level, OFFSET 17, LENGTH 1
	MSG NAME: SHZ_VL_NS - Heated front seats left - next level, OFFSET 20, LENGTH 1
	MSG NAME: SBL_VL_NS - Seat ventilation, front left - next level, OFFSET 21, LENGTH 1
	MSG NAME: SL_ST_ZU - Switch panel is closed, OFFSET 25, LENGTH 1
	MSG NAME: SL_ST_AUF - Switch panel is open, OFFSET 26, LENGTH 1
	MSG NAME: SCHLIESSEN_SL - Close sequence switch panel, OFFSET 27, LENGTH 1
	MSG NAME: OEFFNEN_SL - Open sequence switch panel, OFFSET 28, LENGTH 1
	MSG NAME: EJECT_OK - Eject and Tray Selection CD / HU released, OFFSET 29, LENGTH 1
	MSG NAME: WARN_SL_2 - Object blocks include SL, OFFSET 30, LENGTH 1
	MSG NAME: WARN_SL_1 - CDC is not free Close SL, OFFSET 31, LENGTH 1
ECU NAME: NM_OBF, ID: 0x0405. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_OBF, ID: 0x04E5. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_OBF, ID: 0x0765. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_OBF, ID: 0x07C5. MSG COUNT: 48
	MSG NAME: OBF_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: OBF_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: OBF_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: OBF_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: OBF_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: OBF_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: OBF_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: OBF_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: OBF_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: OBF_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: OBF_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: OBF_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: OBF_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: OBF_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: OBF_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: OBF_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: OBF_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: OBF_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: OBF_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: OBF_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: OBF_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: OBF_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: OBF_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: OBF_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: OBF_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: OBF_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: OBF_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: OBF_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: OBF_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: OBF_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: OBF_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: OBF_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: OBF_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: OBF_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: OBF_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: OBF_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: OBF_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: OBF_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: OBF_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: OBF_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: OBF_PGV08 - State variable 08h, OFFSET 40, LENGTH 1
	MSG NAME: OBF_PGV07 - State variable 07h, OFFSET 41, LENGTH 1
	MSG NAME: OBF_PGV06 - State variable 06h, OFFSET 42, LENGTH 1
	MSG NAME: OBF_PGV05 - State variable 05h, OFFSET 43, LENGTH 1
	MSG NAME: OBF_PGV04 - State variable 04h, OFFSET 44, LENGTH 1
	MSG NAME: OBF_PGV03 - State variable 03h, OFFSET 45, LENGTH 1
	MSG NAME: OBF_PGV02 - State variable 02h, OFFSET 46, LENGTH 1
	MSG NAME: OBF_PGV01 - State variable 01h, OFFSET 47, LENGTH 1
ECU NAME: UBF_A1, ID: 0x001A. MSG COUNT: 9
	MSG NAME: ART_ABW_BET - ART-distance warning actuated on / off, OFFSET 2, LENGTH 2
	MSG NAME: FU_FRSP_BET - Button radio override actuated, OFFSET 7, LENGTH 1
	MSG NAME: ART_ABSTAND - distance factor, OFFSET 8, LENGTH 8
	MSG NAME: PTS_BET - Button actuated parking sensors, OFFSET 16, LENGTH 1
	MSG NAME: BH_FUNK_BET - Button authorities radio operated, OFFSET 18, LENGTH 1
	MSG NAME: ST2_BET - 2-step button is pressed, OFFSET 20, LENGTH 1
	MSG NAME: ST3_BET - 3-step button is pressed, OFFSET 22, LENGTH 1
	MSG NAME: STHL_BET - Switch operated heater, OFFSET 24, LENGTH 1
	MSG NAME: LED_STH_DEF - LEDs defect for auxiliary heating, OFFSET 26, LENGTH 1
ECU NAME: NM_UBF, ID: 0x041D. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_UBF, ID: 0x04FD. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_UBF, ID: 0x077D. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_UBF, ID: 0x07DD. MSG COUNT: 48
	MSG NAME: UBF_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: UBF_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: UBF_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: UBF_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: UBF_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: UBF_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: UBF_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: UBF_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: UBF_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: UBF_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: UBF_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: UBF_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: UBF_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: UBF_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: UBF_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: UBF_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: UBF_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: UBF_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: UBF_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: UBF_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: UBF_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: UBF_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: UBF_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: UBF_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: UBF_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: UBF_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: UBF_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: UBF_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: UBF_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: UBF_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: UBF_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: UBF_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: UBF_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: UBF_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: UBF_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: UBF_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: UBF_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: UBF_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: UBF_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: UBF_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: UBF_PGV08 - State variable 08h, OFFSET 40, LENGTH 1
	MSG NAME: UBF_PGV07 - State variable 07h, OFFSET 41, LENGTH 1
	MSG NAME: UBF_PGV06 - State variable 06h, OFFSET 42, LENGTH 1
	MSG NAME: UBF_PGV05 - State variable 05h, OFFSET 43, LENGTH 1
	MSG NAME: UBF_PGV04 - State variable 04h, OFFSET 44, LENGTH 1
	MSG NAME: UBF_PGV03 - State variable 03h, OFFSET 45, LENGTH 1
	MSG NAME: UBF_PGV02 - State variable 02h, OFFSET 46, LENGTH 1
	MSG NAME: UBF_PGV01 - State variable 01h, OFFSET 47, LENGTH 1
ECU NAME: ARMADA_A1, ID: 0x0012. MSG COUNT: 22
	MSG NAME: AKSE_EIN - Switch ACFE light, OFFSET 0, LENGTH 1
	MSG NAME: AKSE_BLINK - ACFE lights blink, OFFSET 1, LENGTH 1
	MSG NAME: KONTAKT_BF - Check contact passenger seat, OFFSET 2, LENGTH 1
	MSG NAME: SRS_KL - SRS warning light switch, a [1], [0], OFFSET 4, LENGTH 1
	MSG NAME: SRS_BLINK - SRS warning lamp blink a [1], [0], OFFSET 5, LENGTH 1
	MSG NAME: SRS_WERK_FT3 - SRS message 3 "workshop", a [1], [0], OFFSET 6, LENGTH 1
	MSG NAME: SRS_WERK_FT1 - SRS message "workshop" a [1], [0], OFFSET 7, LENGTH 1
	MSG NAME: RAST_SITZ_BF - Check seat latch passenger, OFFSET 10, LENGTH 1
	MSG NAME: KISI_ST - Status child seat, OFFSET 13, LENGTH 3
	MSG NAME: GS_BF - buckle passenger, OFFSET 16, LENGTH 2
	MSG NAME: PSG_DETEC_FAST - Passenger detection almost, OFFSET 19, LENGTH 2
	MSG NAME: OC_BF - Occupant classification passenger, OFFSET 21, LENGTH 3
	MSG NAME: GS_F - buckle driver, OFFSET 24, LENGTH 2
	MSG NAME: OC_F - Occupant classification riders, OFFSET 29, LENGTH 3
	MSG NAME: GS_SHM - SHM buckle (reserved), OFFSET 32, LENGTH 2
	MSG NAME: ISOFIX_BF - Isofix switch passenger (only Roadster), OFFSET 34, LENGTH 2
	MSG NAME: GS_SHR - SHR buckle (reserved), OFFSET 36, LENGTH 2
	MSG NAME: GS_SHL - SHL buckle (reserved), OFFSET 38, LENGTH 2
	MSG NAME: RAST_SHR - Check seat latch HR, OFFSET 44, LENGTH 1
	MSG NAME: RAST_SHL - Check seat latch HL, OFFSET 45, LENGTH 1
	MSG NAME: KONT_HI_RE - Check contacting seat HI RE, OFFSET 46, LENGTH 1
	MSG NAME: KONT_HI_LI - Check contacting seat HI LI, OFFSET 47, LENGTH 1
ECU NAME: ARMADA_A2, ID: 0x0040. MSG COUNT: 16
	MSG NAME: CONF_CRASH - Confirm bit for all crash events toggelnd, OFFSET 0, LENGTH 1
	MSG NAME: CRASH_G - Rollover event 1, OFFSET 1, LENGTH 1
	MSG NAME: CRASH_F - Frontal Event 2, OFFSET 2, LENGTH 1
	MSG NAME: CRASH_E - Heck Event 2, OFFSET 3, LENGTH 1
	MSG NAME: CRASH_D - Page Event 1, OFFSET 4, LENGTH 1
	MSG NAME: CRASH_C - Frontal Event 5, OFFSET 5, LENGTH 1
	MSG NAME: CRASH_B - Heck Event 1, OFFSET 6, LENGTH 1
	MSG NAME: CRASH_A - Frontal Event 1, OFFSET 7, LENGTH 1
	MSG NAME: X_CRASH - Any crash event available, OFFSET 8, LENGTH 1
	MSG NAME: CRASH_O - event tbd, OFFSET 9, LENGTH 1
	MSG NAME: CRASH_N - event tbd, OFFSET 10, LENGTH 1
	MSG NAME: CRASH_M - event tbd, OFFSET 11, LENGTH 1
	MSG NAME: CRASH_L - Page Event 2, OFFSET 12, LENGTH 1
	MSG NAME: CRASH_K - Heck Event 3, OFFSET 13, LENGTH 1
	MSG NAME: CRASH_I - Rollover event 3, OFFSET 14, LENGTH 1
	MSG NAME: CRASH_H - Rollover event 2, OFFSET 15, LENGTH 1
ECU NAME: NM_ARMADA, ID: 0x041C. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_ARMADA, ID: 0x04FC. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_ARMADA, ID: 0x077C. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_ARMADA, ID: 0x07DC. MSG COUNT: 19
	MSG NAME: ARMADA_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: ARMADA_PGV07 - State variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: ARMADA_PGV06 - State variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: ARMADA_PGV05 - State variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: ARMADA_PGV04 - State variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: ARMADA_PGV03 - State variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: ARMADA_PGV02 - State variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: ARMADA_PGV01 - State variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: ARMADA_FM01 - Error message 01h, OFFSET 8, LENGTH 16
	MSG NAME: ARMADA_FM02 - Error message 02h, OFFSET 24, LENGTH 16
	MSG NAME: ARMADA_FM03 - Error message 03h, OFFSET 40, LENGTH 16
	MSG NAME: ARMADA_PGV0F - State variable 0Fh, OFFSET 56, LENGTH 1
	MSG NAME: ARMADA_PGV0E - State variable 0Eh, OFFSET 57, LENGTH 1
	MSG NAME: ARMADA_PGV0D - State variable 0Dh, OFFSET 58, LENGTH 1
	MSG NAME: ARMADA_PGV0C - State variable 0Ch, OFFSET 59, LENGTH 1
	MSG NAME: ARMADA_PGV0B - State variable 0Bh, OFFSET 60, LENGTH 1
	MSG NAME: ARMADA_PGV0A - State variable 0Ah, OFFSET 61, LENGTH 1
	MSG NAME: ARMADA_PGV09 - State variable 09h, OFFSET 62, LENGTH 1
	MSG NAME: ARMADA_PGV08 - State variable 08h, OFFSET 63, LENGTH 1
ECU NAME: WSS_A1, ID: 0x02A4. MSG COUNT: 4
	MSG NAME: PSG_DETECT_FAST - Passenger Detection Fast, OFFSET 2, LENGTH 2
	MSG NAME: WSS_PSG_FAULT - Weight classification passenger fault, OFFSET 4, LENGTH 1
	MSG NAME: WSS_PSG - Weight classification passenger, OFFSET 5, LENGTH 3
	MSG NAME: WSS_ID - WSS Identification, OFFSET 16, LENGTH 8
ECU NAME: NM_WSS, ID: 0x0426. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_WSS, ID: 0x04C6. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_WSS, ID: 0x0706. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_WSS, ID: 0x07E6. MSG COUNT: 64
	MSG NAME: WSS_RES - RReserviert for vector format marking BR211, OFFSET 0, LENGTH 1
	MSG NAME: WSS_PG07 - Process variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: WSS_PG06 - Process variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: WSS_PG05 - Process variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: WSS_PG04 - Process variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: WSS_PG03 - Process variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: WSS_PG02 - Process variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: WSS_PG01 - Process variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: WSS_PG0F - Process variable 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: WSS_PG0E - Process variable 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: WSS_PG0D - Process variable 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: WSS_PG0C - Process variable 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: WSS_PG0B - Process variable 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: WSS_PG0A - Process variable 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: WSS_PG09 - Process variable 09h, OFFSET 14, LENGTH 1
	MSG NAME: WSS_PG08 - Process variable 08h, OFFSET 15, LENGTH 1
	MSG NAME: WSS_PG17 - Process variable 17h, OFFSET 16, LENGTH 1
	MSG NAME: WSS_PG16 - Process variable 16h, OFFSET 17, LENGTH 1
	MSG NAME: WSS_PG15 - Process variable 15h, OFFSET 18, LENGTH 1
	MSG NAME: WSS_PG14 - Process variable 14h, OFFSET 19, LENGTH 1
	MSG NAME: WSS_PG13 - Process variable 13h, OFFSET 20, LENGTH 1
	MSG NAME: WSS_PG12 - Process variable 12h, OFFSET 21, LENGTH 1
	MSG NAME: WSS_PG11 - Process variable 11h, OFFSET 22, LENGTH 1
	MSG NAME: WSS_PG10 - Process variable 10h, OFFSET 23, LENGTH 1
	MSG NAME: WSS_PG1F - Process variable 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: WSS_PG1E - Process variable 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: WSS_PG1D - Process variable 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: WSS_PG1C - Process variable 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: WSS_PG1B - Process variable 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: WSS_PG1A - Process variable 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: WSS_PG19 - Process variable 19h, OFFSET 30, LENGTH 1
	MSG NAME: WSS_PG18 - Process variable 18h, OFFSET 31, LENGTH 1
	MSG NAME: WSS_PG27 - Process variable 27h, OFFSET 32, LENGTH 1
	MSG NAME: WSS_PG26 - Process variable 26h, OFFSET 33, LENGTH 1
	MSG NAME: WSS_PG25 - Process variable 25h, OFFSET 34, LENGTH 1
	MSG NAME: WSS_PG24 - Process variable 24, OFFSET 35, LENGTH 1
	MSG NAME: WSS_PG23 - Process variable 23h, OFFSET 36, LENGTH 1
	MSG NAME: WSS_PG22 - Process variable 22h, OFFSET 37, LENGTH 1
	MSG NAME: WSS_PG21 - Process variable 21h, OFFSET 38, LENGTH 1
	MSG NAME: WSS_PG20 - Process variable 20h, OFFSET 39, LENGTH 1
	MSG NAME: WSS_PG2F - Process variable 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: WSS_PG2E - Process variable 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: WSS_PG2D - Process variable 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: WSS_PG2C - Process variable 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: WSS_PG2B - Process variable 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: WSS_PG2A - Process variable 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: WSS_PG29 - Process variable 29h, OFFSET 46, LENGTH 1
	MSG NAME: WSS_PG28 - Process variable 28h, OFFSET 47, LENGTH 1
	MSG NAME: WSS_PG37 - Process variable 37h, OFFSET 48, LENGTH 1
	MSG NAME: WSS_PG36 - Process variable 36h, OFFSET 49, LENGTH 1
	MSG NAME: WSS_PG35 - Process variable 35h, OFFSET 50, LENGTH 1
	MSG NAME: WSS_PG34 - Process variable 34h, OFFSET 51, LENGTH 1
	MSG NAME: WSS_PG33 - Process variable 33h, OFFSET 52, LENGTH 1
	MSG NAME: WSS_PG32 - Process variable 32h, OFFSET 53, LENGTH 1
	MSG NAME: WSS_PG31 - Process variable 31h, OFFSET 54, LENGTH 1
	MSG NAME: WSS_PG30 - Process variable 30h, OFFSET 55, LENGTH 1
	MSG NAME: WSS_PG3F - Process variable 3Fh, OFFSET 56, LENGTH 1
	MSG NAME: WSS_PG3E - Process variable 3Eh, OFFSET 57, LENGTH 1
	MSG NAME: WSS_PG3D - Process variable 3Dh, OFFSET 58, LENGTH 1
	MSG NAME: WSS_PG3C - Process variable 3Ch, OFFSET 59, LENGTH 1
	MSG NAME: WSS_PG3B - Process variable 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: WSS_PG3A - Process variable 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: WSS_PG39 - Process variable 39h, OFFSET 62, LENGTH 1
	MSG NAME: WSS_PG38 - Process variable 38h, OFFSET 63, LENGTH 1
ECU NAME: SF_A1, ID: 0x01AC. MSG COUNT: 6
	MSG NAME: LE_F_ENT - Back seat driver unlocked, OFFSET 4, LENGTH 1
	MSG NAME: SF_POS_LV - (Abschnitte) (Sections) driver seat position longitudinal adjustment, OFFSET 8, LENGTH 8
	MSG NAME: SF_POS_HV - (Abschnitte) (Sections) driver seat position height adjustment, OFFSET 16, LENGTH 8
	MSG NAME: SF_POS_L - (Abschnitte) (Sections) driver seat position recliner, OFFSET 24, LENGTH 8
	MSG NAME: SF_POS_NV - (Abschnitte) (Sections) Fahrersitzpostion recline, OFFSET 32, LENGTH 8
	MSG NAME: SF_POS_K - (Abschnitte) (Sections) driver seat position headrest adjustment, OFFSET 40, LENGTH 8
ECU NAME: SF_A2, ID: 0x02D0. MSG COUNT: 13
	MSG NAME: ESH_AKT - Entry / exit is approaching a position actively, OFFSET 0, LENGTH 1
	MSG NAME: AUTO_AKT - Driving position to approach active, OFFSET 1, LENGTH 1
	MSG NAME: MF_MAN_SP - save manually set position, OFFSET 2, LENGTH 1
	MSG NAME: MF_MAN_ISP_SP - save manually set interior mirror position, OFFSET 3, LENGTH 1
	MSG NAME: ESH_AUTO_ISP - Positioning perform interior mirror, OFFSET 4, LENGTH 1
	MSG NAME: ESH_AUTO_REST - perform positioning mirror, OFFSET 5, LENGTH 1
	MSG NAME: MF_BET - Memory key driver operates, OFFSET 9, LENGTH 1
	MSG NAME: MF_P3_SP - Store Position 3 - Memory driver, OFFSET 10, LENGTH 1
	MSG NAME: MF_P2_SP - Save position 2 - Memory driver, OFFSET 11, LENGTH 1
	MSG NAME: MF_P1_SP - Save position 1 - Memory driver, OFFSET 12, LENGTH 1
	MSG NAME: MF_P3_EN - occupy position 3 - Memory driver, OFFSET 13, LENGTH 1
	MSG NAME: MF_P2_EN - taking position 2 - Memory driver, OFFSET 14, LENGTH 1
	MSG NAME: MF_P1_EN - occupy position 1 - Memory driver, OFFSET 15, LENGTH 1
ECU NAME: NM_SF, ID: 0x040C. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_SF, ID: 0x04EC. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_SF, ID: 0x076C. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_SF, ID: 0x07CC. MSG COUNT: 64
	MSG NAME: SF_RES - Reserved for vector format marking BR211, OFFSET 0, LENGTH 1
	MSG NAME: SF_PG07 - Process variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: SF_PG06 - Process variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: SF_PG05 - Process variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: SF_PG04 - Process variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: SF_PG03 - Process variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: SF_PG02 - Process variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: SF_PG01 - Process variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: SF_PG0F - Process variable 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: SF_PG0E - Process variable 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: SF_PG0D - Process variable 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: SF_PG0C - Process variable 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: SF_PG0B - Process variable 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: SF_PG0A - Process variable 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: SF_PG09 - Process variable 09h, OFFSET 14, LENGTH 1
	MSG NAME: SF_PG08 - Process variable 08h, OFFSET 15, LENGTH 1
	MSG NAME: SF_PG17 - Process variable 17h, OFFSET 16, LENGTH 1
	MSG NAME: SF_PG16 - Process variable 16h, OFFSET 17, LENGTH 1
	MSG NAME: SF_PG15 - Process variable 15h, OFFSET 18, LENGTH 1
	MSG NAME: SF_PG14 - Process variable 14h, OFFSET 19, LENGTH 1
	MSG NAME: SF_PG13 - Process variable 13h, OFFSET 20, LENGTH 1
	MSG NAME: SF_PG12 - Process variable 12h, OFFSET 21, LENGTH 1
	MSG NAME: SF_PG11 - Process variable 11h, OFFSET 22, LENGTH 1
	MSG NAME: SF_PG10 - Process variable 10h, OFFSET 23, LENGTH 1
	MSG NAME: SF_PG1F - Process variable 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: SF_PG1E - Process variable 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: SF_PG1D - Process variable 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: SF_PG1C - Process variable 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: SF_PG1B - Process variable 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: SF_PG1A - Process variable 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: SF_PG19 - Process variable 19h, OFFSET 30, LENGTH 1
	MSG NAME: SF_PG18 - Process variable 18h, OFFSET 31, LENGTH 1
	MSG NAME: SF_PG27 - Process variable 27h, OFFSET 32, LENGTH 1
	MSG NAME: SF_PG26 - Process variable 26h, OFFSET 33, LENGTH 1
	MSG NAME: SF_PG25 - Process variable 25h, OFFSET 34, LENGTH 1
	MSG NAME: SF_PG24 - Process variable 24, OFFSET 35, LENGTH 1
	MSG NAME: SF_PG23 - Process variable 23h, OFFSET 36, LENGTH 1
	MSG NAME: SF_PG22 - Process variable 22h, OFFSET 37, LENGTH 1
	MSG NAME: SF_PG21 - Process variable 21h, OFFSET 38, LENGTH 1
	MSG NAME: SF_PG20 - Process variable 20h, OFFSET 39, LENGTH 1
	MSG NAME: SF_PG2F - Process variable 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: SF_PG2E - Process variable 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: SF_PG2D - Process variable 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: SF_PG2C - Process variable 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: SF_PG2B - Process variable 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: SF_PG2A - Process variable 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: SF_PG29 - Process variable 29h, OFFSET 46, LENGTH 1
	MSG NAME: SF_PG28 - Process variable 28h, OFFSET 47, LENGTH 1
	MSG NAME: SF_PG37 - Process variable 37h, OFFSET 48, LENGTH 1
	MSG NAME: SF_PG36 - Process variable 36h, OFFSET 49, LENGTH 1
	MSG NAME: SF_PG35 - Process variable 35h, OFFSET 50, LENGTH 1
	MSG NAME: SF_PG34 - Process variable 34h, OFFSET 51, LENGTH 1
	MSG NAME: SF_PG33 - Process variable 33h, OFFSET 52, LENGTH 1
	MSG NAME: SF_PG32 - Process variable 32h, OFFSET 53, LENGTH 1
	MSG NAME: SF_PG31 - Process variable 31h, OFFSET 54, LENGTH 1
	MSG NAME: SF_PG30 - Process variable 30h, OFFSET 55, LENGTH 1
	MSG NAME: SF_PG3F - Process variable 3Fh, OFFSET 56, LENGTH 1
	MSG NAME: SF_PG3E - Process variable 3Eh, OFFSET 57, LENGTH 1
	MSG NAME: SF_PG3D - Process variable 3Dh, OFFSET 58, LENGTH 1
	MSG NAME: SF_PG3C - Process variable 3Ch, OFFSET 59, LENGTH 1
	MSG NAME: SF_PG3B - Process variable 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: SF_PG3A - Process variable 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: SF_PG39 - Process variable 39h, OFFSET 62, LENGTH 1
	MSG NAME: SF_PG38 - Process variable 38h, OFFSET 63, LENGTH 1
ECU NAME: SB_A1, ID: 0x01B6. MSG COUNT: 6
	MSG NAME: LE_B_ENT - Back passenger seat unlocked, OFFSET 4, LENGTH 1
	MSG NAME: SB_POS_LV - (Abschnitte) (Sections) passenger seat position longitudinal adjustment, OFFSET 8, LENGTH 8
	MSG NAME: SB_POS_HV - (Abschnitte) (Sections) passenger seat height adjustment position, OFFSET 16, LENGTH 8
	MSG NAME: SB_POS_L - (Abschnitte) (Sections) passenger seat position recliner, OFFSET 24, LENGTH 8
	MSG NAME: SB_POS_NV - (Abschnitte) (Sections) Beifahrersitzpostion recline, OFFSET 32, LENGTH 8
	MSG NAME: SB_POS_K - (Abschnitte) (Sections) passenger seat position headrest adjustment, OFFSET 40, LENGTH 8
ECU NAME: SB_A2, ID: 0x02B1. MSG COUNT: 7
	MSG NAME: MB_BET - Memory key actuated passenger, OFFSET 9, LENGTH 1
	MSG NAME: MB_P3_SP - Store Position 3 - Memory passenger, OFFSET 10, LENGTH 1
	MSG NAME: MB_P2_SP - Save position 2 - Memory passenger, OFFSET 11, LENGTH 1
	MSG NAME: MB_P1_SP - Save position 1 - Memory passenger, OFFSET 12, LENGTH 1
	MSG NAME: MB_P3_EN - occupy position 3 - Memory passenger, OFFSET 13, LENGTH 1
	MSG NAME: MB_P2_EN - taking position 2 - Memory passenger, OFFSET 14, LENGTH 1
	MSG NAME: MB_P1_EN - occupy position 1 - Memory passenger, OFFSET 15, LENGTH 1
ECU NAME: NM_SB, ID: 0x040D. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_SB, ID: 0x04ED. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_SB, ID: 0x076D. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_SB, ID: 0x07CD. MSG COUNT: 64
	MSG NAME: SB_RES - Reserved for vector format marking BR211, OFFSET 0, LENGTH 1
	MSG NAME: SB_PG07 - Process variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: SB_PG06 - Process variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: SB_PG05 - Process variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: SB_PG04 - Process variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: SB_PG03 - Process variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: SB_PG02 - Process variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: SB_PG01 - Process variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: SB_PG0F - Process variable 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: SB_PG0E - Process variable 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: SB_PG0D - Process variable 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: SB_PG0C - Process variable 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: SB_PG0B - Process variable 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: SB_PG0A - Process variable 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: SB_PG09 - Process variable 09h, OFFSET 14, LENGTH 1
	MSG NAME: SB_PG08 - Process variable 08h, OFFSET 15, LENGTH 1
	MSG NAME: SB_PG17 - Process variable 17h, OFFSET 16, LENGTH 1
	MSG NAME: SB_PG16 - Process variable 16h, OFFSET 17, LENGTH 1
	MSG NAME: SB_PG15 - Process variable 15h, OFFSET 18, LENGTH 1
	MSG NAME: SB_PG14 - Process variable 14h, OFFSET 19, LENGTH 1
	MSG NAME: SB_PG13 - Process variable 13h, OFFSET 20, LENGTH 1
	MSG NAME: SB_PG12 - Process variable 12h, OFFSET 21, LENGTH 1
	MSG NAME: SB_PG11 - Process variable 11h, OFFSET 22, LENGTH 1
	MSG NAME: SB_PG10 - Process variable 10h, OFFSET 23, LENGTH 1
	MSG NAME: SB_PG1F - Process variable 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: SB_PG1E - Process variable 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: SB_PG1D - Process variable 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: SB_PG1C - Process variable 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: SB_PG1B - Process variable 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: SB_PG1A - Process variable 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: SB_PG19 - Process variable 19h, OFFSET 30, LENGTH 1
	MSG NAME: SB_PG18 - Process variable 18h, OFFSET 31, LENGTH 1
	MSG NAME: SB_PG27 - Process variable 27h, OFFSET 32, LENGTH 1
	MSG NAME: SB_PG26 - Process variable 26h, OFFSET 33, LENGTH 1
	MSG NAME: SB_PG25 - Process variable 25h, OFFSET 34, LENGTH 1
	MSG NAME: SB_PG24 - Process variable 24, OFFSET 35, LENGTH 1
	MSG NAME: SB_PG23 - Process variable 23h, OFFSET 36, LENGTH 1
	MSG NAME: SB_PG22 - Process variable 22h, OFFSET 37, LENGTH 1
	MSG NAME: SB_PG21 - Process variable 21h, OFFSET 38, LENGTH 1
	MSG NAME: SB_PG20 - Process variable 20h, OFFSET 39, LENGTH 1
	MSG NAME: SB_PG2F - Process variable 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: SB_PG2E - Process variable 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: SB_PG2D - Process variable 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: SB_PG2C - Process variable 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: SB_PG2B - Process variable 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: SB_PG2A - Process variable 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: SB_PG29 - Process variable 29h, OFFSET 46, LENGTH 1
	MSG NAME: SB_PG28 - Process variable 28h, OFFSET 47, LENGTH 1
	MSG NAME: SB_PG37 - Process variable 37h, OFFSET 48, LENGTH 1
	MSG NAME: SB_PG36 - Process variable 36h, OFFSET 49, LENGTH 1
	MSG NAME: SB_PG35 - Process variable 35h, OFFSET 50, LENGTH 1
	MSG NAME: SB_PG34 - Process variable 34h, OFFSET 51, LENGTH 1
	MSG NAME: SB_PG33 - Process variable 33h, OFFSET 52, LENGTH 1
	MSG NAME: SB_PG32 - Process variable 32h, OFFSET 53, LENGTH 1
	MSG NAME: SB_PG31 - Process variable 31h, OFFSET 54, LENGTH 1
	MSG NAME: SB_PG30 - Process variable 30h, OFFSET 55, LENGTH 1
	MSG NAME: SB_PG3F - Process variable 3Fh, OFFSET 56, LENGTH 1
	MSG NAME: SB_PG3E - Process variable 3Eh, OFFSET 57, LENGTH 1
	MSG NAME: SB_PG3D - Process variable 3Dh, OFFSET 58, LENGTH 1
	MSG NAME: SB_PG3C - Process variable 3Ch, OFFSET 59, LENGTH 1
	MSG NAME: SB_PG3B - Process variable 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: SB_PG3A - Process variable 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: SB_PG39 - Process variable 39h, OFFSET 62, LENGTH 1
	MSG NAME: SB_PG38 - Process variable 38h, OFFSET 63, LENGTH 1
ECU NAME: PFDS_A1, ID: 0x02A8. MSG COUNT: 5
	MSG NAME: PFDS_DEAKT - Pump FDS disabled, OFFSET 3, LENGTH 1
	MSG NAME: PFDS_ENT - Pressure vessel vent, OFFSET 4, LENGTH 1
	MSG NAME: PFDS_OVLD - Overload warning, OFFSET 5, LENGTH 1
	MSG NAME: PFDSMOT_ST - Status FDS-pump motor, OFFSET 6, LENGTH 2
	MSG NAME: P_PFDS - (hPa) (HPa) supply pressure FDS pump, OFFSET 11, LENGTH 5
ECU NAME: NM_PFDS, ID: 0x040E. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_PFDS, ID: 0x04EE. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_PFDS, ID: 0x076E. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_PFDS, ID: 0x07CE. MSG COUNT: 24
	MSG NAME: PFDS_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: PFDS_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: PFDS_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: PFDS_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: PFDS_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: PFDS_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: PFDS_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: PFDS_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: PFDS_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: PFDS_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: PFDS_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: PFDS_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: PFDS_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: PFDS_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: PFDS_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: PFDS_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: PFDS_PGV08 - State variable 08h, OFFSET 16, LENGTH 1
	MSG NAME: PFDS_PGV07 - State variable 07h, OFFSET 17, LENGTH 1
	MSG NAME: PFDS_PGV06 - State variable 06h, OFFSET 18, LENGTH 1
	MSG NAME: PFDS_PGV05 - State variable 05h, OFFSET 19, LENGTH 1
	MSG NAME: PFDS_PGV04 - State variable 04h, OFFSET 20, LENGTH 1
	MSG NAME: PFDS_PGV03 - State variable 03h, OFFSET 21, LENGTH 1
	MSG NAME: PFDS_PGV02 - State variable 02h, OFFSET 22, LENGTH 1
	MSG NAME: PFDS_PGV01 - State variable 01h, OFFSET 23, LENGTH 1
ECU NAME: FDSVL_A1, ID: 0x032C. MSG COUNT: 5
	MSG NAME: FDS_AKT_VL - Dynamic driving seat adjustment active, OFFSET 0, LENGTH 1
	MSG NAME: MITT_AKT_VL - Dynamic Lordosenstützenverstellung active, OFFSET 1, LENGTH 1
	MSG NAME: SEIT_AKT_VL - Side support adjustment active, OFFSET 2, LENGTH 1
	MSG NAME: FDSVL_STAT - FDSVL status, OFFSET 4, LENGTH 2
	MSG NAME: PFDS_ANF_VL - Request FDS pump, OFFSET 6, LENGTH 2
ECU NAME: NM_FDSVL, ID: 0x041E. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_FDSVL, ID: 0x04FE. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_FDSVL, ID: 0x077E. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_FDSVL, ID: 0x07DE. MSG COUNT: 40
	MSG NAME: FDSVL_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: FDSVL_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: FDSVL_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: FDSVL_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: FDSVL_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: FDSVL_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: FDSVL_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: FDSVL_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: FDSVL_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: FDSVL_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: FDSVL_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: FDSVL_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: FDSVL_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: FDSVL_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: FDSVL_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: FDSVL_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: FDSVL_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: FDSVL_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: FDSVL_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: FDSVL_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: FDSVL_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: FDSVL_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: FDSVL_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: FDSVL_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: FDSVL_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: FDSVL_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: FDSVL_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: FDSVL_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: FDSVL_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: FDSVL_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: FDSVL_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: FDSVL_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: FDSVL_PGV08 - State variable 08h, OFFSET 32, LENGTH 1
	MSG NAME: FDSVL_PGV07 - State variable 07h, OFFSET 33, LENGTH 1
	MSG NAME: FDSVL_PGV06 - State variable 06h, OFFSET 34, LENGTH 1
	MSG NAME: FDSVL_PGV05 - State variable 05h, OFFSET 35, LENGTH 1
	MSG NAME: FDSVL_PGV04 - State variable 04h, OFFSET 36, LENGTH 1
	MSG NAME: FDSVL_PGV03 - State variable 03h, OFFSET 37, LENGTH 1
	MSG NAME: FDSVL_PGV02 - State variable 02h, OFFSET 38, LENGTH 1
	MSG NAME: FDSVL_PGV01 - State variable 01h, OFFSET 39, LENGTH 1
ECU NAME: FDSVR_A1, ID: 0x032D. MSG COUNT: 5
	MSG NAME: FDS_AKT_VR - Dynamic driving seat adjustment active, OFFSET 0, LENGTH 1
	MSG NAME: MITT_AKT_VR - Dynamic Lordosenstützenverstellung active, OFFSET 1, LENGTH 1
	MSG NAME: SEIT_AKT_VR - Side support adjustment active, OFFSET 2, LENGTH 1
	MSG NAME: FDSVR_STAT - FDSVR status, OFFSET 4, LENGTH 2
	MSG NAME: PFDS_ANF_VR - Request FDS pump, OFFSET 6, LENGTH 2
ECU NAME: NM_FDSVR, ID: 0x041F. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_FDSVR, ID: 0x04FF. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_FDSVR, ID: 0x077F. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_FDSVR, ID: 0x07DF. MSG COUNT: 40
	MSG NAME: FDSVR_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: FDSVR_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: FDSVR_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: FDSVR_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: FDSVR_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: FDSVR_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: FDSVR_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: FDSVR_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: FDSVR_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: FDSVR_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: FDSVR_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: FDSVR_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: FDSVR_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: FDSVR_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: FDSVR_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: FDSVR_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: FDSVR_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: FDSVR_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: FDSVR_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: FDSVR_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: FDSVR_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: FDSVR_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: FDSVR_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: FDSVR_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: FDSVR_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: FDSVR_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: FDSVR_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: FDSVR_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: FDSVR_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: FDSVR_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: FDSVR_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: FDSVR_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: FDSVR_PGV08 - State variable 08h, OFFSET 32, LENGTH 1
	MSG NAME: FDSVR_PGV07 - State variable 07h, OFFSET 33, LENGTH 1
	MSG NAME: FDSVR_PGV06 - State variable 06h, OFFSET 34, LENGTH 1
	MSG NAME: FDSVR_PGV05 - State variable 05h, OFFSET 35, LENGTH 1
	MSG NAME: FDSVR_PGV04 - State variable 04h, OFFSET 36, LENGTH 1
	MSG NAME: FDSVR_PGV03 - State variable 03h, OFFSET 37, LENGTH 1
	MSG NAME: FDSVR_PGV02 - State variable 02h, OFFSET 38, LENGTH 1
	MSG NAME: FDSVR_PGV01 - State variable 01h, OFFSET 39, LENGTH 1
ECU NAME: SHZ_A1, ID: 0x0210. MSG COUNT: 10
	MSG NAME: SHB_VL_USPG - Sitzheizg./-belüftg. wg off. UnderVoltage., OFFSET 0, LENGTH 1
	MSG NAME: SH_VL_ST - Status Heated front left, OFFSET 3, LENGTH 2
	MSG NAME: SBLFT_VL_ST - Status seat ventilation, front left, OFFSET 6, LENGTH 2
	MSG NAME: SHB_VR_USPG - Sitzheizg./-belüftg. wg off. UnderVoltage., OFFSET 8, LENGTH 1
	MSG NAME: SH_VR_ST - Status Heated front right, OFFSET 11, LENGTH 2
	MSG NAME: SBLFT_VR_ST - Status seat ventilation, front right, OFFSET 14, LENGTH 2
	MSG NAME: SH_HL_USPG - Sitzheizg. wg off. UnderVoltage., OFFSET 16, LENGTH 1
	MSG NAME: SH_HL_ST - Status Seat heating, rear left, OFFSET 19, LENGTH 2
	MSG NAME: SH_HR_USPG - Sitzheizg. wg off. UnderVoltage., OFFSET 24, LENGTH 1
	MSG NAME: SH_HR_ST - Status Seat heating, rear right, OFFSET 27, LENGTH 2
ECU NAME: NM_SHZ, ID: 0x041B. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_SHZ, ID: 0x04FB. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_SHZ, ID: 0x077B. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_SHZ, ID: 0x07DB. MSG COUNT: 64
	MSG NAME: SHZ_RES - Reserved for vector format Flag BR 211, OFFSET 0, LENGTH 1
	MSG NAME: SHZ_PG07 - Process variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: SHZ_PG06 - Process variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: SHZ_PG05 - Process variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: SHZ_PG04 - Process variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: SHZ_PG03 - Process variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: SHZ_PG02 - Process variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: SHZ_PG01 - Process variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: SHZ_PG0F - Process variable 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: SHZ_PG0E - Process variable 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: SHZ_PG0D - Process variable 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: SHZ_PG0C - Process variable 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: SHZ_PG0B - Process variable 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: SHZ_PG0A - Process variable 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: SHZ_PG09 - Process variable 09h, OFFSET 14, LENGTH 1
	MSG NAME: SHZ_PG08 - Process variable 08h, OFFSET 15, LENGTH 1
	MSG NAME: SHZ_PG17 - Process variable 17h, OFFSET 16, LENGTH 1
	MSG NAME: SHZ_PG16 - Process variable 16h, OFFSET 17, LENGTH 1
	MSG NAME: SHZ_PG15 - Process variable 15h, OFFSET 18, LENGTH 1
	MSG NAME: SHZ_PG14 - Process variable 14h, OFFSET 19, LENGTH 1
	MSG NAME: SHZ_PG13 - Process variable 13h, OFFSET 20, LENGTH 1
	MSG NAME: SHZ_PG12 - Process variable 12h, OFFSET 21, LENGTH 1
	MSG NAME: SHZ_PG11 - Process variable 11h, OFFSET 22, LENGTH 1
	MSG NAME: SHZ_PG10 - Process variable 10h, OFFSET 23, LENGTH 1
	MSG NAME: SHZ_PG1F - Process variable 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: SHZ_PG1E - Process variable 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: SHZ_PG1D - Process variable 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: SHZ_PG1C - Process variable 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: SHZ_PG1B - Process variable 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: SHZ_PG1A - Process variable 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: SHZ_PG19 - Process variable 19h, OFFSET 30, LENGTH 1
	MSG NAME: SHZ_PG18 - Process variable 18h, OFFSET 31, LENGTH 1
	MSG NAME: SHZ_PG27 - Process variable 27h, OFFSET 32, LENGTH 1
	MSG NAME: SHZ_PG26 - Process variable 26h, OFFSET 33, LENGTH 1
	MSG NAME: SHZ_PG25 - Process variable 25h, OFFSET 34, LENGTH 1
	MSG NAME: SHZ_PG24 - Process variable 24, OFFSET 35, LENGTH 1
	MSG NAME: SHZ_PG23 - Process variable 23h, OFFSET 36, LENGTH 1
	MSG NAME: SHZ_PG22 - Process variable 22h, OFFSET 37, LENGTH 1
	MSG NAME: SHZ_PG21 - Process variable 21h, OFFSET 38, LENGTH 1
	MSG NAME: SHZ_PG20 - Process variable 20h, OFFSET 39, LENGTH 1
	MSG NAME: SHZ_PG2F - Process variable 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: SHZ_PG2E - Process variable 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: SHZ_PG2D - Process variable 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: SHZ_PG2C - Process variable 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: SHZ_PG2B - Process variable 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: SHZ_PG2A - Process variable 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: SHZ_PG29 - Process variable 29h, OFFSET 46, LENGTH 1
	MSG NAME: SHZ_PG28 - Process variable 28h, OFFSET 47, LENGTH 1
	MSG NAME: SHZ_PG37 - Process variable 37h, OFFSET 48, LENGTH 1
	MSG NAME: SHZ_PG36 - Process variable 36h, OFFSET 49, LENGTH 1
	MSG NAME: SHZ_PG35 - Process variable 35h, OFFSET 50, LENGTH 1
	MSG NAME: SHZ_PG34 - Process variable 34h, OFFSET 51, LENGTH 1
	MSG NAME: SHZ_PG33 - Process variable 33h, OFFSET 52, LENGTH 1
	MSG NAME: SHZ_PG32 - Process variable 32h, OFFSET 53, LENGTH 1
	MSG NAME: SHZ_PG31 - Process variable 31h, OFFSET 54, LENGTH 1
	MSG NAME: SHZ_PG30 - Process variable 30h, OFFSET 55, LENGTH 1
	MSG NAME: SHZ_PG3F - Process variable 3Fh, OFFSET 56, LENGTH 1
	MSG NAME: SHZ_PG3E - Process variable 3Eh, OFFSET 57, LENGTH 1
	MSG NAME: SHZ_PG3D - Process variable 3Dh, OFFSET 58, LENGTH 1
	MSG NAME: SHZ_PG3C - Process variable 3Ch, OFFSET 59, LENGTH 1
	MSG NAME: SHZ_PG3B - Process variable 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: SHZ_PG3A - Process variable 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: SHZ_PG39 - Process variable 39h, OFFSET 62, LENGTH 1
	MSG NAME: SHZ_PG38 - Process variable 38h, OFFSET 63, LENGTH 1
ECU NAME: STH_A1, ID: 0x0094. MSG COUNT: 5
	MSG NAME: STHL_EIN - / Off auxiliary heating independent ventilation, OFFSET 0, LENGTH 1
	MSG NAME: STHL_AUS - / Off auxiliary heater vent, OFFSET 1, LENGTH 1
	MSG NAME: GEBLAESE_EIN - Switch Vehicle fan, OFFSET 4, LENGTH 1
	MSG NAME: VWZ_MENUE - Open code-time menu, OFFSET 5, LENGTH 1
	MSG NAME: SENDLM_EIN - Broadcast programming, a, OFFSET 6, LENGTH 1
ECU NAME: STH_A2, ID: 0x0390. MSG COUNT: 1
	MSG NAME: T_WASSERAUST - (°C) Wasseraustrittstemperatur am Heizgerät, OFFSET 0, LENGTH 8
ECU NAME: NM_STH, ID: 0x0419. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_STH, ID: 0x04F9. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_STH, ID: 0x0779. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_STH, ID: 0x07D9. MSG COUNT: 64
	MSG NAME: STH_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: STH_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: STH_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: STH_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: STH_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: STH_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: STH_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: STH_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: STH_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: STH_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: STH_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: STH_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: STH_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: STH_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: STH_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: STH_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: STH_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: STH_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: STH_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: STH_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: STH_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: STH_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: STH_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: STH_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: STH_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: STH_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: STH_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: STH_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: STH_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: STH_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: STH_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: STH_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: STH_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: STH_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: STH_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: STH_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: STH_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: STH_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: STH_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: STH_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: STH_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: STH_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: STH_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: STH_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: STH_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: STH_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: STH_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: STH_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: STH_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: STH_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: STH_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: STH_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: STH_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: STH_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: STH_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: STH_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: STH_PGV08 - State variable 08h, OFFSET 56, LENGTH 1
	MSG NAME: STH_PGV07 - State variable 07h, OFFSET 57, LENGTH 1
	MSG NAME: STH_PGV06 - State variable 06h, OFFSET 58, LENGTH 1
	MSG NAME: STH_PGV05 - State variable 05h, OFFSET 59, LENGTH 1
	MSG NAME: STH_PGV04 - State variable 04h, OFFSET 60, LENGTH 1
	MSG NAME: STH_PGV03 - State variable 03h, OFFSET 61, LENGTH 1
	MSG NAME: STH_PGV02 - State variable 02h, OFFSET 62, LENGTH 1
	MSG NAME: STH_PGV01 - State variable 01h, OFFSET 63, LENGTH 1
ECU NAME: KLA_A1, ID: 0x0030. MSG COUNT: 22
	MSG NAME: HHS_EIN - Switch on heated rear window, OFFSET 0, LENGTH 1
	MSG NAME: EC_AKT - EC mode active, OFFSET 1, LENGTH 1
	MSG NAME: IFG_EIN - Switch internal sensor Fan, OFFSET 2, LENGTH 1
	MSG NAME: ZWP_EIN - Switch on auxiliary water pump, OFFSET 3, LENGTH 1
	MSG NAME: ZH_EIN_OK - Heater switch allows, OFFSET 4, LENGTH 1
	MSG NAME: LL_DZA - Idle speed increase for the cooling capacity increase, OFFSET 5, LENGTH 1
	MSG NAME: HEIZEN - heating heater, OFFSET 6, LENGTH 1
	MSG NAME: LUEFTEN - Heater vent, OFFSET 7, LENGTH 1
	MSG NAME: NLFTS - (%) (%) Motor fan setpoint speed, OFFSET 8, LENGTH 8
	MSG NAME: M_KOMP - (Nm) (Nm) torque absorption chiller, OFFSET 16, LENGTH 8
	MSG NAME: KOMP_STELL - (%) (%) Refrigeration compressor control signal, OFFSET 24, LENGTH 8
	MSG NAME: DEFROST_AKT - defrost active, OFFSET 33, LENGTH 1
	MSG NAME: REST_AKT - Residual heat mode active, OFFSET 34, LENGTH 1
	MSG NAME: KJAL_ZU - Close radiator shutter, OFFSET 35, LENGTH 1
	MSG NAME: ABVENT_W_ZU - Shutoff valve connect heat exchangers, OFFSET 36, LENGTH 1
	MSG NAME: ZH_ANF - (Stufen) (Stages) request Zuheizleistung, OFFSET 37, LENGTH 3
	MSG NAME: GEB_LSTG - (%) (%) Fan power, OFFSET 40, LENGTH 8
	MSG NAME: UL_AKT_KLA - convection active, OFFSET 48, LENGTH 1
	MSG NAME: LKO_VORN - Position ventilation flap above, OFFSET 50, LENGTH 2
	MSG NAME: LKM_VORN - Position ventilation flap center, OFFSET 52, LENGTH 2
	MSG NAME: LKU_VORN - Position ventilation flap down, OFFSET 54, LENGTH 2
	MSG NAME: T_INNEN_KLA - (°C) (° C) indoor temperature, OFFSET 56, LENGTH 8
ECU NAME: KLA_A2, ID: 0x0250. MSG COUNT: 7
	MSG NAME: FHR_KLA - rear window open / close right, OFFSET 0, LENGTH 1
	MSG NAME: FHL_KLA - Open windows, rear left / Close, OFFSET 1, LENGTH 1
	MSG NAME: FVR_KLA - Front windows open / close right, OFFSET 2, LENGTH 1
	MSG NAME: FVL_KLA - Open windows front left / Close, OFFSET 3, LENGTH 1
	MSG NAME: SHD_KLA - Open / close SHD / top, OFFSET 4, LENGTH 1
	MSG NAME: KB_RI_KLA - Direction touch control: open [0], close [1], OFFSET 5, LENGTH 1
	MSG NAME: KB_MOD_KLA - Touch control automatic operation [1] Manual [0], OFFSET 6, LENGTH 1
ECU NAME: KLA_A3, ID: 0x02D8. MSG COUNT: 1
	MSG NAME: T_TAU - (°C) Taupunkttemperatur, OFFSET 0, LENGTH 8
ECU NAME: KLA_A5, ID: 0x00F1. MSG COUNT: 2
	MSG NAME: HZL_ANF - (%) (%) Heating power requirement, OFFSET 0, LENGTH 8
	MSG NAME: T_AUSSEN_WM - (°C) (° C) Outside air temperature for heat management, OFFSET 8, LENGTH 8
ECU NAME: NM_KLA, ID: 0x0411. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_KLA, ID: 0x04F1. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_KLA, ID: 0x0771. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_KLA, ID: 0x07D1. MSG COUNT: 19
	MSG NAME: KLA_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: KLA_PGV07 - State variable 07h, OFFSET 1, LENGTH 1
	MSG NAME: KLA_PGV06 - State variable 06h, OFFSET 2, LENGTH 1
	MSG NAME: KLA_PGV05 - State variable 05h, OFFSET 3, LENGTH 1
	MSG NAME: KLA_PGV04 - State variable 04h, OFFSET 4, LENGTH 1
	MSG NAME: KLA_PGV03 - State variable 03h, OFFSET 5, LENGTH 1
	MSG NAME: KLA_PGV02 - State variable 02h, OFFSET 6, LENGTH 1
	MSG NAME: KLA_PGV01 - State variable 01h, OFFSET 7, LENGTH 1
	MSG NAME: KLA_FM01 - Error message 01h, OFFSET 8, LENGTH 16
	MSG NAME: KLA_FM02 - Error message 02h, OFFSET 24, LENGTH 16
	MSG NAME: KLA_FM03 - Error message 03h, OFFSET 40, LENGTH 16
	MSG NAME: KLA_PGV0F - State variable 0Fh, OFFSET 56, LENGTH 1
	MSG NAME: KLA_PGV0E - State variable 0Eh, OFFSET 57, LENGTH 1
	MSG NAME: KLA_PGV0D - State variable 0Dh, OFFSET 58, LENGTH 1
	MSG NAME: KLA_PGV0C - State variable 0Ch, OFFSET 59, LENGTH 1
	MSG NAME: KLA_PGV0B - State variable 0Bh, OFFSET 60, LENGTH 1
	MSG NAME: KLA_PGV0A - State variable 0Ah, OFFSET 61, LENGTH 1
	MSG NAME: KLA_PGV09 - State variable 09h, OFFSET 62, LENGTH 1
	MSG NAME: KLA_PGV08 - State variable 08h, OFFSET 63, LENGTH 1
ECU NAME: BSG_A1, ID: 0x0009. MSG COUNT: 13
	MSG NAME: BN_NTLF - Wiring emergency: Prio1- and Prio2-consumers, Second battery supports, OFFSET 0, LENGTH 1
	MSG NAME: BN_NTLF_P1 - Wiring emergency: Prio1-consumers, OFFSET 1, LENGTH 1
	MSG NAME: BN_NTLF_P2 - Wiring emergency: Prio2-consumers, OFFSET 2, LENGTH 1
	MSG NAME: BN_WARN4 - Wiring Warning: Starterltg. Interrupt. or fuse Starterbatt. malfunction, OFFSET 4, LENGTH 1
	MSG NAME: BN_WARN3 - Wiring Warning: defective BSG / current sensor or relay K2 defective, OFFSET 5, LENGTH 1
	MSG NAME: BN_WARN2 - Wiring Warning: emergency (Prio1- or Prio2-felony charge of.), OFFSET 6, LENGTH 1
	MSG NAME: BN_WARN1 - Wiring Warning: emergency (.. Prio1- & 2 felony charge of, Second Batt supports), OFFSET 7, LENGTH 1
	MSG NAME: BN_KL61 - Battery is not charged, OFFSET 8, LENGTH 1
	MSG NAME: SOHS_B - battery old, OFFSET 11, LENGTH 1
	MSG NAME: SOCS_B - partially discharged battery, OFFSET 13, LENGTH 1
	MSG NAME: SOCS_START - start Availability, OFFSET 14, LENGTH 1
	MSG NAME: HHS_BSG - Control heated rear window, OFFSET 16, LENGTH 2
	MSG NAME: BSG_AKT - Battery SG active, OFFSET 23, LENGTH 1
ECU NAME: BSG_A2, ID: 0x00A0. MSG COUNT: 1
	MSG NAME: BACKUP_CP - Batterie Backup für CP, OFFSET 1, LENGTH 3
ECU NAME: NM_BSG, ID: 0x0412. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_BSG, ID: 0x04F2. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_BSG, ID: 0x0772. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_BSG, ID: 0x07D2. MSG COUNT: 40
	MSG NAME: BSG_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: BSG_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: BSG_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: BSG_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: BSG_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: BSG_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: BSG_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: BSG_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: BSG_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: BSG_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: BSG_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: BSG_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: BSG_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: BSG_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: BSG_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: BSG_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: BSG_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: BSG_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: BSG_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: BSG_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: BSG_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: BSG_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: BSG_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: BSG_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: BSG_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: BSG_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: BSG_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: BSG_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: BSG_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: BSG_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: BSG_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: BSG_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: BSG_PGV08 - State variable 08h, OFFSET 32, LENGTH 1
	MSG NAME: BSG_PGV07 - State variable 07h, OFFSET 33, LENGTH 1
	MSG NAME: BSG_PGV06 - State variable 06h, OFFSET 34, LENGTH 1
	MSG NAME: BSG_PGV05 - State variable 05h, OFFSET 35, LENGTH 1
	MSG NAME: BSG_PGV04 - State variable 04h, OFFSET 36, LENGTH 1
	MSG NAME: BSG_PGV03 - State variable 03h, OFFSET 37, LENGTH 1
	MSG NAME: BSG_PGV02 - State variable 02h, OFFSET 38, LENGTH 1
	MSG NAME: BSG_PGV01 - State variable 01h, OFFSET 39, LENGTH 1
ECU NAME: MSS_A1, ID: 0x0015. MSG COUNT: 19
	MSG NAME: FL_EIN_MSS - Turn on high beams, OFFSET 0, LENGTH 1
	MSG NAME: NSW_EIN_MSS - switch fog lights, OFFSET 1, LENGTH 1
	MSG NAME: SGH_EIN_MSS - Switch Bugle, OFFSET 2, LENGTH 1
	MSG NAME: BLI_EIN_MSS - MSS flashing on, OFFSET 3, LENGTH 1
	MSG NAME: T_HIRU_EIN - Taxi call for help settle, OFFSET 4, LENGTH 1
	MSG NAME: UMLUFT_MSS - close air recirculation flap, OFFSET 5, LENGTH 1
	MSG NAME: IL_EIN_MSS - Switch interior light, OFFSET 6, LENGTH 1
	MSG NAME: ZV_ZU_MSS - close Central, OFFSET 7, LENGTH 1
	MSG NAME: BLI_HELL_MSS - (ms) (Ms) Duration Indicator light phase, OFFSET 8, LENGTH 8
	MSG NAME: SGH_AN_MSS - (ms) (Ms) duration of Hupens, OFFSET 16, LENGTH 8
	MSG NAME: NSW_HELL_MSS - (ms) (Ms) duration fog lamp light phase, OFFSET 24, LENGTH 8
	MSG NAME: FL_HELL_MSS - (ms) (Ms) duration high-beam light phase, OFFSET 32, LENGTH 8
	MSG NAME: FU_FRSP_AKT - Radio override active, OFFSET 40, LENGTH 1
	MSG NAME: BHF_LED_AKT - Switch LED Radio Communications, OFFSET 42, LENGTH 1
	MSG NAME: ANF_ZT - Request numeric keypad HU, OFFSET 43, LENGTH 1
	MSG NAME: LADEN_AKT - 220V external load is connected, OFFSET 44, LENGTH 1
	MSG NAME: AUDIO_MUTE2 - Muting the audio source for radio reception, OFFSET 45, LENGTH 1
	MSG NAME: AUDIO_MUTE1 - Audio Mute, OFFSET 46, LENGTH 1
	MSG NAME: SIR_EIN_MSS - turn siren, OFFSET 47, LENGTH 1
ECU NAME: MSS_A2, ID: 0x01AE. MSG COUNT: 13
	MSG NAME: DZ_KL - Roof sign warning light a, OFFSET 0, LENGTH 1
	MSG NAME: DZ_LA_DEF - Roof sign lamp defect, OFFSET 1, LENGTH 1
	MSG NAME: DZ_PRF - Check roof sign (interruption), OFFSET 2, LENGTH 1
	MSG NAME: DZ_DEF - Roof sign defective (short circuit), OFFSET 3, LENGTH 1
	MSG NAME: MSS_USPG - MSS detects undervoltage, OFFSET 4, LENGTH 1
	MSG NAME: MSS_ALM - Silent alarm triggered, OFFSET 5, LENGTH 1
	MSG NAME: NOTALM_DEF - Emergency alarm system is defective, OFFSET 6, LENGTH 1
	MSG NAME: MSS_EE_DEF - Electrical on MSS defective, OFFSET 7, LENGTH 1
	MSG NAME: FNK_STAT - A radio status [1] [0], OFFSET 8, LENGTH 1
	MSG NAME: MSS_SUMMER - Summer drive in combination, OFFSET 9, LENGTH 1
	MSG NAME: MSS_USPG_MO - MSS detects under-voltage when the engine is running, OFFSET 21, LENGTH 1
	MSG NAME: FSB_FEHLER - Windshield Hzg. malfunction, OFFSET 22, LENGTH 1
	MSG NAME: FSB_HZG_AUS - Windshield Hzg. From wg. timer, OFFSET 23, LENGTH 1
ECU NAME: MSS_A3, ID: 0x01CE. MSG COUNT: 2
	MSG NAME: DEST_LAT - (ms) (Ms) GPS Latitude, South = [-]; North = [+], OFFSET 0, LENGTH 32
	MSG NAME: DEST_LONG - (ms) (Ms) GPS Longitude, West = [-]; East = [+], OFFSET 32, LENGTH 32
ECU NAME: MSS_A4, ID: 0x0248. MSG COUNT: 7
	MSG NAME: FHR_ALARM - Close rear right, OFFSET 0, LENGTH 1
	MSG NAME: FHL_ALARM - Close rear left, OFFSET 1, LENGTH 1
	MSG NAME: FVR_ALARM - Close window front right, OFFSET 2, LENGTH 1
	MSG NAME: FVL_ALARM - Close front left, OFFSET 3, LENGTH 1
	MSG NAME: SHD_ALARM - close SHD, OFFSET 4, LENGTH 1
	MSG NAME: RI_ALARM - Direction Alarmbetätigg .: Open [0], close [1], OFFSET 5, LENGTH 1
	MSG NAME: MOD_ALARM - Automatic operation [1] Manual [0], OFFSET 6, LENGTH 1
ECU NAME: MSSK_A1, ID: 0x0046. MSG COUNT: 21
	MSG NAME: SGH_EIN_K - Switch Bugle, OFFSET 0, LENGTH 1
	MSG NAME: LHP_EIN_K - turn flasher, OFFSET 1, LENGTH 1
	MSG NAME: FL_EIN_K - Turn on high beams, OFFSET 2, LENGTH 1
	MSG NAME: BLI_RE_K - Directional blinking right, OFFSET 3, LENGTH 1
	MSG NAME: BLI_LI_K - Directional blinking left, OFFSET 4, LENGTH 1
	MSG NAME: SCH_WI_2_K - switch on the windscreen level 2, OFFSET 8, LENGTH 1
	MSG NAME: SCH_WI_1_K - switch on the windscreen level 1, OFFSET 9, LENGTH 1
	MSG NAME: SCH_WI_INT_K - Turn wiper interval, OFFSET 10, LENGTH 1
	MSG NAME: WASCHEN_K - turn wash, OFFSET 11, LENGTH 1
	MSG NAME: TIPP_WISCH_K - Switch Brief wipe, OFFSET 12, LENGTH 1
	MSG NAME: HECK_INT_K - Rear window Intermittent wipe, OFFSET 16, LENGTH 1
	MSG NAME: HECK_WISCH_K - Rear window wipe / wash, OFFSET 17, LENGTH 1
	MSG NAME: WBL_EIN_K - Hazard lights a, OFFSET 18, LENGTH 1
	MSG NAME: STL_EIN_K - Switch on parking lights, OFFSET 19, LENGTH 1
	MSG NAME: ABL_EIN_K - switch on low beam, OFFSET 20, LENGTH 1
	MSG NAME: NSW_EIN_K - switch fog lights, OFFSET 21, LENGTH 1
	MSG NAME: NSL_EIN_K - Switch rear fog light, OFFSET 22, LENGTH 1
	MSG NAME: SHD_STOP - sunroof stop, OFFSET 24, LENGTH 1
	MSG NAME: HD_AUF_K - open Hubdach, OFFSET 25, LENGTH 1
	MSG NAME: SHD_ZU_K - sunroof close, OFFSET 26, LENGTH 1
	MSG NAME: SHD_AUF_K - open sunroof, OFFSET 27, LENGTH 1
ECU NAME: MSSK_A2, ID: 0x0208. MSG COUNT: 3
	MSG NAME: SBF_K_TGL - Passenger seat - toggle, OFFSET 0, LENGTH 1
	MSG NAME: SBF_ZUR_K - Passenger seat - back along, OFFSET 6, LENGTH 1
	MSG NAME: SBF_VOR_K - Passenger seat - along ago, OFFSET 7, LENGTH 1
ECU NAME: TP_MSS_AGW3, ID: 0x01D8. MSG COUNT: 1
	MSG NAME: TP_MSS_AGW3 - Kommunikation vom MSS zum AGW, OFFSET 0, LENGTH 64
ECU NAME: TP_MSS_KOMBI2, ID: 0x01A6. MSG COUNT: 1
	MSG NAME: TP_MSS_KOMBI - Kommunikation vom MSS zum KOMBI, OFFSET 0, LENGTH 64
ECU NAME: NM_MSS, ID: 0x0406. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MSS, ID: 0x04E6. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_MSS, ID: 0x0766. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_MSS, ID: 0x07C6. MSG COUNT: 64
	MSG NAME: MSS_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: MSS_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: MSS_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: MSS_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: MSS_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: MSS_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: MSS_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: MSS_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: MSS_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: MSS_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: MSS_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: MSS_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: MSS_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: MSS_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: MSS_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: MSS_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: MSS_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: MSS_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: MSS_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: MSS_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: MSS_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: MSS_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: MSS_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: MSS_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: MSS_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: MSS_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: MSS_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: MSS_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: MSS_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: MSS_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: MSS_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: MSS_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: MSS_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: MSS_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: MSS_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: MSS_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: MSS_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: MSS_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: MSS_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: MSS_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: MSS_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: MSS_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: MSS_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: MSS_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: MSS_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: MSS_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: MSS_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: MSS_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: MSS_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: MSS_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: MSS_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: MSS_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: MSS_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: MSS_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: MSS_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: MSS_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: MSS_PGV04 - State variable 04h, OFFSET 56, LENGTH 1
	MSG NAME: MSS_PGV03 - State variable 03h, OFFSET 57, LENGTH 1
	MSG NAME: MSS_PGV02 - State variable 02h, OFFSET 58, LENGTH 1
	MSG NAME: MSS_PGV01 - State variable 01h, OFFSET 59, LENGTH 1
	MSG NAME: MSS_FV3B - Error vector 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: MSS_FV3A - Error vector 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: MSS_FV39 - Error vector 39h, OFFSET 62, LENGTH 1
	MSG NAME: MSS_FV38 - Error vector 38h, OFFSET 63, LENGTH 1
ECU NAME: PTS_A1, ID: 0x02B0. MSG COUNT: 1
	MSG NAME: PTS_ST_AUS - PTS ist komplett ausgeschaltet, OFFSET 0, LENGTH 1
ECU NAME: PTS_A2, ID: 0x020E. MSG COUNT: 1
	MSG NAME: P_PTS - PTS warnt, OFFSET 7, LENGTH 1
ECU NAME: NM_PTS, ID: 0x0413. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_PTS, ID: 0x04F3. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_PTS, ID: 0x0773. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_PTS, ID: 0x07D3. MSG COUNT: 64
	MSG NAME: PTS_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: PTS_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: PTS_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: PTS_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: PTS_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: PTS_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: PTS_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: PTS_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: PTS_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: PTS_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: PTS_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: PTS_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: PTS_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: PTS_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: PTS_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: PTS_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: PTS_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: PTS_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: PTS_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: PTS_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: PTS_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: PTS_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: PTS_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: PTS_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: PTS_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: PTS_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: PTS_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: PTS_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: PTS_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: PTS_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: PTS_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: PTS_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: PTS_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: PTS_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: PTS_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: PTS_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: PTS_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: PTS_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: PTS_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: PTS_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: PTS_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: PTS_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: PTS_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: PTS_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: PTS_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: PTS_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: PTS_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: PTS_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: PTS_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: PTS_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: PTS_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: PTS_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: PTS_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: PTS_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: PTS_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: PTS_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: PTS_PGV04 - State variable 04h, OFFSET 56, LENGTH 1
	MSG NAME: PTS_PGV03 - State variable 03h, OFFSET 57, LENGTH 1
	MSG NAME: PTS_PGV02 - State variable 02h, OFFSET 58, LENGTH 1
	MSG NAME: PTS_PGV01 - State variable 01h, OFFSET 59, LENGTH 1
	MSG NAME: PTS_FV3B - Error vector 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: PTS_FV3A - Error vector 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: PTS_FV39 - Error vector 39h, OFFSET 62, LENGTH 1
	MSG NAME: PTS_FV38 - Error vector 38h, OFFSET 63, LENGTH 1
ECU NAME: RDK_A1, ID: 0x0198. MSG COUNT: 20
	MSG NAME: SERVICE - service, OFFSET 0, LENGTH 1
	MSG NAME: RDK_INI - uninitialized tire pressure monitoring system, OFFSET 1, LENGTH 1
	MSG NAME: P_VERL_S - Rapid pressure loss, OFFSET 2, LENGTH 1
	MSG NAME: P_MIN - minimum pressure, OFFSET 3, LENGTH 1
	MSG NAME: P_VERL_L - Slow pressure loss, OFFSET 4, LENGTH 1
	MSG NAME: VBZ - Load state / speed, OFFSET 5, LENGTH 1
	MSG NAME: S_UE - Jammer / overheating, OFFSET 6, LENGTH 1
	MSG NAME: WARNFARBE - Warning color (red [1] / Yellow [0]), OFFSET 7, LENGTH 1
	MSG NAME: RDK_OFF - RDK disabled, OFFSET 8, LENGTH 1
	MSG NAME: RR - spare, OFFSET 10, LENGTH 1
	MSG NAME: RHR - Right rear tire, OFFSET 11, LENGTH 1
	MSG NAME: RHL - Rear tires on the left, OFFSET 12, LENGTH 1
	MSG NAME: RVR - front tire right, OFFSET 13, LENGTH 1
	MSG NAME: RVL - front left tire, OFFSET 14, LENGTH 1
	MSG NAME: MITPOS - See tire positions, OFFSET 15, LENGTH 1
	MSG NAME: P_RVL - (bar) (Bar) tire pressure front left, OFFSET 16, LENGTH 8
	MSG NAME: P_RVR - (bar) (Bar) tire pressure front right, OFFSET 24, LENGTH 8
	MSG NAME: P_RHL - (bar) (Bar) tire pressure left rear, OFFSET 32, LENGTH 8
	MSG NAME: P_RHR - (bar) (Bar) Rear tire pressure right, OFFSET 40, LENGTH 8
	MSG NAME: P_RR - (bar) (Bar) tire pressure spare tire, OFFSET 48, LENGTH 8
ECU NAME: NM_RDK, ID: 0x0418. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_RDK, ID: 0x04F8. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_RDK, ID: 0x0778. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_RDK, ID: 0x07D8. MSG COUNT: 64
	MSG NAME: RDK_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: RDK_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: RDK_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: RDK_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: RDK_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: RDK_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: RDK_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: RDK_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: RDK_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: RDK_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: RDK_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: RDK_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: RDK_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: RDK_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: RDK_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: RDK_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: RDK_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: RDK_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: RDK_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: RDK_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: RDK_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: RDK_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: RDK_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: RDK_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: RDK_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: RDK_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: RDK_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: RDK_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: RDK_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: RDK_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: RDK_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: RDK_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: RDK_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: RDK_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: RDK_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: RDK_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: RDK_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: RDK_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: RDK_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: RDK_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: RDK_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: RDK_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: RDK_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: RDK_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: RDK_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: RDK_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: RDK_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: RDK_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: RDK_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: RDK_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: RDK_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: RDK_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: RDK_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: RDK_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: RDK_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: RDK_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: RDK_PGV01 - State variable 01h, OFFSET 56, LENGTH 1
	MSG NAME: RDK_FV3E - Error vector 3Eh, OFFSET 57, LENGTH 1
	MSG NAME: RDK_FV3D - Error vector 3Dh, OFFSET 58, LENGTH 1
	MSG NAME: RDK_FV3C - Error vector 3Ch, OFFSET 59, LENGTH 1
	MSG NAME: RDK_FV3B - Error vector 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: RDK_FV3A - Error vector 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: RDK_FV39 - Error vector 39h, OFFSET 62, LENGTH 1
	MSG NAME: RDK_FV38 - Error vector 38h, OFFSET 63, LENGTH 1
ECU NAME: AGW_A1, ID: 0x0034. MSG COUNT: 7
	MSG NAME: WARN_SL_HU - HU is unable to provide release for opening, OFFSET 0, LENGTH 1
	MSG NAME: WARN_SL_CDC - CDC can not grant approval for Close, OFFSET 1, LENGTH 1
	MSG NAME: AUF_OK_HU - open allowed, OFFSET 2, LENGTH 1
	MSG NAME: ZU_OK_CDC - Close allowed, OFFSET 3, LENGTH 1
	MSG NAME: EJECT_CDC - Switch panel closed to CDC, OFFSET 4, LENGTH 1
	MSG NAME: EJECT_HU - Switch panel blocked for HU, OFFSET 5, LENGTH 1
	MSG NAME: SBS_AKT - Voice control system active, OFFSET 8, LENGTH 1
ECU NAME: AGW_A2, ID: 0x020A. MSG COUNT: 1
	MSG NAME: P_AGW - Prioritäten am AGW, OFFSET 5, LENGTH 3
ECU NAME: AGW_A3, ID: 0x0138. MSG COUNT: 6
	MSG NAME: CANCEL_HU - Rejection of numeric input HU, OFFSET 1, LENGTH 1
	MSG NAME: STERN_HU - Star key operated, OFFSET 2, LENGTH 1
	MSG NAME: RAUTE_HU - Argyle key is pressed, OFFSET 3, LENGTH 1
	MSG NAME: ZIFFER_HU - Keypad Head Unit, OFFSET 4, LENGTH 4
	MSG NAME: FUNKTIONSTASTEN - function keys, OFFSET 10, LENGTH 3
	MSG NAME: AKT_SYS - active application, OFFSET 13, LENGTH 3
ECU NAME: GPS_A1, ID: 0x0338. MSG COUNT: 2
	MSG NAME: LATITUDE - (ms) (Ms) GPS Latitude (North + =), OFFSET 0, LENGTH 32
	MSG NAME: LONGITUDE - (ms) (Ms) GPS Longitude (East + =), OFFSET 32, LENGTH 32
ECU NAME: GPS_A2, ID: 0x0339. MSG COUNT: 6
	MSG NAME: UTC_YEARS - (years) (Years) UTC years, OFFSET 0, LENGTH 16
	MSG NAME: UTC_MONTHS - (months) (Months) UTC months, OFFSET 16, LENGTH 8
	MSG NAME: UTC_DAYS - (days) (Days) UTC days, OFFSET 24, LENGTH 8
	MSG NAME: UTC_HOURS - (h) (H) UTC hours, OFFSET 32, LENGTH 8
	MSG NAME: UTC_MINUTES - (min) (Min) UTC minutes, OFFSET 40, LENGTH 8
	MSG NAME: UTC_SECONDS - (s) (S) UTC seconds, OFFSET 48, LENGTH 16
ECU NAME: GPS_A3, ID: 0x033A. MSG COUNT: 13
	MSG NAME: GPS_SPEED - (cm/s) (Cm / s) GPS Speed, OFFSET 0, LENGTH 16
	MSG NAME: GPS_HEADING - (°) (°) GPS Heading (0 ° = North), OFFSET 16, LENGTH 8
	MSG NAME: GPS_HEIGHT - (m) (M) GPS height, OFFSET 24, LENGTH 8
	MSG NAME: GPS_FIX - GPS fix, OFFSET 37, LENGTH 3
	MSG NAME: POS_AVLB - GPS position avilable, OFFSET 40, LENGTH 1
	MSG NAME: DIFF_POS_AVLB - Differential GPS position data available, OFFSET 41, LENGTH 1
	MSG NAME: DEAD_RCK - Dead reckoning available, OFFSET 42, LENGTH 1
	MSG NAME: IDG - Inside digitalized area (on map), OFFSET 43, LENGTH 1
	MSG NAME: FDG - Fully digitalized area, OFFSET 44, LENGTH 1
	MSG NAME: MDM - Matched to digitally map, OFFSET 45, LENGTH 1
	MSG NAME: CALI - Calibrated, OFFSET 46, LENGTH 1
	MSG NAME: V_DOP - Vertical Dilution Of Position, OFFSET 48, LENGTH 8
	MSG NAME: H_DOP - Horizontal Dilution Of Position, OFFSET 56, LENGTH 8
ECU NAME: IPS_A1, ID: 0x01BA. MSG COUNT: 6
	MSG NAME: IPS_UPD_ACK - IPS Update Acknowledge, OFFSET 0, LENGTH 1
	MSG NAME: IPS_ERROR - IPS error, OFFSET 1, LENGTH 3
	MSG NAME: IPS_WATCH - IPS Watchdog, OFFSET 4, LENGTH 4
	MSG NAME: IPS_TIME - IPS display time, OFFSET 8, LENGTH 4
	MSG NAME: IPS_INDICATION - IPS icon display, OFFSET 12, LENGTH 4
	MSG NAME: IPS_ATTRIBUTE - IPS Icon attributes, OFFSET 20, LENGTH 4
ECU NAME: TP_AGW_KOMBI1, ID: 0x01A4. MSG COUNT: 1
	MSG NAME: TP_AGW_KOMBI - Kommunikation AGW zum KOMBI, OFFSET 0, LENGTH 64
ECU NAME: TP_AGW_MSS3, ID: 0x0334. MSG COUNT: 1
	MSG NAME: TP_AGW_MSS3 - Kommunikation AGW zum MSS, OFFSET 0, LENGTH 64
ECU NAME: TP_AGW_TELEAID6, ID: 0x03E3. MSG COUNT: 1
	MSG NAME: TP_AGW_TELEAID - Kommunikation AGW zum TELEAID, OFFSET 0, LENGTH 64
ECU NAME: NM_AGW, ID: 0x0416. MSG COUNT: 1
	MSG NAME: NM - Netzwerkmanagement, OFFSET 0, LENGTH 64
ECU NAME: D_RS_AGW, ID: 0x04F6. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST0, ID: 0x0680. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST1, ID: 0x0681. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST10, ID: 0x068A. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST11, ID: 0x068B. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST12, ID: 0x068C. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST13, ID: 0x068D. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST14, ID: 0x068E. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST15, ID: 0x068F. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST2, ID: 0x0682. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST3, ID: 0x0683. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST4, ID: 0x0684. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST5, ID: 0x0685. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST6, ID: 0x0686. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST7, ID: 0x0687. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST8, ID: 0x0688. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: D_RS_MOST9, ID: 0x0689. MSG COUNT: 1
	MSG NAME: D_RS - KWP2000 Diagnose-Response, OFFSET 0, LENGTH 64
ECU NAME: SG_APPL_AGW, ID: 0x0776. MSG COUNT: 1
	MSG NAME: SG_APPL - Steuergerät an externe Applikation, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_AAG, ID: 0x072F. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_AGW, ID: 0x05C9. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_ALB, ID: 0x05BE. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_ARMADA, ID: 0x06A3. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_BSG, ID: 0x072D. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_DBE, ID: 0x0678. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_EZS, ID: 0x04DF. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_FDSVL, ID: 0x06A1. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_FDSVR, ID: 0x06A0. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_HFS, ID: 0x0568. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_KLA, ID: 0x078E. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_KOMBI, ID: 0x05AB. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_LRK, ID: 0x06B0. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_MRM, ID: 0x06C1. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_MSS, ID: 0x0720. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_OBF, ID: 0x06BA. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_PFDS, ID: 0x0731. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_PTS, ID: 0x072C. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_RDK, ID: 0x06A7. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_RWT, ID: 0x05BF. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_SAM_B, ID: 0x067E. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_SAM_H, ID: 0x057C. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_SAM_V, ID: 0x067D. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_SB, ID: 0x06B2. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_SD, ID: 0x07C4. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_SF, ID: 0x06B3. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_SHZ, ID: 0x0564. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_STH, ID: 0x073F. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_THL, ID: 0x0756. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_THR, ID: 0x0754. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_TVL, ID: 0x06D7. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_TVR, ID: 0x06C0. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_UBF, ID: 0x06A2. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: APPL_SG_WSS, ID: 0x06B7. MSG COUNT: 1
	MSG NAME: APPL_SG - Externe Applikation zu Steuergerät, OFFSET 0, LENGTH 64
ECU NAME: SD_RS_AGW, ID: 0x07D6. MSG COUNT: 64
	MSG NAME: AGW_KENN - byte identification for> 8, OFFSET 0, LENGTH 1
	MSG NAME: AGW_FV07 - Error vector 07h, OFFSET 1, LENGTH 1
	MSG NAME: AGW_FV06 - Error vector 06h, OFFSET 2, LENGTH 1
	MSG NAME: AGW_FV05 - Error vector 05h, OFFSET 3, LENGTH 1
	MSG NAME: AGW_FV04 - Error vector 04h, OFFSET 4, LENGTH 1
	MSG NAME: AGW_FV03 - Error vector 03h, OFFSET 5, LENGTH 1
	MSG NAME: AGW_FV02 - Error vector 02h, OFFSET 6, LENGTH 1
	MSG NAME: AGW_FV01 - Error vector 01h, OFFSET 7, LENGTH 1
	MSG NAME: AGW_FV0F - Error vector 0Fh, OFFSET 8, LENGTH 1
	MSG NAME: AGW_FV0E - Error vector 0Eh, OFFSET 9, LENGTH 1
	MSG NAME: AGW_FV0D - Error vector 0Dh, OFFSET 10, LENGTH 1
	MSG NAME: AGW_FV0C - Error vector 0Ch, OFFSET 11, LENGTH 1
	MSG NAME: AGW_FV0B - Error vector 0Bh, OFFSET 12, LENGTH 1
	MSG NAME: AGW_FV0A - Error vector 0Ah, OFFSET 13, LENGTH 1
	MSG NAME: AGW_FV09 - Error vector 09h, OFFSET 14, LENGTH 1
	MSG NAME: AGW_FV08 - Error vector 08h, OFFSET 15, LENGTH 1
	MSG NAME: AGW_FV17 - Error vector 17h, OFFSET 16, LENGTH 1
	MSG NAME: AGW_FV16 - Error vector 16h, OFFSET 17, LENGTH 1
	MSG NAME: AGW_FV15 - Error vector 15h, OFFSET 18, LENGTH 1
	MSG NAME: AGW_FV14 - Error vector 14h, OFFSET 19, LENGTH 1
	MSG NAME: AGW_FV13 - Error vector 13h, OFFSET 20, LENGTH 1
	MSG NAME: AGW_FV12 - Error vector 12h, OFFSET 21, LENGTH 1
	MSG NAME: AGW_FV11 - Error vector 11h, OFFSET 22, LENGTH 1
	MSG NAME: AGW_FV10 - Error vector 10h, OFFSET 23, LENGTH 1
	MSG NAME: AGW_FV1F - Error vector 1Fh, OFFSET 24, LENGTH 1
	MSG NAME: AGW_FV1E - Error vector 1Eh, OFFSET 25, LENGTH 1
	MSG NAME: AGW_FV1D - Error vector 1Dh, OFFSET 26, LENGTH 1
	MSG NAME: AGW_FV1C - Error vector 1Ch, OFFSET 27, LENGTH 1
	MSG NAME: AGW_FV1B - Error vector 1Bh, OFFSET 28, LENGTH 1
	MSG NAME: AGW_FV1A - Error vector 1Ah, OFFSET 29, LENGTH 1
	MSG NAME: AGW_FV19 - Error vector 19h, OFFSET 30, LENGTH 1
	MSG NAME: AGW_FV18 - Error vector 18h, OFFSET 31, LENGTH 1
	MSG NAME: AGW_FV27 - Error vector 27h, OFFSET 32, LENGTH 1
	MSG NAME: AGW_FV26 - Error vector 26h, OFFSET 33, LENGTH 1
	MSG NAME: AGW_FV25 - Error vector 25h, OFFSET 34, LENGTH 1
	MSG NAME: AGW_FV24 - Error vector 24, OFFSET 35, LENGTH 1
	MSG NAME: AGW_FV23 - Error vector 23h, OFFSET 36, LENGTH 1
	MSG NAME: AGW_FV22 - Error vector 22h, OFFSET 37, LENGTH 1
	MSG NAME: AGW_FV21 - Error vector 21h, OFFSET 38, LENGTH 1
	MSG NAME: AGW_FV20 - Error vector 20h, OFFSET 39, LENGTH 1
	MSG NAME: AGW_FV2F - Error vector 2Fh, OFFSET 40, LENGTH 1
	MSG NAME: AGW_FV2E - Error vector 2Eh, OFFSET 41, LENGTH 1
	MSG NAME: AGW_FV2D - Error vector 2Dh, OFFSET 42, LENGTH 1
	MSG NAME: AGW_FV2C - Error vector 2Ch, OFFSET 43, LENGTH 1
	MSG NAME: AGW_FV2B - Error vector 2Bh, OFFSET 44, LENGTH 1
	MSG NAME: AGW_FV2A - Error vector 2Ah, OFFSET 45, LENGTH 1
	MSG NAME: AGW_FV29 - Error vector 29h, OFFSET 46, LENGTH 1
	MSG NAME: AGW_FV28 - Error vector 28h, OFFSET 47, LENGTH 1
	MSG NAME: AGW_FV37 - Error vector 37h, OFFSET 48, LENGTH 1
	MSG NAME: AGW_FV36 - Error vector 36h, OFFSET 49, LENGTH 1
	MSG NAME: AGW_FV35 - Error vector 35h, OFFSET 50, LENGTH 1
	MSG NAME: AGW_FV34 - Error vector 34h, OFFSET 51, LENGTH 1
	MSG NAME: AGW_FV33 - Error vector 33h, OFFSET 52, LENGTH 1
	MSG NAME: AGW_FV32 - Error vector 32h, OFFSET 53, LENGTH 1
	MSG NAME: AGW_FV31 - Error vector 31h, OFFSET 54, LENGTH 1
	MSG NAME: AGW_FV30 - Error vector 30h, OFFSET 55, LENGTH 1
	MSG NAME: AGW_PGV01 - State variable 01h, OFFSET 56, LENGTH 1
	MSG NAME: AGW_FV3E - Error vector 3Eh, OFFSET 57, LENGTH 1
	MSG NAME: AGW_FV3D - Error vector 3Dh, OFFSET 58, LENGTH 1
	MSG NAME: AGW_FV3C - Error vector 3Ch, OFFSET 59, LENGTH 1
	MSG NAME: AGW_FV3B - Error vector 3Bh, OFFSET 60, LENGTH 1
	MSG NAME: AGW_FV3A - Error vector 3Ah, OFFSET 61, LENGTH 1
	MSG NAME: AGW_FV39 - Error vector 39h, OFFSET 62, LENGTH 1
	MSG NAME: AGW_FV38 - Error vector 38h, OFFSET 63, LENGTH 1
