panel size, 159x107mm
PCB thickness, 0.8mm
number of layers, 2
soldermask color, Red
silkscreen color, White
oz copper, 1oz
finish, HASL lead free
stencils, top+bottom
pcs per panel, 9
min trace width, 0.1524mm / 0.0060in
min drill size, 0.3048mm / 0.0120in
