+++
brief = "Footprint anchor should placed at the location of Pin-1"
+++

For through hole components the footprint anchor should be placed at the location of pin 1.

{{< klcimg src="F7.2" title="Footprint anchor is set to location of Pin-1" >}}