# Problem Statement

Build a 100-bit left/right rotator, with synchronous load and left/right enable. A rotator shifts-in the shifted-out bit from the other end of the register, unlike a shifter that discards the shifted-out bit and shifts in a zero. If enabled, a rotator rotates the bits around and does not modify/discard them.

- load: Loads shift register with data[99:0] instead of rotating.
- ena[1:0]: Chooses whether and which direction to rotate.
    - 2'b01 rotates right by one bit
    - 2'b10 rotates left by one bit
    - 2'b00 and 2'b11 do not rotate.
- q: The contents of the rotator.