# Problem Statement

Create 16 D flip-flops. It's sometimes useful to only modify parts of a group of flip-flops. The byte-enable inputs control whether each byte of the 16 registers should be written to on that cycle. byteena[1] controls the upper byte d[15:8], while byteena[0] controls the lower byte d[7:0].

resetn is a synchronous, active-low reset.

All DFFs should be triggered by the positive edge of clk.



[Find the verilog Solution](solution_verilog.v)
