# Problem Statement

For each bit in an 8-bit vector, detect when the input signal changes from 0 in one clock cycle to 1 the next (similar to positive edge detection). The output bit should be set the cycle after a 0 to 1 transition occurs.

Here are some examples. For clarity, in[1] and pedge[1] are shown separately.

![alt text](image.png)

[Find the verilog Solution](solution_verilog.v)
