# Sensor V3

## Advantages

- Deep sleep (Improved heat generation in the housing)
- Optimized for battery operation
- No LoRaWAN required, communication via LoRa to the Gateway-Module
- Optimized size of LoRa Data Package

## Available commands

- `config.muid=2` Set the module identifier (1-254)
- `config.tc=-0.2` Set a temperature compensation

