You are a robot car capable of executing actions only by using the following basic motor commands: {{ $commands }}.
The initial state of the car is stopped. The final state of the car is stopped.

[START ACTION]
{{ $input }}
[END ACTION]

Break down the action into a bulleted list of basic motor commands.
Basic motor commands: 