diff -aur SDK_10.0.10.118/sdk/bsp/peripherals/src/hw_dma.c ../build/extbld/third_party/bsp/dialog/da14695/sdk/SDK_10.0.10.118/sdk/bsp/peripherals/src/hw_dma.c
--- SDK_10.0.10.118/sdk/bsp/peripherals/src/hw_dma.c	2019-12-20 11:51:02.000000000 +0300
+++ ../build/extbld/third_party/bsp/dialog/da14695/sdk/SDK_10.0.10.118/sdk/bsp/peripherals/src/hw_dma.c	2020-07-09 23:26:18.590168140 +0300
@@ -37,7 +37,7 @@
         void *user_data;
 } dma_callbacks_user_data[8];
 
-#define DMA_CHN_REG(reg, chan) ((volatile uint32 *)(&(reg)) + ((chan) * 8))
+#define DMA_CHN_REG(reg, chan) ((volatile uint32_t *)(&(reg)) + ((chan) * 8))
 
 /**
  * \brief Initialize DMA Channel
@@ -49,11 +49,11 @@
 {
         volatile dma_size_t *dma_x_len_reg;
         volatile dma_size_t *dma_x_int_reg;
-        volatile uint32 *dma_x_ctrl_reg;
-        volatile uint32 *dma_x_a_start_reg;
-        volatile uint32 *dma_x_b_start_reg;
-        uint32 src_address;
-        uint32 dest_address;
+        volatile uint32_t *dma_x_ctrl_reg;
+        volatile uint32_t *dma_x_a_start_reg;
+        volatile uint32_t *dma_x_b_start_reg;
+        uint32_t src_address;
+        uint32_t dest_address;
 
         /* Make sure the DMA channel length is not zero */
         ASSERT_WARNING(channel_setup->length > 0);
@@ -184,7 +184,7 @@
         dma_callbacks_user_data[channel].callback = cb;
 
         // Look up DMAx_A_START_REG address
-        volatile uint32 *dma_x_a_start_reg = DMA_CHN_REG(DMA->DMA0_A_START_REG, channel);
+        volatile uint32_t *dma_x_a_start_reg = DMA_CHN_REG(DMA->DMA0_A_START_REG, channel);
 
         // Look up DMAX_LEN_REG address
         volatile dma_size_t *dma_x_len_reg = DMA_CHN_REG(DMA->DMA0_LEN_REG, channel);
@@ -219,7 +219,7 @@
         dma_callbacks_user_data[channel].callback = cb;
 
         // Look up DMAx_B_START_REG address
-        volatile uint32 *dma_x_b_start_reg = DMA_CHN_REG(DMA->DMA0_B_START_REG, channel);
+        volatile uint32_t *dma_x_b_start_reg = DMA_CHN_REG(DMA->DMA0_B_START_REG, channel);
 
         // Look up DMAX_LEN_REG address
         volatile dma_size_t *dma_x_len_reg = DMA_CHN_REG(DMA->DMA0_LEN_REG, channel);
@@ -325,7 +325,7 @@
         uint16_t i;
         volatile dma_size_t *dma_x_len_reg;
         volatile dma_size_t *dma_x_int_reg;
-        volatile uint32 *dma_x_ctrl_reg;
+        volatile uint32_t *dma_x_ctrl_reg;
         risen = DMA->DMA_INT_STATUS_REG;
 
         for (i = 0; risen != 0 && i < 8; ++i, risen >>= 1) {
