Supported Devices & Architectures
=================================

armsr-armv7
-----------

* Arm SystemReady (EFI) 32-bit

armsr-armv8
-----------

* Arm SystemReady (EFI) 64-bit

ath79-generic
--------------

* ALFA Network

  - AP121F

* AVM

  - FRITZ!WLAN Repeater 300E [#avmflash]_
  - Fritz!WLAN Repeater 450E [#avmflash]_
  - Fritz!Box 4020 [#avmflash]_

* Buffalo

  - WZR-HP-AG300H / WZR-600DHP
  - WZR-HP-G300NH (rtl8366s)

* devolo

  - WiFi pro 1200e [#lan_as_wan]_
  - WiFi pro 1200i
  - WiFi pro 1750c
  - WiFi pro 1750e [#lan_as_wan]_
  - WiFi pro 1750i
  - WiFi pro 1750x

* D-Link

  - DAP-1330 A1 [#lan_as_wan]_
  - DAP-1365 A1 [#lan_as_wan]_
  - DAP-2660 A1 [#lan_as_wan]_
  - DAP-2680 A1 [#lan_as_wan]_
  - DAP-2695 A1 [#lan_as_wan]_
  - DIR-505 A1 [#lan_as_wan]_
  - DIR-505 A2 [#lan_as_wan]_
  - DIR-825 B1

* Enterasys

  - WS-AP3705i

* Extreme Networks

  - WS-AP3805i

* GL.iNet

  - 6416A
  - GL-AR150
  - GL-AR300M-Lite
  - GL-AR750
  - GL-USB150 (Microuter)

* Joy-IT

  - JT-OR750i

* LibreRouter

  - LibreRouter v1 [#missing_radios]_

* NETGEAR

  - WNDR3700 (v1, v2)
  - WNDR3800
  - WNR2200 (8M, 16M)
  - WNDRMAC (v2)

* OCEDO

  - Koala
  - Raccoon

* Onion

  - Omega [#modular_ethernet]_

* OpenMesh

  - A40
  - A60
  - MR600 (v1, v2)
  - MR900 (v1, v2)
  - MR1750 (v1, v2)
  - OM2P (v1, v2, v4)
  - OM2P-HS (v1, v2, v3, v4)
  - OM2P-LC
  - OM5P
  - OM5P-AC (v1, v2)
  - OM5P-AN

* Plasma Cloud

  - PA300
  - PA300E

* Siemens

  - WS-AP3610

* Sophos

  - AP100
  - AP100c
  - AP55
  - AP55c

* Teltonika

  - RUT230 (v1)

* TP-Link

  - Archer A7 (v5)
  - Archer C5 (v1)
  - Archer C6 (v2 EU/RU/JP)
  - Archer C7 (v2, v4, v5)
  - Archer C59 (v1)
  - Archer C60 (v1)
  - CPE210 (v1.0, v1.1, v2.0, v3.0, v3.1, v3.20)
  - CPE220 (v3.0)
  - CPE510 (v1.0, v1.1, v2.0, v3.0)
  - CPE710 (v1.0)
  - EAP225-Outdoor (v1, v3)
  - TL-WDR3500 (v1)
  - TL-WDR3600 (v1)
  - TL-WDR4300 (v1)
  - TL-WR810N (v1)
  - TL-WR842N/ND (v3)
  - TL-WR1043N/ND (v2, v3, v4, v5)
  - TL-WR2543N/ND (v1)
  - WBS210 (v1.20, v2.0)
  - WBS510 (v1.20)

* Ubiquiti

  - UniFi AC Lite
  - UniFi AC LR
  - UniFi AC Mesh
  - UniFi AC Mesh Pro
  - UniFi AC Pro
  - UniFi AP
  - UniFi AP LR
  - UniFi AP Outdoor+
  - UniFi AP PRO
  - UniFi Swiss Army Knife Ultra

ath79-mikrotik
--------------

* Mikrotik

  - RB951Ui-2nD (hAP)
  - RBwAPR-2nD (wAP R)

ath79-nand
----------

* Aerohive

  - HiveAP 121

* GL.iNet

  - GL-AR300M
  - GL-AR750S
  - GL-XE300

* NETGEAR

  - WNDR3700 (v4)
  - WNDR4300 (v1)

* Zyxel

  - NBG6716

brcm2708-bcm2708
----------------

* Raspberry Pi 1

brcm2708-bcm2709
----------------

* Raspberry Pi 2


ipq40xx-generic
---------------

* 8devices

  - Jalapeno

* Aruba

  - AP-303
  - AP-303H
  - AP-365
  - Instant On AP11
  - Instant On AP11D
  - Instant On AP17

* AVM

  - FRITZ!Box 4040 [#avmflash]_
  - FRITZ!Box 7520 (v1) [#eva_ramboot]_ [#lan_as_wan]_
  - FRITZ!Box 7530 [#eva_ramboot]_ [#lan_as_wan]_
  - FRITZ!Repeater 1200 [#eva_ramboot]_

* GL.iNet

  - GL-AP1300
  - GL-B1300

* Linksys

  - EA6350 (v3)

* NETGEAR

  - EX6100 (v2)
  - EX6150 (v2)

* OpenMesh

  - A42
  - A62

* Plasma Cloud

  - PA1200
  - PA2200

* Zyxel

  - NBG6617

ipq40xx-mikrotik
----------------

* Mikrotik

  - DISC Lite5 ac (RBDiscG-5acD)
  - hAP ac2
  - SXTsq 5 ac (RBSXTsqG-5acD)

ipq806x-generic
---------------

* NETGEAR

  - R7800

* Ubiquiti

  - UniFi AC HD

lantiq-xrx200
-------------

* Arcadyan

  - VGV7510KW22 (o2 Box 6431)

* AVM

  - FRITZ!Box 7360 (v1, v2) [#avmflash]_ [#lan_as_wan]_
  - FRITZ!Box 7360 SL [#avmflash]_ [#lan_as_wan]_
  - FRITZ!Box 7362 SL [#eva_ramboot]_ [#lan_as_wan]_
  - FRITZ!Box 7412 [#eva_ramboot]_

* TP-Link

  - TD-W8970 (v1) [#lan_as_wan]_

lantiq-xway
-----------

* AVM

  - FRITZ!Box 7312 [#avmflash]_

* NETGEAR

  - DGN3500B [#lan_as_wan]_

mediatek-filogic
----------------

* ASUS

  - TUF AX4200
  - TUF AX6000

* Cudy

  - WR3000 (v1)

* GL.iNet

  - GL-MT3000

* NETGEAR

  - WAX220

* Ubiquiti

  - UniFi 6 Plus

* Zyxel

  - NWA50AX Pro

mediatek-mt7622
---------------

* Linksys

  - E8450

* Ubiquiti

  - UniFi 6 LR (v1)

mpc85xx-p1010
-------------

* Enterasys

  - WS-AP3715i

* Sophos

  - RED 15w Rev.1

* TP-Link

  - TL-WDR4900 (v1)

mpc85xx-p1020
---------------

* Aerohive

  - HiveAP 330

* Enterasys

  - WS-AP3710i

* Extreme Networks

  - WS-AP3825i

* Hewlett-Packard

  - MSM460

* Ocedo

  - Panda

ramips-mt7620
-------------

* ASUS

  - RT-AC51U

* GL.iNet

  - GL-MT300A
  - GL-MT300N
  - GL-MT750

* NETGEAR

  - EX3700
  - EX3800
  - EX6130

* Nexx

  - WT3020AD/F/H

* TP-Link

  - Archer C2 (v1)
  - Archer C20 (v1)
  - Archer C20i
  - Archer C50 (v1)

* Xiaomi

  - MiWiFi Mini

ramips-mt7621
-------------

* ASUS

  - RT-AC57U (v1)
  - RT-AX53U

* Cudy

  - WR1300 (v1)
  - WR2100
  - X6 (v1, v2)

* D-Link

  - COVR-X1860 (A1)
  - DAP-X1860 (A1)
  - DIR-860L (B1)
  - DIR-878 (A1)
  - DIR-882 (A1)

* GL.iNet

  - GL-MT1300

* MERCUSYS

  - MR70X (v1)

* NETGEAR

  - EX6150 (v1)
  - R6220
  - R6260
  - WAC104
  - WAX202

* TP-Link

  - EAP615-Wall (v1)
  - RE500 (v1)
  - RE650 (v1)

* Ubiquiti

  - UniFi 6 Lite
  - UniFi nanoHD

* Wavlink

  - WS-WN572HP3 (4G)

* Xiaomi

  - Xiaomi Mi Router 3G (v1, v2)
  - Xiaomi Mi Router 4A (Gigabit Edition v1, v2)

* Zbtlink

  - WG3526-16M
  - WG3526-32M

* Zyxel

  - NWA50AX
  - WSM20

ramips-mt76x8
-------------

* Cudy

  - WR1000 (v1)

* GL.iNet

  - GL-MT300N (v2)
  - microuter-N300
  - VIXMINI

* NETGEAR

  - R6020
  - R6120

* RAVPower

  - RP-WD009

* TP-Link

  - Archer C20 (v4, v5)
  - Archer C50 (v3, v4)
  - RE200 (v2, v3, v4)
  - TL-MR3020 (v3)
  - TL-MR3420 (v5)
  - TL-MR6400 (v5)
  - TL-WA801ND (v5)
  - TL-WR841N (v13)
  - TL-WR902AC (v3)

* VoCore

  - VoCore2

* Xiaomi

  - Xiaomi Mi Router 4A (100M Edition)
  - Xiaomi Mi Router 4A (100M International Edition)
  - Xiaomi Mi Router 4C

realtek-rtl838x
---------------

* D-Link

  - DGS-1210-10P (F1)

rockchip-armv8
--------------

* FriendlyElec

  - NanoPi R2S
  - NanoPi R3S
  - NanoPi R4S (4GB LPDDR4)

sunxi-cortexa7
--------------

* LeMaker

  - Banana Pi M1

x86-generic
-----------

* x86-generic
* x86-virtualbox
* x86-vmware

See also: :doc:`x86`

x86-geode
---------

* x86-geode

See also: :doc:`x86`

x86-64
------

* x86-64-generic
* x86-64-virtualbox
* x86-64-vmware

See also: :doc:`x86`

Footnotes
---------

.. [#avmflash]
  For instructions on how to flash AVM devices, visit https://fritz-tools.readthedocs.io

.. [#eva_ramboot]
  For instructions on how to flash AVM NAND devices, see the respective
  commit which added support in OpenWrt.

.. [#lan_as_wan]
  All LAN ports on this device are used as WAN.

.. [#missing_radios]
  This device contains more than two WLAN radios, which is currently
  unsupported by Gluon. Only the first two radios will work.

.. [#modular_ethernet]
  These devices follow a modular principle,
  which means even basic functionality like ethernet is provided by an expansion-board,
  that may not be bundled with the device itself.
  Such expansions are recommended for the config mode, but are not strictly necessary,
  as exposed serial ports may grant sufficient access as well.
