Gluon 2022.1.3
==============

Bugfixes
--------

* Ipq40xx Wave2 devices temporarily use non-ct firmware again to work around 802.11s unicast package loss in ath10k-ct
  (`#2692 <https://github.com/freifunk-gluon/gluon/issues/2692>`_)

* Modify kernel builds slightly to work around a boot hang on various devices based on the QCA9563 SoC - especially the Unifi AC-* devices
  (`#2784 <https://github.com/freifunk-gluon/gluon/issues/2784>`_)

* Work around an issue with wifi setup timing by waiting a bit while device initialisation is ongoing
  (`#2779 <https://github.com/freifunk-gluon/gluon/issues/2779>`_)


Known issues
------------

* Upgrading EdgeRouter-X from versions before v2020.1.x may lead to a soft-bricked state due to bad blocks on the NAND flash which the NAND driver before this release does not handle well.
  (`#1937 <https://github.com/freifunk-gluon/gluon/issues/1937>`_)

* The integration of the BATMAN_V routing algorithm is incomplete.

  - Mesh neighbors don't appear on the status page. (`#1726 <https://github.com/freifunk-gluon/gluon/issues/1726>`_)
    Many tools have the BATMAN_IV metric hardcoded, these need to be updated to account for the new throughput
    metric.
  - Throughput values are not correctly acquired for different interface types.
    (`#1728 <https://github.com/freifunk-gluon/gluon/issues/1728>`_)
    This affects virtual interface types like bridges and VXLAN.

* Default TX power on many Ubiquiti devices is too high, correct offsets are unknown
  (`#94 <https://github.com/freifunk-gluon/gluon/issues/94>`_)

  Reducing the TX power in the Advanced Settings is recommended.

* In configurations without VXLAN, the MAC address of the WAN interface is modified even when Mesh-on-WAN is disabled
  (`#496 <https://github.com/freifunk-gluon/gluon/issues/496>`_)

  This may lead to issues in environments where a fixed MAC address is expected (like VMware when promiscuous mode is disallowed).
