| LibDriver GT30L32S4W 1.0.0 GT30L32S4W full function driver

Macros
gt30l32s4w link driver function
gt30l32s4w driver function

gt30l32s4w link driver modules More...

## Macros
#define | DRIVER_GT30L32S4W_LINK_INIT(HANDLE, STRUCTURE) memset(HANDLE, 0, sizeof(STRUCTURE))
| initialize gt30l32s4w_handle_t structure More...
#define | DRIVER_GT30L32S4W_LINK_SPI_INIT(HANDLE, FUC) (HANDLE)->spi_init = FUC
| link spi_init function More...
#define | DRIVER_GT30L32S4W_LINK_SPI_DEINIT(HANDLE, FUC) (HANDLE)->spi_deinit = FUC
| link spi_deinit function More...
#define | DRIVER_GT30L32S4W_LINK_SPI_WRITE_READ(HANDLE, FUC) (HANDLE)->spi_write_read = FUC
| link spi_write_read function More...
#define | DRIVER_GT30L32S4W_LINK_DELAY_MS(HANDLE, FUC) (HANDLE)->delay_ms = FUC
| link delay_ms function More...
#define | DRIVER_GT30L32S4W_LINK_DEBUG_PRINT(HANDLE, FUC) (HANDLE)->debug_print = FUC
| link debug_print function More...

## Detailed Description

gt30l32s4w link driver modules

## Macro Definition Documentation

## ◆ DRIVER_GT30L32S4W_LINK_DEBUG_PRINT

#define DRIVER_GT30L32S4W_LINK_DEBUG_PRINT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->debug_print = FUC

link debug_print function

Parameters

  [in] | HANDLE | pointer to a gt30l32s4w handle structure
  [in] | FUC | pointer to a debug_print function address

Note
  none

Definition at line 186 of file driver_gt30l32s4w.h.

## ◆ DRIVER_GT30L32S4W_LINK_DELAY_MS

#define DRIVER_GT30L32S4W_LINK_DELAY_MS | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->delay_ms = FUC

link delay_ms function

Parameters

  [in] | HANDLE | pointer to a gt30l32s4w handle structure
  [in] | FUC | pointer to a delay_ms function address

Note
  none

Definition at line 178 of file driver_gt30l32s4w.h.

## ◆ DRIVER_GT30L32S4W_LINK_INIT

#define DRIVER_GT30L32S4W_LINK_INIT | ( |  | HANDLE,
|  |  | STRUCTURE
| ) |  | memset(HANDLE, 0, sizeof(STRUCTURE))

initialize gt30l32s4w_handle_t structure

Parameters

  [in] | HANDLE | pointer to a gt30l32s4w handle structure
  [in] | STRUCTURE | gt30l32s4w_handle_t

Note
  none

Definition at line 146 of file driver_gt30l32s4w.h.

## ◆ DRIVER_GT30L32S4W_LINK_SPI_DEINIT

#define DRIVER_GT30L32S4W_LINK_SPI_DEINIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_deinit = FUC

link spi_deinit function

Parameters

  [in] | HANDLE | pointer to a gt30l32s4w handle structure
  [in] | FUC | pointer to a spi_deinit function address

Note
  none

Definition at line 162 of file driver_gt30l32s4w.h.

## ◆ DRIVER_GT30L32S4W_LINK_SPI_INIT

#define DRIVER_GT30L32S4W_LINK_SPI_INIT | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_init = FUC

link spi_init function

Parameters

  [in] | HANDLE | pointer to a gt30l32s4w handle structure
  [in] | FUC | pointer to a spi_init function address

Note
  none

Definition at line 154 of file driver_gt30l32s4w.h.

## ◆ DRIVER_GT30L32S4W_LINK_SPI_WRITE_READ

#define DRIVER_GT30L32S4W_LINK_SPI_WRITE_READ | ( |  | HANDLE,
|  |  | FUC
| ) |  | (HANDLE)->spi_write_read = FUC

link spi_write_read function

Parameters

  [in] | HANDLE | pointer to a gt30l32s4w handle structure
  [in] | FUC | pointer to a spi_write_read function address

Note
  none

Definition at line 170 of file driver_gt30l32s4w.h.