## NAME

gtf - calculate VESA GTF mode lines

## SYNOPSIS

gtf h-resolution v-resolution refresh

## DESCRIPTION

Gtf is a utility for calculating VESA GTF modes. Given the desired horizontal and vertical resolutions and refresh rate (in Hz), the parameters for a matching VESA GTF mode are printed out. Two output formats are supported: mode lines suitable for the Xorg xorg.conf(5) file, and mode parameters suitable for the Linux fbset(8) utility.

## OPTIONS

-v | --verboseEnable verbose printouts This shows a trace for each step of the computation.

-x | --xorgmodePrint the mode parameters as Xorg-style mode lines. This is the default format.

-f | --fbsetPrint the mode parameters in a format suitable for fbset(8) .

## SEE ALSO

xorg.conf(5), cvt(1)

## AUTHOR

Andy Ritger.

This program is based on the Generalized Timing Formula (GTF(TM)) Standard Version: 1.0, Revision: 1.0. The GTF Excel(TM) spreadsheet, a sample (and the definitive) implementation of the GTF Timing Standard is available at <ftp://ftp.vesa.org/pub/GTF/VTF_V1R1.xls>.