|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
PBV_DAB_frame_map.h
Go to the documentation of this file.
1
7// This is a guard condition so that contents of this file are not included
8// more than once.
9#ifndef APP_PBV_DAB_FRAME_MAP_H
10#define APP_PBV_DAB_FRAME_MAP_H
11
12#include <xc.h> // include processor files - each processor file is guarded.
13#include "PBV_interface.h"
14
15
16
19void App_PBV_DAB_Init(void);
20void App_PBV_DAB_Task_10ms(void);
21void App_PBV_DAB_Task_1s(void);
22 PBV_Datatype_TX_t * App_PBV_DAB_Get_TX_Log_ptr(void);
23
24#endif /* APP_PBV_DAB_FRAME_MAP_H */
25
App_PBV_DAB_Get_TX_Log_ptr
PBV_Datatype_TX_t * App_PBV_DAB_Get_TX_Log_ptr(void)
App_PBV_DAB_Init
void App_PBV_DAB_Init(void)
This function initializes the local pbv objects. these objects are then passed on to the app_PBV_init...
Definition PBV_dab_frame_map.c:95
App_PBV_DAB_Task_10ms
void App_PBV_DAB_Task_10ms(void)
10ms PBV task to be execution
Definition PBV_dab_frame_map.c:121
App_PBV_DAB_Task_1s
void App_PBV_DAB_Task_1s(void)
1 second PBV task to be execution
Definition PBV_dab_frame_map.c:150
PBV_Datatype_TX_t
Definition PBV_interface.h:75