|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
SMPS_Controller_Options_T Struct Reference

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/pwrctrl/dcdt/smps_control.h>`

Collaboration diagram for SMPS_Controller_Options_T:

## Data Fields
uint16_t | triggerSelectFlag
uint16_t | delayValue
volatile unsigned int * | trigger
volatile unsigned int * | period

## Detailed Description

Definition at line 467 of file smps_control.h.

## Field Documentation

## ◆ delayValue

uint16_t delayValue

Definition at line 473 of file smps_control.h.

## ◆ period

volatile unsigned int* period

Definition at line 475 of file smps_control.h.

## ◆ trigger

volatile unsigned int* trigger

Definition at line 474 of file smps_control.h.

## ◆ triggerSelectFlag

uint16_t triggerSelectFlag

Definition at line 469 of file smps_control.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/pwrctrl/dcdt/smps_control.h