|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Functions | Variables
fault.c File Reference
Fault Monitor » Fault Configuration

Contains fault functions including the fault handler, fault object initialization and fault execution. More...

`#include "xc.h"`
`#include <stdbool.h>`
`#include <stddef.h>`
`#include "cmp/cmp1.h"`
`#include "cmp/cmp3.h"`
`#include "pwm_hs/pwm.h"`
`#include "system/pins.h"`
`#include "config/macros.h"`
`#include "device/device.h"`
`#include "pwrctrl/pwrctrl.h"`
`#include "fault_common.h"`
`#include "fault.h"`
`#include "fault_comm_interface.h"`
Include dependency graph for fault.c:

Go to the source code of this file.

## Functions
static void | Fault_EnableShortCircuitProtection (void)
| Enable Short circuit hardware protection.
void | Fault_Handler (void)
| Handles the fault trip by turning off the power control switching.
void | Fault_Initialize (void)
| Initialize the fault objects.
void | Fault_Execute (void)
| Executes the fault handlers.
void | Fault_Reset (void)
| Clears the fault object flag bits.
void | Fault_Execute_100ms (void)
| Fault evaluation for Temperature and other slow fault detection executed every 100ms.

## Variables
bool | loadDisconnect = false

## Detailed Description

<>

Definition in file fault.c.

## Variable Documentation

## ◆ loadDisconnect

bool loadDisconnect = false

Definition at line 28 of file fault.c.