|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
TEMP_SETTINGS_s Struct Reference

A custom data type for temperature measurement. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/device/dev_temp.h>`

Collaboration diagram for TEMP_SETTINGS_s:

## Data Fields
uint8_t | OverTemperatureFlag
| Over temperature flag.
uint8_t | SensorLost
| if sensor is present
uint16_t | AdcReading
| temperature value raw sampled from ADC
uint16_t | AdcAverage
| temperature
uint16_t | TemperatureCelcius
| temperature celcius.
uint16_t | TempBuffer [MAX_NUM_SAMPLES_TEMP_BUFFER]
| buffer for calcualting average.
uint16_t | BufferFull
| flag to monitor if full then allow averaging.
uint16_t | ResetBuffer
| reset Temp_buffer
uint16_t | BufferIndex
| buffer index

## Detailed Description

Definition at line 43 of file dev_temp.h.

## Field Documentation

## ◆ AdcAverage

uint16_t AdcAverage

Definition at line 47 of file dev_temp.h.

## ◆ AdcReading

uint16_t AdcReading

Definition at line 46 of file dev_temp.h.

## ◆ BufferFull

uint16_t BufferFull

Definition at line 50 of file dev_temp.h.

## ◆ BufferIndex

uint16_t BufferIndex

Definition at line 52 of file dev_temp.h.

## ◆ OverTemperatureFlag

uint8_t OverTemperatureFlag

Definition at line 44 of file dev_temp.h.

## ◆ ResetBuffer

uint16_t ResetBuffer

Definition at line 51 of file dev_temp.h.

## ◆ SensorLost

uint8_t SensorLost

Definition at line 45 of file dev_temp.h.

## ◆ TempBuffer

uint16_t TempBuffer[MAX_NUM_SAMPLES_TEMP_BUFFER]

Definition at line 49 of file dev_temp.h.

## ◆ TemperatureCelcius

uint16_t TemperatureCelcius

Definition at line 48 of file dev_temp.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/device/dev_temp.h