|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
FAN_DATA_s Struct Reference

A custom data type for fan. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/device/dev_fan.h>`

Collaboration diagram for FAN_DATA_s:

## Data Fields
uint8_t | CurrentSpeedPercent
| Current Speed in percentage.
uint8_t | TargetSpeedPercent
| targetted Speed in percentage
uint16_t | MaxSpeedPercent
| based on period value (CCXPRL). Use this to limit the fan max speed
uint16_t | Tick
| set the execution rate in multiples of 100ms
uint16_t | StepSizePercent
| set the increment rate per tick in percentage
uint16_t | TargetSpeedRaw
| targetted value raw.
uint16_t | CurrentSpeedRaw
| current value raw.
uint16_t | MaxSpeedRaw
| based on period value (CCXPRL).
uint8_t | OverrideFlag
| override flag. sets tick value to 1, step_size to 20 and target to 100%

## Detailed Description

Definition at line 50 of file dev_fan.h.

## Field Documentation

## ◆ CurrentSpeedPercent

uint8_t CurrentSpeedPercent

Definition at line 51 of file dev_fan.h.

## ◆ CurrentSpeedRaw

uint16_t CurrentSpeedRaw

Definition at line 57 of file dev_fan.h.

## ◆ MaxSpeedPercent

uint16_t MaxSpeedPercent

Definition at line 53 of file dev_fan.h.

## ◆ MaxSpeedRaw

uint16_t MaxSpeedRaw

Definition at line 58 of file dev_fan.h.

## ◆ OverrideFlag

uint8_t OverrideFlag

Definition at line 59 of file dev_fan.h.

## ◆ StepSizePercent

uint16_t StepSizePercent

Definition at line 55 of file dev_fan.h.

## ◆ TargetSpeedPercent

uint8_t TargetSpeedPercent

Definition at line 52 of file dev_fan.h.

## ◆ TargetSpeedRaw

uint16_t TargetSpeedRaw

Definition at line 56 of file dev_fan.h.

## ◆ Tick

uint16_t Tick

Definition at line 54 of file dev_fan.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/device/dev_fan.h