|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
START_UP_RAMP_s Struct Reference
Power Control » Power Control Data Types

Stores data related to the ramping up/down of the reference. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/pwrctrl/pwrctrl_typedef.h>`

Collaboration diagram for START_UP_RAMP_s:

## Data Fields
uint16_t | Counter
| Soft-Start Execution Counter. This setting is set/cleared by the device driver and is 'read only'.
uint16_t | Delay
| Soft-Start Period (POD, RAMP PERIOD, PGD, etc.)
uint16_t | StepSize
| Size/value of one reference increment/decrement or this period.
uint16_t * | ptrReference
| pointer the reference variable
uint16_t * | ptrReferenceTarget
| pointer to the ramp-up reference target
bool | RampComplete
| indicates when ramp-up is complete

## Detailed Description

This data structure manages the ramping up/down of the reference depending on the target. "reference" is the actual reference currently being used while "targetReference" can be different that reference during soft-start.

Definition at line 98 of file pwrctrl_typedef.h.

## Field Documentation

## ◆ Counter

uint16_t Counter

Definition at line 100 of file pwrctrl_typedef.h.

## ◆ Delay

uint16_t Delay

Definition at line 101 of file pwrctrl_typedef.h.

## ◆ ptrReference

uint16_t* ptrReference

Definition at line 103 of file pwrctrl_typedef.h.

## ◆ ptrReferenceTarget

uint16_t* ptrReferenceTarget

Definition at line 104 of file pwrctrl_typedef.h.

## ◆ RampComplete

bool RampComplete

Definition at line 105 of file pwrctrl_typedef.h.

## ◆ StepSize

uint16_t StepSize

Definition at line 102 of file pwrctrl_typedef.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/pwrctrl/pwrctrl_typedef.h